For 1990-2009 cars

### Removal Procedure

Important: The front seat recliner is an integral part of the front seat back frame. If the recliner needs to be replaced then the entire front seat back frame must be replaced.

1. Remove the front seat. Refer to Bucket Seat Replacement .
2. Remove the seat back cover. Refer to Front Seat Back Cushion Cover Replacement .
3. Separate the seat back pad from the seat back frame (1).
4. Replace the entire seat back frame (1) and recliner assembly (4).

### Installation Procedure

1. Replace the entire seat back frame (1) and recliner assembly (4).
2. Install the seat back cover. Refer to Front Seat Back Cushion Cover Replacement .
3. Install the front seat. Refer to Bucket Seat Replacement .