For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Body Control Module (BCM) | Below the right side of the IP, right of the IP compartment | Body Control System Component Views | Body Control System Connector End Views
Door Lock Switch Plate (Door Mounted, Striker) | Mounted to the lower, front end of the rear side door | Power Door Systems Component Views | Power Door Systems Connector End Views
Door Lock Switch Plate (Pillar Mounted, Striker) | Mounted to the lower, rear side of the B-pillar | Power Door Systems Component Views | Power Door Systems Connector End Views
Front Door Lock | Inside, rear end of the front door | Power Door Systems Component Views | Power Door Systems Connector End Views
Front Door Lock (Actuator) | Part of the front door lock | Power Door Systems Component Views | Power Door Systems Connector End Views
Front Door Lock (Ajar Indicator Switch) | Part of the front door lock | Power Door Systems Component Views | Power Door Systems Connector End Views
Front Door Lock Cylinder Switch | Inside the front door | Power Door Systems Component Views | Power Door Systems Connector End Views
Front Door Lock Switch | In the front door armrest | Power Door Systems Component Views | Power Door Systems Connector End Views
Front Window Regulator Motor | Inside the front door | Power Door Systems Component Views | Power Door Systems Connector End Views
Front Window Switch | In the armrest of the front door | Power Door Systems Component Views | Power Door Systems Connector End Views
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views | Electrical Center Identification Views
Heater-A/C Control | Center of the IP, below the radio | HVAC Component Views | HVAC Connector End Views
Heater-A/C Control (Rear Window Defogger Switch) | Part of the heater-A/C control | HVAC Component Views | HVAC Connector End Views
Instrument Cluster | Left side of the IP | Instrument Panel, Gages, and Console Component Views | Instrument Panel, Gages, and Console Connector End Views
Interior Lamp and Multi-function Switch | Center in front of the roof headliner | Lighting Systems Component Views | Lighting Systems Connector End Views
Interior Lamp and Multi-function Switch (Power Sliding Door On/Off Switch) | Part of the interior lamp and multi-function switch | Lighting Systems Component Views | Power Door Systems Connector End Views
Interior Lamp and Multi-function Switch (Power Sliding Door Open/Close Switch) | Part of the interior lamp and multi-function switch | Lighting Systems Component Views | Power Door Systems Connector End Views
Liftgate Door Lock | Inside the liftgate, below the license plate | Body Rear End Component Views | Body Rear End Connector End Views
Liftgate Door Lock (Actuator) | Part of the liftgate door lock | Body Rear End Component Views | Body Rear End Connector End Views
Liftgate Door Lock Cylinder Switch | Inside the liftgate, above the license lamps | Body Rear End Component Views | Body Rear End Connector End Views
Outside Rearview Mirror | On the outside of the front door | Power Door Systems Component Views | Power Door Systems Connector End Views
Outside Rearview Mirror (Heated Defogger) | In the outside rearview mirror | Power Door Systems Component Views | Power Door Systems Connector End Views
Outside Rearview Mirror (Mirror Motor Pack) | In the outside rearview mirror | Power Door Systems Component Views | Power Door Systems Connector End Views
Outside Rearview Mirror Remote Control Switch | Mounted to the top front left front door armrest panel | Power Door Systems Component Views | Power Door Systems Connector End Views
Power Sliding Door Detent Switch | Inside the right rear door, mounted to the rear of the door | Power Door Systems Component Views | Power Door Systems Connector End Views
Power Sliding Door Open/Close Switch (RH B-Pillar) | Middle of the right B-pillar | Power Door Systems Component Views | Power Door Systems Connector End Views
Power Sliding Door Unlatch Actuator | In the right power sliding door at the front of of the door | Power Door Systems Component Views | Power Door Systems Connector End Views
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views | Engine Controls Connector End Views
Rear Door Lock (Actuator) | In the rear side door | Power Door Systems Component Views | Power Door Systems Connector End Views
Rear Side Door Actuator Control Module | Right quarter panel, above the wheelhouse | Power Door Systems Component Views | Power Door Systems Connector End Views
Rear Side Door Actuator Motor | Right quarter panel, above the wheelhouse | Power Door Systems Component Views | --
Rear Side Door Actuator Motor (Optical Sensor) | Part of the rear side door actuator motor | Power Door Systems Component Views | --
Rear Sliding Door Alarm | Attached to the rear side door actuator motor | Power Door Systems Component Views | --
Relay Center | Right side of IP, mounted to the bracket along with the BCM, near the rear top right side of the IP compartment | Power and Grounding Component Views | Power and Grounding Connector End Views
Remote Control Door Lock Receiver (RCDLR) | Behind the center of the IP, underside of the IP trim, near the windshield defrost vent | Keyless Entry Component Views | Keyless Entry Connector End Views
Sliding Door Jamb Switch | Mounted to the rear opening of the rear side door | Power Door Systems Component Views | Power Door Systems Connector End Views
Transaxle Range Switch | Rear left side of the engine compartment, mounted to the top of the transaxle | Engine Controls Component Views | Automatic Transmission Related Connector End Views
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views | Power and Grounding Connector End Views
C101 (20 cavities) | IP wiring harness to the engine wiring harness, in the lower left side of the engine compartment, near the EBCM | Harness Routing Views | Inline Harness Connector End Views
C200 (56 cavities) | IP wiring harness to the right side of the body wiring harness, behind the right side of the IP compartment, below P100 | Harness Routing Views | Inline Harness Connector End Views
C203 (56 cavities) | IP wiring harness to the left side of the body wiring harness, left side of the steering column, below P101 | Harness Routing Views | Inline Harness Connector End Views
C301 (10 cavities) | Body wiring harness to the left side door wiring harness, behind the left kick panel, left of the parking brake | Harness Routing Views | Inline Harness Connector End Views
C302 (16 cavities) | Body wiring harness to the right front side door wiring harness, behind the right kick panel | Harness Routing Views | Inline Harness Connector End Views
C303 (16 cavities) | Body wiring harness to the left front side door wiring harness, behind the left kick panel, left of the parking brake | Harness Routing Views | Inline Harness Connector End Views
C304 (10 cavities) | Body wiring harness to the right front side door wiring harness, behind the right kick panel | Harness Routing Views | Inline Harness Connector End Views
C308 (23 cavities) | Body wiring harness to the roof wiring harness, inside the right B-pillar, behind the lower trim | Harness Routing Views | Inline Harness Connector End Views
C400 (2 cavities) | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate | -- | Inline Harness Connector End Views
C401 (4 cavities) | Body wiring harness to the liftgate wiring harness, above the left rear side of the roof headliner, near P405 and the liftgate | Harness Routing Views | Inline Harness Connector End Views
C403 (3 cavities) | Body wiring harness to the liftgate wiring harness, above the left rear side of the roof headliner, near P405 and the liftgate | Harness Routing Views | Inline Harness Connector End Views
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views | --
G302 | Secured near the base of the right B-pillar | Harness Routing Views | --
G401 | Secured to the lower left D-pillar | -- | --
G402 | Secured to the lower right D-pillar | Harness Routing Views | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views | --
P405 | Between the left side of the liftgate and the roof | Harness Routing Views | --
P406 | Between the right side of the liftgate and the roof | Harness Routing Views | --
P500 | Between the left A-pillar and the left front door | Harness Routing Views | --
P600 | Between the right A-pillar and the right front door | Harness Routing Views | --
S202 | IP harness, leftt side of the IP approximately 15 cm (6 in) from the rear window wiper/washer and multi-function switch breakout | -- | --
S209 | IP harness, center of the IP approximately 8 cm (3 in) from the security indicator lamp breakout | -- | --
S213 | IP harness, center of IP approximately 72 cm (28 in) from the cigar lighter | -- | --
S264 | IP harness, right side of the IP approximately 16 cm (6 in) from the relay center breakout | -- | --
S275 | IP harness, right side of the IP approximately 6 cm (2.5 in) from the BCM breakout | -- | --
S302 | Body harness, right front door approximately 7 cm (3 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S303 | Body harness, front of the right B-pillar approximately 26 cm (10 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S307 | Body harness, under the right front door sill approximately 2 cm (1 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S311 | Body harness, under the right front door sill approximately 13 cm (5 in) from the C302 breakout | -- | --
S314 | Body harness, under the right front seat approximately 2 cm (1 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S315 | Body harness, under the right front seat approximately 8 cm (3 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S318 | Body harness, under the right front door sill approximately 17 cm (7 in) C302 breakout | -- | --
S319 | Body harness, under the right front door sill approximately 17 cm (7 in) C302 breakout | -- | --
S323 | Body harness, under the left front seat approximately 7 cm (3 in) from the seat belt switch breakout | -- | --
S324 | Body harness, top/forward area of the left rear wheel well approximately 5 cm (2 in) behind the second oval clamp | -- | --
S326 | Body harness, top/forward area of the left rear wheel well approximately 13 cm (5 in) behind the second oval clamp | -- | --
S327 | Body harness, under the left front seat approximately 13 cm (5 in) from the seat belt switch breakout | -- | --
S330 | Body harness, left of B-pillar, approximately 40 cm (16 in) from seat belt switch breakout | -- | --
S390 | Roof harness, overhead console approximately 10 cm (4 in) from the right sunshade lighted vanity mirror breakout | -- | --
S392 | Roof harness, right B-pillar approximately 27 cm (10 in) from the power sliding door open/close switch (right B-pillar) | -- | --
S395 | Roof harness, right side of the overhead console approximately 13 cm (5 in) from the he power sliding door open/close switch (right B-pillar) breakout | -- | --
S460 | Liftgate harness center of the liftgate approximately 7 cm (3 in) from the liftgate lock cylinder switch breakout | -- | --
S504 | Left door harness, left door approximately 10 cm (4 in) from the left window switch breakout | -- | --
S604 (w/AB5) | Right door harness, right door approximately 10 cm (4 in) from the right window switch breakout | -- | --
S604 (w/o AB5) | Right door harness, between P600 and the right front speaker breaker | -- | --
S817 | Sliding door harness, inside the right rear side door approximately 11 cm (4 in) from the right rear door latch release actuator breakout | -- | --