For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Brake Fluid Level Indicator Sensor | Right side of the brake fluid reservoir | Hydraulic Brake Component Views | Hydraulic Brake Connector End Views
Brake Modulator | Left side of the engine compartment, mounted to the brake master cylinder | Antilock Brake System Component Views | --
Cruise Control Module | Engine compartment, near the left strut tower | Cruise Control Component Views | Cruise Control Connector End Views
Data Link Connector (DLC) | Below the steering column, bottom of the knee bolster | Data Link Communications Component Views | Data Link Communications Connector End Views
Electronic Brake Control Module (EBCM) | Lower left side of the engine compartment | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Electronic Brake Control Relay | Part of EBCM | -- | --
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views | Electrical Center Identification Views
Fusible Link Z | Bolted to the starter solenoid | -- | --
Instrument Cluster | Left side of the IP | Instrument Panel, Gages, and Console Component Views | Instrument Panel, Gages, and Console Connector End Views
Left Front Wheel Speed Sensor | Part of the left front hub assembly | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Left Rear Wheel Speed Sensor | Part of the left rear hub assembly | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views | Engine Controls Connector End Views
Rear Window Wiper/Washer and Multi-function Switch (Fog Lamp/TCC Switch) | Part of the rear window wiper/washer and multi-function switch | Wiper/Washer Component Views | Lighting Systems Connector End Views
Right Front Wheel Speed Sensor | Part of the right front hub assembly | Antilock Brake System Connector End Views | Antilock Brake System Connector End Views
Right Rear Wheel Speed Sensor | Part of the right rear hub assembly | Antilock Brake System Connector End Views | Antilock Brake System Connector End Views
Splice Pack SP205 | Below the steering column, bottom of the knee bolster | Data Link Communications Component Views | Data Link Communications Connector End Views
Stop Lamp Switch | Mounted to the brake pedal support | Cruise Control Component Views | Lighting Systems Connector End Views
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views | Power and Grounding Connector End Views
C101 (20 cavities) | IP wiring harness to the engine wiring harness, in the lower left side of the engine compartment, near the EBCM | Harness Routing Views | Inline Harness Connector End Views
C171 (2 cavities) | IP wiring harness to the left wheel speed sensor wiring harness, below the air cleaner assembly, mounted to the left inner fender | Harness Routing Views | Inline Harness Connector End Views
C172 (2 cavities) | IP wiring harness to the right wheel speed sensor wiring harness, below the windshield fluid reservoir | Harness Routing Views | Inline Harness Connector End Views
C203 (56 cavities) | IP wiring harness to the left side of the body wiring harness, left side of the steering column, below P101 | Harness Routing Views | Inline Harness Connector End Views
C305 (12 cavities) | Body wiring harness to the electronic brake control wiring harness and fuel sender wiring harness, mounted as a pass through, beneath the vehicle behind the driver seat | Harness Routing Views | Inline Harness Connector End Views
C306 (2 cavities) | Electronic brake control wiring harness to the right rear wheel speed sensor wiring harness, under the right side of the vehicle, front of the right rear wheel | Harness Routing Views | Inline Harness Connector End Views
C309 (2 cavities) | Electronic Brake control wiring harness to the left rear wheel speed sensor wiring harness, under the left side of the vehicle, front of the left rear wheel | Harness Routing Views | Inline Harness Connector End Views
G114 | Engine compartment, left and above the starter, near the starter solenoid | Harness Routing Views | --
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views | --
P101 | On the left side of the bulkhead, right of the left strut tower | Harness Routing Views | --
S108 | Engine harness, front left side of the engine compartment approximately 8 cm (3 in) from the PCM breakout | -- | --
S205 | IP harness, left side of the IP approximately 8 cm (3 in) from the hazard lamp/turn signal flasher breakout | -- | --
S230 | IP harness, right side of the IP approximately 4 cm (2 in) from the rear window wiper/washer and multi-function switch breakout | -- | --
S242 | IP harness, left side of the IP approximately 14 cm (6 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --