For 1990-2009 cars

Table 1: | A/C Compressor Clutch Coil
Table 2: | A/C Refrigerant Pressure Sensor
Table 3: | Ambient Air Temperature Sensor
Table 4: | Auxiliary Blower Motor
Table 5: | Auxiliary Blower Motor Resistor
Table 6: | Auxiliary Coolant Bypass Pump
Table 7: | Auxiliary Coolant Pump Switch
Table 8: | Auxiliary Heater-A/C Control Connector C1 (Temperature Control)
Table 9: | Auxiliary Heater-A/C Control Connector C2 (Auxiliary Blower Switch)
Table 10: | Auxiliary Temperature Valve Actuator
Table 11: | Blower Motor Resistor
Table 12: | Electric Air Inlet Actuator
Table 13: | Electric Slave Actuator
Table 14: | Heater-A/C Control Connector C1 (Blower Motor Switch)
Table 15: | Heater-A/C Control Connector C2 (Compressor and Air Delivery Control)
Table 16: | Rear Window Wiper/Washer and Multi-function Switch Connector C2 (Auxiliary Blower Switch)

#### A/C Compressor Clutch Coil

Connector Part Information |

• | 1216-2017

• | 2-Way F Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1050 | Ground
B | DK GRN | 59 | A/C Compressor Clutch Solenoid Feed

#### A/C Refrigerant Pressure Sensor

Connector Part Information |

• | 1211-0192

• | 3-Way F Metri-Pack 150 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 2751 | A/C Pressure Return
B | GRY | 2700 | 5 Volt Reference
C | RED/BLK | 380 | A/C Refrigerant Pressure Sensor Signal

#### Ambient Air Temperature Sensor

Connector Part Information |

• | 1205-2641

• | 2-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN/BLK | 735 | Outside Ambient Temperature Sensor Signal
B | BLK | 1550 | Ground

#### Auxiliary Blower Motor

Connector Part Information |

• | 1203-3769

• | 2-Way F Metri-Pack 630 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 1052 | Auxiliary Blower Motor Output
B | BRN | 641 | Fused Output

#### Auxiliary Blower Motor Resistor

Connector Part Information |

• | 1205-2856

• | 4-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | ORN | 1052 | Auxiliary Blower Motor Output
C | YEL | 1176 | Auxiliary Blower Resistor Low Output
D | LT BLU | 1072 | Auxiliary Blower Resistor Medium Output

#### Auxiliary Coolant Bypass Pump

Connector Part Information |

• | 12084126

• | 2-Way F Metri-Pack 150 Series Sealed(BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK | 1050 | Ground
2 | YEL | 61 | Low Reference

#### Auxiliary Coolant Pump Switch

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series Sealed(BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 1239 | Ignition 1 Voltage
B | YEL | 61 | Low Reference

#### Auxiliary Heater-A/C Control Connector C1 (Temperature Control)

Connector Part Information |

• | 1206-4978

• | 6-Way F Micro-Pack 100 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN | 641 | Fused Input Feed
2 | GRY | 8 | Interior Lamps Dimming Input Feed
3 | GRY | 778 | Auxiliary Blower Switch Control Input Feed
4 | LT BLU | 733 | Air Temperature Valve Position Sensor Output Signal
5 | BLK | 955 | Auxiliary Temperature Output Feed
6 | BLK | 850 | Ground

#### Auxiliary Heater-A/C Control Connector C2 (Auxiliary Blower Switch)

Connector Part Information |

• | 1206-4752

• | 6-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | BLK | 1750 | Ground
D | YEL | 1176 | Auxiliary Blower Resistor Low Output
E | LT BLU | 1072 | Auxiliary Blower Resistor Medium Output
F | ORN | 1052 | Auxiliary Blower Motor Output

#### Auxiliary Temperature Valve Actuator

Connector Part Information |

• | 1204-0953

• | 6-Way F Micro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
5-6 | -- | -- | Not Used
7 | BLK | 850 | Ground
8 | BLK | 955 | Auxiliary Temperature Input Feed
9 | -- | -- | Not Used
10 | BRN | 641 | Fused Input Feed

#### Blower Motor Resistor

Connector Part Information |

• | 1205-2854

• | 7-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 63 | Blower Switch Input M1 Position
B | YEL | 60 | Blower Switch Input Low Position
C | PPL | 73 | Blower Switch Input M3 Position
D | LT BLU | 72 | Blower Switch Input M2 Position
E | BLK | 150 | Ground
F | ORN | 52 | Blower Switch Input High Position
G | ORN | 40 | Fused Input Feed

#### Electric Air Inlet Actuator

Connector Part Information |

• | 1206-4993

• | 6-Way F Micro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
5 | BRN | 241 | Fused Input Feed
6 | LT BLU/BLK | 684 | Air Inlet Valve Signal Input
7 | BLK | 150 | Ground
8-10 | -- | -- | Not Used

#### Electric Slave Actuator

Connector Part Information |

• | 1206-4993

• | 6-Way F Micro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
5-6 | -- | -- | Not Used
7 | BLK | 150 | Ground
8 | LT BLU | 733 | Temperature Valve Position Signal Input
9 | -- | -- | Not Used
10 | BRN | 241 | Fused Input Feed

#### Heater-A/C Control Connector C1 (Blower Motor Switch)

Connector Part Information |

• | 1206-4998

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 119 | Heater-A/C ON/OFF Signal Output
B | BRN | 41 | Fused Input Feed
C | ORN | 52 | Blower Switch High Position Output
D | -- | -- | Not Used
E | PPL | 73 | Blower Switch M3 Position Output
F | LT BLU | 72 | Blower Switch M2 Position Output
G | TAN | 63 | Blower Switch M1 Position Output
H | YEL | 60 | Blower Switch Low Position Output

#### Heater-A/C Control Connector C2 (Compressor and Air Delivery Control)

Connector Part Information |

• | 1206-4799

• | 12-Way F Micro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 119 | Heater-A/C ON/OFF Signal Input
B | DK GRN/WHT | 762 | A/C Request Signal Output
C | BRN | 241 | Fused Input Feed
D | WHT | 193 | Rear Defogger Relay Output-Coil
E | ORN | 640 | Fused Input Feed
F | -- | -- | Not Used
G | LT BLU | 733 | Temperature Control Position Signal Output
H | LT BLU/BLK | 684 | Air Inlet Valve Signal Output
J | GRY | 8 | Interior Lamps Dimming Input Feed
K | BLK | 150 | Ground
L-M | -- | -- | Not Used

#### Rear Window Wiper/Washer and Multi-function Switch Connector C2 (Auxiliary Blower Switch)

Connector Part Information |

• | 1216-2455

• | 8-Way F Metri-Pack 280 Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 1176 | Auxiliary Blower Motor Resistor Low Output
B | ORN | 1052 | Auxiliary Blower Motor Resistor High Output
C | LT BLU | 1072 | Auxiliary Blower Motor Resistor Medium Output
D | -- | -- | Not Used
E | BLK | 1450 | Ground
F | -- | -- | Not Used
G | GRY | 778 | Auxiliary Blower Switch Control Output Feed
H | GRY | 8 | Interior Lamps Dimming Input Feed