For 1990-2009 cars

#### C313

Connector Part Information |

• | 12064749

• | 2-Way M Metri-Pack 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 340 | Fused input feed
B | BLK | 550 | Ground

#### C314

Connector Part Information |

• | 12064749

• | 2-Way M Metri-Pack 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 340 | Fused input feed
B | BLK | 550 | Ground

#### Driver / Passenger Seat Adjuster Motor Assembly

Connector Part Information |

• | 12015344

• | 6-Way F metri-pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 282 | Seat rear height up movement output
B | LT BLU | 283 | Seat rear height down movement output
C | LT GRN | 284 | Seat back movement output
D | TAN | 285 | Seat forward movement output
E | DK GRN | 286 | Seat front height up movement output
F | DK BLU | 287 | Seat front height down movement output

#### Driver Seat Adjuster Switch

Connector Part Information |

• | 12066386

• | 8-Way F Pin Grip Connector (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 287 | Seat front height down movement output
B | DK GRN | 286 | Seat front height up movement output
C | BLK | 550 | Ground
D | TAN | 285 | Seat forward movement output
E | LT GRN | 284 | Seat back movement output
F | ORN | 340 | Fused input feed
G | LT BLU | 283 | Seat rear height down movement output
H | YEL | 282 | Seat rear height up movement output

#### Seat Heater Module--Driver

Connector Part Information |

• | 12110047

• | 6-Way M Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | -- | Heated Seat Control
B | LT BLU | -- | Heated Seat Switch Signal
C | GRN/WHT | -- | Heated Seat Switch Signal
D | YEL | -- | Battery Positive Voltage
E | BLK/RED | -- | Heated Seat Temperature Sensor Signal
F | BLK | -- | Ground

#### Seat Heater Module--Passenger

Connector Part Information |

• | 12110047

• | 6-Way M Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | -- | Heated Seat Control
B | LT BLU | -- | Heated Seat Switch Signal
C | GRN/WHT | -- | Heated Seat Switch Signal
D | YEL | -- | Battery Positive Voltage
E | BLK/RED | -- | Heated Seat Temperature Sensor Signal
F | BLK | -- | Ground

#### Rear Window Wiper/Washer and Multifunction Switch--C4

Connector Part Information |

• | 12047976

• | 8-Way M Metri-Pack Mixed Series (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | Interior Dimming Signal
B | BLK | 1450 | Ground
C | BRN | 241 | Ignition 3 Voltage
D | LT BLU/BLK | 1505 | Right Heated Seat Signal
E | LT BLU | 1462 | Heated Seat Switch Signal
F-H | -- | -- | Not Used

#### Passenger Seat Adjuster Switch

Connector Part Information |

• | 12066386

• | 8-Way F Pin Grip Connector (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 283 | Seat rear height down movement output
B | YEL | 282 | Seat rear height up movement output
C | BLK | 550 | Ground
D | LT GRN | 284 | Seat back movement output
E | TAN | 285 | Seat forward movement output
F | ORN/BLK | 340 | Fused input feed
G | DK BLU | 287 | Seat front height down movement output
H | DK GRN | 286 | Seat front height up movement output

#### Seat Belt Switch

Connector Part Information |

• | 12052833

• | 2-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/WHT | 238 | Driver seat belt input (ground)
B | BLK | &50 | Ground