For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Dryer Bracket to Auto Level Control Air Compressor Bolt/Screw | 7 N·m | 62 lb in
Automatic Level Control Air Compressor Bracket Bolts /Screws | 4 N·m | 35 lb In
Automatic Level Control Air Compressor Bracket to Underbody Nut | 10 N·m | 89 lb in
Automatic Level Control Air Compressor Bracket to Underbody Bolt/Screw | 50 N·m | 37 lb ft
Automatic Level Control Air Compressor Head to Compressor Bolt/Screw | 6 N·m | 53 lb in
Automatic Level Control Air Compressor Relay to Auto Level Control Air Compressor Bracket Bolt/Screw | 3 N·m | 27 lb in
Automatic Level Control Air Compressor Rubber Shield to Auto Level Control Air Compressor Bracket Bolt/Screw | 3 N·m | 27 lb In
Automatic Level Control Sensor Adjustment Bolt/Screw | 5 N·m | 44 lb In
Automatic Level Control Sensor to Automatic Level Control Sensor Bracket Bolt/Screw | 4 N·m | 35 lb In
Automatic Level Control Sensor Ball Stud to Tie Rod or Automatic Level Control Sensor Arm | 4 N·m | 35 lb in
Automatic Level Control Sensor to Underbody Bolt/Screw | 10 N·m | 89 lb In
Inflation Timer Relay to Panel Bolt/Screw | 3 N·m | 27 lb in
Inflator Solenoid to Panel Nut | 3 N·m | 27 lb in
Inflator Fill Valve to Panel Nut | 6 N·m | 53 lb in