For 1990-2009 cars

## Rear Seat Back Cushion Frame Replacement AQ4 Captains Chair

### Removal Procedure

1. Remove the rear seat back cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement .
2. Pinch the base of the head restraint guides and remove the guide from the seat back frame.

### Installation Procedure

1. Install the head restraint guides to the seat back frame.
2. Install the rear seat back cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement .

## Rear Seat Back Cushion Frame Replacement Rear AL4 Rear Bucket

### Removal Procedure

1. Remove the rear seat back cover and pad (2). Refer to Rear Seat Back Cushion Cover and Pad Replacement .
2. Pinch the base of the head restraint guides and remove the guide from the seat back frame (1).

### Installation Procedure

1. Install the head restraint guides to the seat back frame.
2. Install the rear seat back cover and pad (2). Refer to Rear Seat Back Cushion Cover and Pad Replacement .

## Rear Seat Back Cushion Frame Replacement AT5 - 60/40 Split Bench

### Removal Procedure

1. Remove the rear seat back cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement .
2. Pinch the base of the head restraint guides and remove the guide from the seat back frame (1).

### Installation Procedure

1. Install the head restraint guides to the seat back frame (1).
2. Install the rear seat back cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement .

## Rear Seat Back Cushion Frame Replacement AM9 - 50/50 Split Bench

### Removal Procedure

1. Remove the rear seat back cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement .
2. Pinch the base of the head restraint guides and remove the guide from the seat back frame (1).

### Installation Procedure

1. Install the head restraint guides to the seat back frame (1).
2. Install the rear seat back cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement .