For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Rear License Plate Lamp Assembly Procedure Push the tab inward on the right side of the license plate lamp in order to release the lamp from the rear bumper cover. Pull downward to access and disconnect the electrical connector from the lamp socket.
2 | Rear License Plate Bulb Socket Tip Twist the socket counterclockwise in order to remove from the lamp from the housing and to access the bulb.