For 1990-2009 cars

Connector 1: | 1-2 Shift Solenoid (SS) Valve, Wiring Harness Side (M82)
Connector 2: | 2-3 Shift Solenoid (SS) Valve, Wiring Harness Side (M82)
Connector 3: | 4-5 Shift Solenoid (SS) Valve, Wiring Harness Side (M82)
Connector 4: | A/C Compressor Clutch (C60)
Connector 5: | A/C Refrigerant Pressure Sensor (C60)
Connector 6: | Accelerator Pedal Position (APP) Sensor
Connector 7: | Accessory Power Outlet
Connector 8: | Air Temperature Actuator - Left
Connector 9: | Air Temperature Actuator - Right
Connector 10: | Audio Amplifier - X1
Connector 11: | Audio Amplifier - X2
Connector 12: | Audio Amplifier - X3
Connector 13: | Automatic Transmission Shift Lock Control Solenoid (M82)
Connector 14: | Backup Lamp
Connector 15: | Blower Motor
Connector 16: | Blower Motor High Speed Relay
Connector 17: | Blower Motor Resistor
Connector 18: | Body Control Module (BCM) X1
Connector 19: | Body Control Module (BCM) X2
Connector 20: | Body Control Module (BCM) X3
Connector 21: | Body Control Module (BCM) X4
Connector 22: | Brake Booster Pump Motor
Connector 23: | Brake Booster Vacuum Sensor
Connector 24: | Brake Fluid Level Switch
Connector 25: | Brake Pedal Position (BPP) Sensor
Connector 26: | Camshaft Position (CMP) Actuator Solenoid Valve - Exhaust
Connector 27: | Camshaft Position (CMP) Actuator Solenoid Valve - Intake
Connector 28: | Camshaft Position (CMP) Sensor - Exhaust
Connector 29: | Camshaft Position (CMP) Sensor - Intake
Connector 30: | Center High Mounted Stop Lamp (CHMSL)
Connector 31: | Crankshaft Position (CKP) Sensor
Connector 32: | Data Link Connector (DLC)
Connector 33: | Data Link Resistor
Connector 34: | Door Lock Actuator - Driver (AU3)
Connector 35: | Door Lock Actuator - Passenger (AU3)
Connector 36: | Door Lock Switch - Driver (AU3)
Connector 37: | Door Lock Switch - Passenger (AU3)
Connector 38: | Electronic Brake Control Module (EBCM)
Connector 39: | Engine Control Module (ECM) X1
Connector 40: | Engine Control Module (ECM) X2
Connector 41: | Engine Coolant Level Switch
Connector 42: | Engine Coolant Temperature (ECT) Sensor
Connector 43: | Engine Cooling Fan
Connector 44: | Engine Oil Pressure (EOP) Switch
Connector 45: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
Connector 46: | Evaporative Emission (EVAP) Canister Vent Solenoid Valve
Connector 47: | Evaporator Temperature Sensor (C60)
Connector 48: | Fog Lamp - Left Front (T96)
Connector 49: | Fog Lamp - Right Front (T96)
Connector 50: | Fog Lamp Switch (T96)
Connector 51: | Folding Top Cover Actuator
Connector 52: | Fuel Injector 1
Connector 53: | Fuel Injector 2
Connector 54: | Fuel Injector 3
Connector 55: | Fuel Injector 4
Connector 56: | Fuel Pump and Sender Assembly
Connector 57: | Fuel Rail Pressure (FRP) Sensor
Connector 58: | Fuel Tank Pressure (FTP) Sensor
Connector 59: | Generator X1
Connector 60: | Generator X2
Connector 61: | Ground Table
Connector 62: | Hazard Warning Switch
Connector 63: | Headlamp - Left High Beam
Connector 64: | Headlamp - Left Low Beam
Connector 65: | Headlamp - Right High Beam
Connector 66: | Headlamp - Right Low Beam
Connector 67: | Heated Oxygen Sensor (HO2S) 1
Connector 68: | Heated Oxygen Sensor (HO2S) 2
Connector 69: | High Pressure Fuel Pump
Connector 70: | Horn - Left
Connector 71: | Horn - Right
Connector 72: | Horn Switch X1
Connector 73: | Horn Switch X2
Connector 74: | HVAC Control Module X1
Connector 75: | HVAC Control Module X2
Connector 76: | HVAC Control Module X3
Connector 77: | I/P Dimmer Switch
Connector 78: | Ignition Coil 1
Connector 79: | Ignition Coil 2
Connector 80: | Ignition Coil 3
Connector 81: | Ignition Coil 4
Connector 82: | Ignition Switch
Connector 83: | Inflatable Restraint Front End Sensor - Left
Connector 84: | Inflatable Restraint Front End Sensor - Right
Connector 85: | Inflatable Restraint I/P Module X1
Connector 86: | Inflatable Restraint I/P Module X2
Connector 87: | Inflatable Restraint I/P Module Indicator
Connector 88: | Inflatable Restraint Passenger Presence System (PPS) Module
Connector 89: | Inflatable Restraint Sensing and Diagnostic Module (SDM)
Connector 90: | Inflatable Restraint Steering Wheel Module X1
Connector 91: | Inflatable Restraint Steering Wheel Module X2
Connector 92: | Inflatable Restraint Steering Wheel Module Coil X1
Connector 93: | Inflatable Restraint Steering Wheel Module Coil X2
Connector 94: | Inflatable Restraint Steering Wheel Module Coil X3
Connector 95: | Input Speed Sensor (ISS), Wiring Harness Side (M82)
Connector 96: | Inside Rearview Mirror
Connector 97: | Instrument Panel Cluster (IPC)
Connector 98: | Intake Air Pressure and Temperature Sensor
Connector 99: | Internal Mode Switch (IMS) Assembly, Wiring Harness Side (M82)
Connector 100: | Knock Sensor (KS) - 1
Connector 101: | Knock Sensor (KS) - 2
Connector 102: | License Lamp - Left
Connector 103: | License Lamp - Right
Connector 104: | Manifold Absolute Pressure (MAP) Sensor
Connector 105: | Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor
Connector 106: | Mode Actuator
Connector 107: | Output Speed Sensor (OSS), Wiring Harness Side (M82)
Connector 108: | Outside Air Temperature Sensor
Connector 109: | Outside Rearview Mirror - Driver (D48)
Connector 110: | Outside Rearview Mirror - Passenger (D48)
Connector 111: | Outside Rearview Mirror Switch (D48)
Connector 112: | Park Brake Switch
Connector 113: | Park Lamp - Left Front
Connector 114: | Park Lamp - Right Front
Connector 115: | Pressure Control (PC) Solenoid Valve, Wiring Harness Side (M82)
Connector 116: | Radio - X1
Connector 117: | Radio - X2
Connector 118: | Rear Compartment Courtesy Lamp
Connector 119: | Rear Compartment Lid Ajar Switch
Connector 120: | Rear Compartment Lid Latch Release Actuator
Connector 121: | Rear Compartment Lid Release Switch
Connector 122: | Rear Window Defogger Grid X1
Connector 123: | Rear Window Defogger Grid X2
Connector 124: | Recirculation Actuator
Connector 125: | Remote Control Door Lock Receiver (RCDLR) (AU3/AU0)
Connector 126: | Seat Adjuster Switch - Driver (AF2)
Connector 127: | Seat Belt Pretensioner - Driver
Connector 128: | Seat Belt Pretensioner - Passenger
Connector 129: | Seat Belt Switch - Driver
Connector 130: | Seat Belt Switch - Passenger
Connector 131: | Seat Front Vertical Motor - Driver (AF2)
Connector 132: | Speaker - Left Front
Connector 133: | Speaker - Left Rear
Connector 134: | Speaker - Left Tweeter
Connector 135: | Speaker - Right Front
Connector 136: | Speaker - Right Rear
Connector 137: | Speaker - Right Tweeter
Connector 138: | Speaker - Subwoofer
Connector 139: | Starter Motor X1
Connector 140: | Starter Motor X2
Connector 141: | Steering Angle Sensor
Connector 142: | Steering Wheel Control Switch - Left (K34)
Connector 143: | Steering Wheel Control Switch - Right (UK3)
Connector 144: | Tail/Stop Lamp - Left
Connector 145: | Tail/Stop Lamp - Right
Connector 146: | Theft Deterrent Module (TDM)
Connector 147: | Throttle Body
Connector 148: | Torque Converter Clutch Pulse Width Modulated (TCC PWM) Solenoid Valve, Wiring Harness Side (M82)
Connector 149: | Traction Control Switch (TCS)
Connector 150: | Transmission Control Module (TCM) (M82)
Connector 151: | Transmission Manual Shift Shaft Switch, Wiring Harness Side (M82)
Connector 152: | Turbocharger Bypass Valve Solenoid
Connector 153: | Turbocharger Wastegate Solenoid
Connector 154: | Turn Signal Lamp - Left Front
Connector 155: | Turn Signal Lamp - Left Rear
Connector 156: | Turn Signal Lamp - Right Front
Connector 157: | Turn Signal Lamp - Right Rear
Connector 158: | Turn Signal Repeater Lamp - Left
Connector 159: | Turn Signal Repeater Lamp - Right
Connector 160: | Turn Signal/Multifunction Switch X1
Connector 161: | Turn Signal/Multifunction Switch X2
Connector 162: | Wheel Speed Sensor (WSS) - Left Front
Connector 163: | Wheel Speed Sensor (WSS) - Left Rear
Connector 164: | Wheel Speed Sensor (WSS) - Right Front
Connector 165: | Wheel Speed Sensor (WSS) - Right Rear
Connector 166: | Window Motor - Driver (A31)
Connector 167: | Window Motor - Passenger (A31)
Connector 168: | Window Switch - Driver (A31)
Connector 169: | Window Switch - Passenger (A31)
Connector 170: | Windshield Washer Fluid Pump
Connector 171: | Windshield Wiper Motor
Connector 172: | Windshield Wiper/Washer Switch
Connector 173: | Yaw and Lateral Accelerometer Sensor

### 1-2 Shift Solenoid (SS) Valve, Wiring Harness Side (M82)

#### Connector Part Information

- OEM: 12146094
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150.2 Series P2S (GY)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### 1-2 Shift Solenoid (SS) Valve, Wiring Harness Side (M82)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BK | 1222 | 1-2 Shift Solenoid Valve Control
B | WH | 1525 | Clutch Pressure Control Solenoid Valve 1 High Control

### 2-3 Shift Solenoid (SS) Valve, Wiring Harness Side (M82)

#### Connector Part Information

- OEM: 12146094
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150.2 Series P2S (GY)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### 2-3 Shift Solenoid (SS) Valve, Wiring Harness Side (M82)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BU | 1223 | 2-3 Shift Solenoid Valve Control
B | WH | 1525 | Clutch Pressure Control Solenoid Valve 1 High Control

### 4-5 Shift Solenoid (SS) Valve, Wiring Harness Side (M82)

#### Connector Part Information

- OEM: 12146094
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150.2 Series P2S (GY)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### 4-5 Shift Solenoid (SS) Valve, Wiring Harness Side (M82)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | GY | 898 | 4-5 SS Control
B | WH | 1525 | Clutch Pressure Control Solenoid Valve 1 High Control

### A/C Compressor Clutch (C60)

#### Connector Part Information

- OEM: 12052644
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150 Series, Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### A/C Compressor Clutch (C60)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 250 | Ground
B | 0.5 D-GN | 59 | A/C Compressor Clutch Supply Voltage

### A/C Refrigerant Pressure Sensor (C60)

#### Connector Part Information

- OEM: 13532244
- Service: 88988301
- Description: 3-Way F GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### A/C Refrigerant Pressure Sensor (C60)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN | 5514 | Low Reference
2 | 0.35 GY | 2700 | 5-Volt Reference 3
3 | 0.35 OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal

### Accelerator Pedal Position (APP) Sensor

#### Connector Part Information

- OEM: 15397577
- Service: 88953153
- Description: 6-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191818/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Accelerator Pedal Position (APP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PU | 1272 | Low Reference
B | 0.35 L-BU | 1162 | Accelerator Pedal Position Sensor 2 Signal
C | 0.35 TN | 1274 | 5-Volt Reference 3
D | 0.35 BN | 1271 | Low Reference
E | 0.35 D-BU | 1161 | Accelerator Pedal Position Sensor 1 Signal
F | 0.35 WH/BK | 1164 | 5-Volt Reference 2

### Accessory Power Outlet

#### Connector Part Information

- OEM: 12176836
- Service: 15305923
- Description: 3-Way F Metri-Pack 280 Series (GY)

#### Terminal Part Information

- Pins: A, C
- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Accessory Power Outlet

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 RD/WH | 240 | Battery Positive Voltage
B | -- | -- | Not Used
C | 1.0 BK | 550 | Ground

### Air Temperature Actuator - Left

#### Connector Part Information

- OEM: 12064982
- Service: 12102633
- Description: 5-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Air Temperature Actuator - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 1791 | Low Reference
2 | 0.35 L-BU | 733 | Air Temperature Door Position Signal
3 | 0.35 L-BU/BK | 1688 | 5-Volt Reference
4 | 0.35 D-BU | 1199 | Air Temperature Door Control
5 | 0.35 L-GN/BK | 1647 | Recirculation Door Control B

### Air Temperature Actuator - Right

#### Connector Part Information

- OEM: 12064982
- Service: 12102633
- Description: 5-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Air Temperature Actuator - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 1791 | Low Reference
2 | 0.35 D-BU | 1646 | Passenger Air Temperature Door Position Signal
3 | 0.35 L-BU/BK | 1688 | 5-Volt Reference
4 | 0.35 L-GN/BK | 1647 | Open Recirculation Door Control
5 | 0.35 TN | 2273 | Mode Door Control

### Audio Amplifier - X1

#### Connector Part Information

- OEM: 6098-4713
- Service: 88988652
- Description: 8-Way F 2.8 Series (BK)

#### Terminal Part Information

- Pins: 1, 2
- Terminal/Tray: 8100-4445/22
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-35 (VT)

- Pins: 3, 4, 7, 8
- Terminal/Tray: 8100-4444/22
- Core/Insulation Crimp: 2/A
- Release Tool/Test Probe: 15315247/J-35616-35 (VT)

#### Audio Amplifier - X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.0 RD/WH | 640 | Battery Positive Voltage
2 | 2.0 BK/WH | 751 | Ground
3 | 0.8 D-BU/WH | 346 | Left Subwoofer Speaker Output (+)
4 | 0.8 L-GN/BK | 1794 | Left Subwoofer Speaker Output (-)
5-6 | -- | -- | Not Used
7 | 0.8 L-BU/BK | 315 | Right Subwoofer Speaker Output (-)
8 | 0.8 D-GN | 1795 | Right Subwoofer Speaker Output (+)

### Audio Amplifier - X2

#### Connector Part Information

- OEM: 6098-4611
- Service: 15134091
- Description: 16-Way F 1.5 Series (BK)

#### Terminal Part Information

- Pins: 1-8, 13-16
- Terminal/Tray: 8240-0128/22
- Core/Insulation Crimp: Pins 1-8 - C/A
- Core/Insulation Crimp: Pins 13-16 - See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Audio Amplifier - X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 YE | 1956 | Left Tweeter Speaker Output (-)
2 | 0.8 TN | 1856 | Left Tweeter Speaker Output (+)
3 | 0.8 PU | 1952 | Right Tweeter Speaker Output (-)
4 | 0.8 L-GN | 1852 | Right Tweeter Speaker Output (+)
5 | 0.8 YE | 116 | Left Rear Speaker Signal Output (-)
6 | 0.8 BN | 199 | Left Rear Speaker Output (+)
7 | 0.8 L-BU | 115 | Right Rear Speaker Signal Output (-)
8 | 0.8 D-BU | 46 | Right Rear Speaker Output (+)
9-12 | -- | -- | Not Used
13 | 1.0 L-GN | 200 | Right Front Speaker Output (+)
14 | 1.0 D-GN | 117 | Right Front Speaker Signal Output (-)
15 | 1.0 TN | 201 | Left Front Speaker Output (+)
16 | 1.0 GY | 118 | Left Front Speaker Signal Output (-)

### Audio Amplifier - X3

#### Connector Part Information

- OEM: 7283-9076-30
- Service: 15394150
- Description: 16-Way F Kaizen 64 Series (BK)

#### Terminal Part Information

- Pins: 1-4, 6, 9-12, 16
- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Audio Amplifier - X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN | 511 | Left Front Low Level Audio Signal (+)
2 | 0.5 D-GN | 1947 | Left Front Low Level Audio Signal (-)
3 | 0.5 BN | 1999 | Left Rear Low Level Audio Signal (-)
4 | 0.5 BN/WH | 599 | Left Rear Low Level Audio Signal
5 | -- | -- | Not Used
6 | 0.35 PK | 314 | Radio On Signal
7-8 | -- | -- | Not Used
9 | 0.5 L-GN | 1948 | Right Front Low Level Audio Signal (-)
10 | 0.5 L-GN/WH | 512 | Right Front Low Level Audio Signal (+)
11 | 0.5 D-BU | 546 | Right Rear Low Level Audio Signal (+)
12 | 0.5 TN | 1946 | Right Rear Low Level Audio Signal (-)
13-15 | -- | -- | Not Used
16 | 0.35 L-GN | 1011 | Remote Radio Control Signal

### Automatic Transmission Shift Lock Control Solenoid (M82)

#### Connector Part Information

- OEM: 12052832
- Service: 12085535
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Automatic Transmission Shift Lock Control Solenoid (M82)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-GN/WH | 1932 | Ignition Lock Cylinder Control Actuator Signal
B | 0.35 BN | 4 | Accessory Voltage

### Backup Lamp

#### Connector Part Information

- OEM: 7223-1324-60
- Service: 88988460
- Description: 2-Way F 090 Series (GN)

#### Terminal Part Information

- Terminal/Tray: 7116-1420/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

#### Backup Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-GN | 24 | Backup Lamp Supply Voltage
2 | 0.5 BK | 750 | Ground

### Blower Motor

#### Connector Part Information

- OEM: 7283-5590-40
- Service: 88988702
- Description: 2-Way F YESC/USCAR Class III Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Blower Motor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3.0 OG | 52 | Blower Motor High Control
2 | 3.0 BN | 141 | Ignition 3 Voltage

### Blower Motor High Speed Relay

#### Connector Part Information

- OEM: 12034003
- Service: 88987189
- Description: 5-Way F Special Metri-Pack 630 Conn (BK)

#### Terminal Part Information

- Pins: 1, 2, 4, 5
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Blower Motor High Speed Relay

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3.0 BK | 2050 | Ground
2 | 3.0 BN | 141 | Ignition 3 Voltage
3 | -- | -- | Not Used
4 | 3.0 OG | 52 | Blower Motor High Control
5 | 3.0 OG | 52 | Blower Motor High Control

### Blower Motor Resistor

#### Connector Part Information

- OEM: 12059296
- Service: 12059296
- Description: 5-Way F Metri-Pack 480 Series (RD)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Blower Motor Resistor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 3.0 OG | 52 | Blower Motor High Control
B | 2.0 YE | 60 | Blower Motor Low Control
C | 2.0 TN | 63 | Blower Motor Medium 1 Control
D | 2.0 L-BU | 72 | Medium 2 Blower Motor Control
E | 3.0 OG | 52 | Blower Motor High Control

### Body Control Module (BCM) X1

#### Connector Part Information

- OEM: 15393122
- Service: 88987847
- Description: 72-Way F Micro-64 Unsealed (BU with GY case)

#### Terminal Part Information

- Pins: 8, 13-17, 19, 22, 26, 31, 35, 44, 47, 51, 53-57, 60-61
- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

- Pins: 33, 58
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Body Control Module (BCM) X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-5 | -- | -- | Not Used
6 | 0.35 YE | 682 | Door Lock/Unlock Signal (AU3)
7 | 0.35 BN | 682 | Door Lock/Unlock Signal (AU3)
8 | 0.35 WH | 1080 | Park Lamp Relay Control
9-12 | -- | -- | Not Used
13 | 0.35 PK | 849 | Brake Fluid Level Sensor Signal
14 | 0.5 L-BU | 1134 | Park Brake Switch Signal
15 | 0.35 YE | 5199 | Run/Crank Relay Coil Control
16 | 0.35 WH | 193 | Rear Defog Relay Control
17 | 0.5 D-BU | 15 | Right Turn Signal Lamps Supply Voltage
18 | -- | -- | Not Used
19 | 0.35 PK/WH | 746 | Right Front Door Ajar Switch Signal
20-21 | -- | -- | Not Used
22 | 0.35 GY/BK | 745 | Left Front Door Ajar Switch Signal
23-25 | -- | -- | Not Used
26 | 0.5 L-GN | 1478 | Coolant Level Switch Signal
27-30 | -- | -- | Not Used
31 | 0.5 L-BU | 20 | Stop Lamp Supply Voltage
32 | -- | -- | Not Used
33 | 0.35 D-GN/WH | 1135 | A/T Shift Lock Control Supply Voltage
34 | -- | -- | Not Used
35 | 0.5 L-BU | 14 | Left Turn Signal Lamps Supply Voltage
36-39 | -- | -- | Not Used
40 | 0.35 L-BU | 1788 | Traction Control Switch Signal (JL9)
41-43 | -- | -- | Not Used
44 | 0.35 TN/WH | 1969 | Headlamp High Beam Relay Control
45-46 | -- | -- | Not Used
47 | 0.35 YE | 196 | Windshield Wiper Motor Park Switch Signal
48-50 | -- | -- | Not Used
51 | 0.35 D-GN | 113 | Windshield Wiper Switch Signal 2
52 | -- | -- | Not Used
53 | 0.5 L-BU | 20 | Stop Lamp Supply Voltage
54 | 0.35 YE | 317 | Fog Lamp Relay Control (T96)
55 | 0.35 OG/BK | 744 | Rear Compartment Lid Ajar Switch Signal
56 | 0.5 OG/BK | 737 | Rear Compartment Lamp Control
57 | 0.35 BN | 253 | Trunk Release Relay Control
58 | 0.35 D-BU | 38 | Backup Lamp Relay Control
59 | -- | -- | Not Used
60 | 0.35 TN | 28 | Horn Relay Control
61 | 0.5 BK/WH | 651 | Ground
62-66 | -- | -- | Not Used
67 | 0.5 YE | 61 | Low Reference
68-69 | -- | -- | Not Used
70 | 0.5 D-GN/WH | 636 | Ambient Air Temperature Sensor Signal
71-72 | -- | -- | Not Used

### Body Control Module (BCM) X2

#### Connector Part Information

- OEM: 15393121
- Service: 88987848
- Description: 72-Way F Micro-64 Unsealed (GY)

#### Terminal Part Information

- Pins: 1-5, 9-11, 14-20, 26, 31, 33, 38, 44, 47, 51, 56-59, 61-62, 66-69, 71-72
- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Body Control Module (BCM) X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus (+)
2 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus (+)
3 | 0.35 PK/WH | 1970 | Headlamp Relay Control
4 | 0.35 PU | 524 | Headlamp Dimmer Switch High Beam Signal
5 | 0.35 BN/WH | 301 | Park Lamp Switch On Signal
6-8 | -- | -- | Not Used
9 | 0.35 WH | 111 | Hazard Warning Switch Signal
10 | 0.35 TN | 1576 | Rear Compartment Lock Actuator Unlock
11 | 0.35 D-GN | 264 | Security Indicator Supply Voltage
12-13 | -- | -- | Not Used
14 | 0.35 TN | 28 | Horn Relay Control
15 | 0.35 WH | 103 | Headlamp Switch Headlamps On Signal
16 | 0.35 OG | 192 | Front Fog Lamp Switch Signal (T96)
17 | 0.35 PU/WH | 549 | Headlamp Switch Headlamps Off Signal
18 | 0.35 WH | 5359 | 5-Volt Reference
19 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-)
20 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-)
21-25 | -- | -- | Not Used
26 | 0.35 D-GN | 44 | I/P Lamp Dimmer Switch Signal
27-30 | -- | -- | Not Used
31 | 0.35 YE | 5361 | Brake Pedal Position Sensor Signal
32-37 | -- | -- | Not Used
38 | 0.35 L-GN/BK | 5060 | Low Speed GMLAN Serial Data
39-43 | -- | -- | Not Used
44-50 | -- | -- | Not Used
51 | 0.35 BN | 1356 | Flash To Pass Switch Signal
52-55 | -- | -- | Not Used
56 | 0.35 WH | 1390 | Off/Run/Crank Voltage
57 | 0.35 GY | 112 | Windshield Wiper Switch Low/Pulse Signal
58 | 0.35 PU | 719 | Low Reference
59 | 0.35 BN | 5360 | Low Reference
60 | -- | -- | Not Used
61 | 0.35 GY | 1884 | Cruise Control Switch Signal (K34)
62 | 0.35 WH/BK | 1073 | 5-Volt Reference
63-65 | -- | -- | Not Used
66 | 0.35 YE/BK | 1418 | Left Rear Turn Signal Switch Signal
67 | 0.35 D-GN/WH | 1419 | Right Rear Turn Signal Switch Signal
68 | 0.35 L-BU | 292 | Rear Window Defogger Grid Switch Signal
69 | 0.35 D-GN/WH | 762 | A/C Request Signal (C60)
70 | -- | -- | Not Used
71 | 0.35 PU | 5234 | Passenger Seat Belt Indicator
72 | 0.35 WH | 193 | Rear Window Defogger Grid Relay Control

### Body Control Module (BCM) X3

#### Connector Part Information

- OEM: 15492675
- Service: See Catalog
- Description: 41-Way F Metri-Pack 280 800 Series (RD)

#### Terminal Part Information

- Pins: A1, A3, A4, A5, A7, A8, A9, A10, A12, B1, D4, B3, B5, C12, D7
- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: Pins A1, A3, A4, A5, A7, A9, A10, A12, B1, B12, D4 - E/A
- Core/Insulation Crimp: Pins B3, B5, C12, D7 - E/C
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: C5, D1, D5, D6, D10, D12, D11
- Terminal/Tray: 12110842/4
- Core/Insulation Crimp: Pins C5, D1, D5, D6, D10, D12 - F/G
- Core/Insulation Crimp: Pins D11 - A/B
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Body Control Module (BCM) X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A1 | 0.5 TN | 294 | Door Lock Actuator Unlock Control (AU3)
A2 | -- | -- | Not Used
A3 | 0.5 D-BU/WH | 149 | Courtesy Lamp Supply Voltage
A4 | 0.5 GY | 295 | Door Lock Actuator Lock Control (AU3)
A5 | 0.5 GY | 295 | Door Lock Actuator Lock Control (AU3)
A6 | -- | -- | Not Used
A7 | 0.5 BN | 9 | Park Lamp Supply Voltage
A8 | 0.5 PK | 339 | Ignition 1 Voltage
A9 | 0.8 YE | 618 | Left Rear Turn Signal Lamp Supply Voltage
A10 | 0.5 GY | 157 | Courtesy Lamp Control
A11 | -- | -- | Not Used
A12 | 0.8 D-GN | 619 | Right Rear Stop/Turn Signal Lamp Supply Voltage
B1 | 0.5 TN | 694 | Driver Door Lock Actuator Unlock Control (AU3)
B2 | -- | -- | Not Used
B3 | 0.35 RD/WH | 1240 | Battery Positive Voltage
B4 | -- | -- | Not Used
B5 | 0.35 BN | 4 | Accessory Voltage
B6-B7 | -- | -- | Not Available
B8-B11 | -- | -- | Not Used
B12 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
C1-C2 | -- | -- | Not Available
C3-C4 | -- | -- | Not Used
C5 | 3.0 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
C6-C7 | -- | -- | Not Available
C8-C11 | -- | -- | Not Used
C12 | 0.35 OG | 228 | Windshield Washer Pump Control
D1 | 5.0 RD/BK | 142 | Battery Positive Voltage
D2-D3 | -- | -- | Not Used
D4 | 0.5 RD/WH | 840 | Battery Positive Voltage
D5 | 3.0 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage (AU3)
D6 | 3.0 PK | 739 | Ignition 1 Voltage
D7 | 0.35 PK | 1339 | Ignition 1 Voltage
D8-D9 | -- | -- | Not Used
D10 | 3.0 RD/BK | 442 | Battery Positive Voltage
D11 | 2.0 RD/WH | 640 | Battery Positive Voltage (UQ3)
D12 | 3.0 RD/BK | 242 | Battery Positive Voltage

### Body Control Module (BCM) X4

#### Connector Part Information

- OEM: 15492668
- Service: 88988776
- Description: 68-Way F Metri-Pack 280 Series, Flexlock (L-GY)

#### Terminal Part Information

- Pins: F2, F4, F5, F6, F6
- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: B1, C1, C8, C11, C12, D1, D3, E6, F1, F9, D10, D10
- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: Pins B1, C1, C8, C11, C12, D1, D3, E6, F1, F9 - E/C
- Core/Insulation Crimp: Pins D10 - See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: D4, E12
- Terminal/Tray: 12110842/4
- Core/Insulation Crimp: Pins D4 - F/G
- Core/Insulation Crimp: Pins E12 - A/B
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Body Control Module (BCM) X4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A1-A12 | -- | -- | Not Used
B1 | 0.35 OG | 228 | Windshield Washer Pump Control
B2-B12 | -- | -- | Not Used
C1 | 0.35 RD/WH | 1440 | Battery Positive Voltage
C2-C5 | -- | -- | Not Used
C6-C7 | -- | -- | Not Available
C8 | 0.35 BN | 4 | Accessory Voltage
C9-C10 | -- | -- | Not Used
C11 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
C12 | 0.35 GY/BK | 1458 | Instrument Panel Lamp Supply Voltage
D1 | 0.35 RD/WH | 1040 | Battery Positive Voltage
D2 | -- | -- | Not Used
D3 | 0.35 YE | 5199 | Run/Crank Relay Coil Control
D4 | 3.0 BN | 141 | Ignition 3 Voltage
D5 | -- | -- | Not Used
D6-D7 | -- | -- | Not Available
D8-D9 | -- | -- | Not Used
D10 | 0.8 RD/WH | 1140 | Battery Positive Voltage
D11-D12 | -- | -- | Not Used
E1-E5 | -- | -- | Not Used
E6 | 0.35 PK | 439 | Ignition 1 Voltage
E7-E11 | -- | -- | Not Used
E12 | 2.0 BK | 550 | Ground
F1 | 0.35 RD/WH | 1540 | Battery Positive Voltage
F2 | 0.5 GY | 8 | Instrument Panel Lamp Supply Voltage
F3 | -- | -- | Not Used
F4 | 0.5 PK | 339 | Ignition 1 Voltage
F5 | 0.35 PK | 339 | Ignition 1 Voltage
F6-F8 | -- | -- | Not Used
F9 | 0.35 PK | 1539 | Ignition 1 Voltage
F10-F12 | -- | -- | Not Used

### Brake Booster Pump Motor

#### Connector Part Information

- OEM: 7282-5575-10
- Service: See Catalog
- Description: 2-Way M 2.8 Series (D-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Brake Booster Pump Motor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5OG | 1470 | Brake Booster Pump Motor Supply Voltage
2 | 0.5 BK/WH | 1250 | Ground

### Brake Booster Vacuum Sensor

#### Connector Part Information

- OEM: 1 928 403 966
- Service: See Catalog
- Description: 3-Way F Kompakt 2.8 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Brake Booster Vacuum Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-GN | 6257 | Brake Booster Vacuum Sensor Supply Voltage
2 | 0.5 L-GN/BK | 6257 | Brake Booster Vacuum Sensor Ground
3 | 0.5 D-BU | 1809 | Brake Booster Vacuum Sensor Signal

### Brake Fluid Level Switch

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Brake Fluid Level Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 849 | Brake Fluid Level Sensor Signal
B | 0.5 BK/WH | 451 | Ground

### Brake Pedal Position (BPP) Sensor

#### Connector Part Information

- OEM: 15332132
- Service: 88953364
- Description: 3-Way F GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Brake Pedal Position (BPP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 WH | 5359 | 5-Volt Reference
B | 0.35 YE | 5361 | Brake Pedal Position Sensor Signal
C | 0.35 BN | 5360 | Low Reference

### Camshaft Position (CMP) Actuator Solenoid Valve - Exhaust

#### Connector Part Information

- OEM: 15336004
- Service: 15306187
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Camshaft Position (CMP) Actuator Solenoid Valve - Exhaust

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply (4)
B | 0.5 L-GN | 5282 | Camshaft Phaser Exhaust Solenoid Control

### Camshaft Position (CMP) Actuator Solenoid Valve - Intake

#### Connector Part Information

- OEM: 15335987
- Service: 15306430
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Camshaft Position (CMP) Actuator Solenoid Valve - Intake

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply (4)
B | 0.5 PU | 5284 | Camshaft Phaser Intake Solenoid Control

### Camshaft Position (CMP) Sensor - Exhaust

#### Connector Part Information

- OEM: 13519047
- Service: See Catalog
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Camshaft Position (CMP) Sensor - Exhaust

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 GY | 705 | 5-Volt Reference 2
B | 0.5 TN | 552 | Low Reference
C | 0.5 D-GN | 5273 | Camshaft Position Exhaust Sensor Signal

### Camshaft Position (CMP) Sensor - Intake

#### Connector Part Information

- OEM: 13519047
- Service: See Catalog
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Camshaft Position (CMP) Sensor - Intake

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 GY | 705 | 5-Volt Reference 2
B | 0.5 TN | 552 | Low Reference
C | 0.5 OG | 5275 | Camshaft Position Intake Sensor Signal

### Center High Mounted Stop Lamp (CHMSL)

#### Connector Part Information

- OEM: 15449029
- Service: See Catalog
- Description: 2-Way F GT 150 Series, Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Center High Mounted Stop Lamp (CHMSL)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 750 | Ground
B | 0.5 L-BU | 20 | Stop Lamp Supply Voltage

### Crankshaft Position (CKP) Sensor

#### Connector Part Information

- OEM: 31403-3710
- Service: See Catalog
- Description: 3-Way F 64 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 33467-0003/23
- Core/Insulation Crimp: H/H
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

#### Crankshaft Position (CKP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | 605 | 5-Volt Reference 3
2 | 0.35 TN | 452 | Low Reference
3 | 0.35 YE | 573 | Crankshaft Position Sensor Signal

### Data Link Connector (DLC)

#### Connector Part Information

- OEM: 13510085
- Service: Not Serviced
- Description: 16-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Pins: 1, 4-6, 14, 16
- Terminal/Tray: 12129484/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Data Link Connector (DLC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
2-3 | -- | -- | Not Used
4 | 0.5 BK | 550 | Ground
5 | 0.5 BK/WH | 651 | Ground
6 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus (+)
7-13 | -- | -- | Not Used
14 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-)
15 | -- | -- | Not Used
16 | 0.5 RD/WH | 40 | Battery Positive Voltage

### Data Link Resistor

#### Connector Part Information

- OEM: 15326801
- Service: 15306156
- Description: 2-Way F GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Data Link Resistor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus (+)
B | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-)

### Door Lock Actuator - Driver (AU3)

#### Connector Part Information

- OEM: 6-1355683-1
- Service: See Catalog
- Description: 6-Way F Series Sealed (BK)

#### Terminal Part Information

- Pins: 2-4, 6
- Terminal/Tray: 4-969005-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-560/J-35616-33 (YE)

#### Door Lock Actuator - Driver (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 TN | 694 | Driver Door Lock Actuator Unlock Control
3 | 0.5 GY | 295 | Door Lock Actuator Lock Control
4 | 0.35 GY/BK | 745 | Left Front Door Ajar Switch Signal
5 | -- | -- | Not Used
6 | 0.35 BK | 550 | Ground

### Door Lock Actuator - Passenger (AU3)

#### Connector Part Information

- OEM: 6-1355683-1
- Service: See Catalog
- Description: 6-Way F Series Sealed (BK)

#### Terminal Part Information

- Pins: 1, 3, 5, 6
- Terminal/Tray: 964274-2/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-560/J-35616-33 (YE)

#### Door Lock Actuator - Passenger (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN/WH | 746 | Right Front Door Ajar Switch Signal
2 | -- | -- | Not Used
3 | 0.35 BK | 550 | Ground
4 | -- | -- | Not Used
5 | 0.5 TN | 294 | Door Lock Actuator Unlock Control
6 | 0.5 GY | 295 | Door Lock Actuator Lock Control

### Door Lock Switch - Driver (AU3)

#### Connector Part Information

- OEM: 15417063
- Service: 88987857
- Description: 3-Way F Micro-Pack 064 Series (BK)

#### Terminal Part Information

- Pins: A, B
- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: Pins: E/C
- Core/Insulation Crimp: Pins: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Door Lock Switch - Driver (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 550 | Ground
B | 0.35 GY | 8 | Instrument Lamp Supply Voltage
C | 0.5 WH | 682 | Door Lock/Unlock Signal

### Door Lock Switch - Passenger (AU3)

#### Connector Part Information

- OEM: 15417063
- Service: 88987857
- Description: 3-Way F Micro-Pack 064 Series (BK)

#### Terminal Part Information

- Pins: A, B
- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: Pins: E/C
- Core/Insulation Crimp: Pins: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Door Lock Switch - Passenger (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 550 | Ground
B | 0.35 GY | 8 | Instrument Lamp Supply Voltage
C | 0.5 WH | 682 | Door Lock/Unlock Signal

### Electronic Brake Control Module (EBCM)

#### Connector Part Information

- OEM: 6-1355628-4
- Service: 19115598
- Description: 47-Way F MK25/60 Series (BK)

#### Terminal Part Information

- Pins: 1, 16
- Terminal/Tray: 7114-4142-02/10
- Core/Insulation Crimp: A/3
- Release Tool/Test Probe: 12094430/J-35616-43 (RD)

- Pins: 2-15, 17-31, 33-47
- Terminal/Tray: 638551-3
- Core/Insulation Crimp: See Terminal Repair
- Release Tool/Test Probe: See Terminal Repair Kit

- Pins: 32
- Terminal/Tray: 7114-4141-02
- Core/Insulation Crimp: See Terminal Repair
- Release Tool/Test Probe: See Terminal Repair Kit

#### Electronic Brake Control Module (EBCM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3.0 RD/BK | 542 | Low Reference
2-7 | -- | -- | Not Used
8 | 0.5 PK | 1439 | Ignition 1 Voltage
9-10 | -- | -- | Not Used
11 | 0.5 TN/BK | 2500 | High Speed Serial Data Bus (+)
12 | 0.5 TN/BK | 2500 | High Speed Serial Data Bus (+)
13 | 0.5 TN | 2501 | High Speed Serial Data Bus (-)
14 | 0.5 TN | 2501 | High Speed Serial Data Bus (-)
15 | -- | -- | Not Used
16 | 3.0 BK | 350 | Ground
17 | -- | -- | Not Used
18 | 0.5 PK/BK | 6434 | Can Bus High Serial Data
19 | 0.5 GY/BK | 6435 | Can Bus Low Serial Data
20-21 | -- | -- | Not Used
22 | 0.5 D-GN | 2087 | 12-Volt Reference
23-25 | -- | -- | Not Used
26 | 0.5 L-GN | 6257 | Brake Booster Vacuum Sensor Supply Voltage
27 | 0.5 L-GN/BK | 6258 | Brake Booster Vacuum Sensor Ground
28 | -- | -- | Not Used
29 | 0.5 L-BU | 2088 | Low Reference
30-31 | -- | -- | Not Used
32 | 2.0 RD/WH | 540 | Battery Positive Voltage
33 | 0.5 TN | 833 | Low Reference
34 | 0.5 D-GN | 872 | Right Front Wheel Speed Sensor Signal
35 | -- | -- | Not Used
36 | 0.5 TN | 884 | Left Rear Wheel Speed Sensor Signal
37 | 0.5 OG | 885 | Low Reference
38-40 | -- | -- | Not Used
41 | 0.5 D-BU | 1809 | Brake Booster Vacuum Sensor Signal
42 | 0.5 WH | 883 | Low Reference
43 | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal
44 | -- | -- | Not Used
45 | 0.5 L-BU | 830 | Left Front Wheel Speed Sensor Signal
46 | 0.5 YE | 873 | Low Reference
47 | -- | -- | Not Used

### Engine Control Module (ECM) X1

#### Connector Part Information

- OEM:1 928 404 781
- Service: 19149311
- Description: 96-Way F 120 MAT, 280 BDK Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498135/19
- Core/Insulation Crimp: Pins: 1-2,6-7,15-18,24,34,36-39,41-42,44,48,59-60,64,66-68,82-84,86,88,89-92,95-96 - J/J
- Core/Insulation Crimp: Pins: 5,26-29, 51-53,73,75 - K/K
- Core/Insulation Crimp: Pins: 10,13,30,35,45-46,54-56,78-80 - P/P
- Release Tool/Test Probe: J-38125-213/J-35616-16 (L-GN)

#### Engine Control Module (ECM) X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-9 | -- | -- | Not Used
10 | 0.35 OG | 225 | Generator Turn On Signal
11-12 | -- | -- | Not Used
13 | 0.35 BN/WH | 2130 | Low Reference
14 | -- | -- | Not Used
15 | 0.5 GY | 705 | 5-Volt Reference 2
16 | 0.5 D-GN | 6391 | Turbocharger Bypass Valve Control
17 | 0.5 TN/BK | 231 | Oil Pressure Switch Signal
18 | 0.5 YE | 258 | Turbocharger Wastegate Solenoid Control
19-23 | -- | -- | Not Used
24 | 0.8 YE | 581 | Throttle Actuator Control Open
25 | -- | -- | Not Used
26 | 1.0 L-BU | 4804 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 4
27 | 1.0 L-BU/WH | 4904 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 4
28 | 1.0 D-BU | 4802 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 2
29 | 1.0 D-BU/WH | 4902 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 2
30 | 0.35 GY | 23 | Generator Field Duty Cycle Signal
31-33 | -- | -- | Not Used
34 | 0.5 D-GN | 5273 | Camshaft Position Exhaust Sensor Signal
35 | 0.35 YE | 573 | Crankshaft Position Sensor Signal
36 | 0.5 YE | 2918 | Fuel Rail Pressure Sensor Signal
37 | 0.5 L-GN | 432 | Manifold Absolute Pressure Sensor Signal
38 | 0.5 GY | 598 | 5-Volt Reference 1
39 | 0.5 GY | 2701 | 5-Volt Reference 3
40 | -- | -- | Not Used
41 | 0.5 TN | 552 | Low Reference
42 | 0.5 TN | 808 | Low Reference
43 | -- | -- | Not Used
44 | 0.5 TN | 2761 | Low Reference
45 | 0.5 GY | 605 | 5-Volt Reference 3
46 | 0.35 TN | 452 | Low Reference
47 | -- | -- | Not Used
48 | 0.8 BN | 582 | Throttle Actuator Control Closed
49-50 | -- | -- | Not Used
51 | 1.0 BN | 4801 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 1
52 | 1.0 D-GN | 4803 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 3
53 | 1.0 D-GN/WH | 4903 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 3
54 | 0.35 BN/WH | 419 | MIL Control
55 | 0.35 PU | 2121 | IC 1 Control
56 | 0.35 D-GN/WH | 2124 | IC 4 Control
57-58 | -- | -- | Not Used
59 | 0.5 D-BU | 496 | Knock Sensor 1 Signal
60 | 0.5 GY | 2303 | Knock Sensor 2 Signal
61-63 | -- | -- | Not Used
64 | 0.5 TN | 407 | Low Reference
65 | -- | -- | Not Used
66 | 0.5 PU | 7330 | Pre-Throttle Air Temp and Press (TMAP) Air Pressure Signal
67 | 0.5 TN/WH | 3111 | Heated Oxygen Sensor Low Signal Sensor 1
68 | 0.5 WH | 5279 | Heated Oxygen Sensor Pump Current Sensor 1
69-72 | -- | -- | Not Used
73 | 1.0 PU | 7300 | High Pressure Fuel Pump Actuator Low Control
74 | -- | -- | Not Used
75 | 1.0 BN/WH | 4901 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 1
76-77 | -- | -- | Not Used
78 | 0.35 BN | 2129 | Low Reference
79 | 0.35 L-BU | 2123 | IC 3 Control
80 | 0.35 OG/WH | 2122 | IC 2 Control
81 | -- | -- | Not Used
82 | 0.5 YE | 410 | Engine Coolant Temperature Sensor Signal
83 | 0.5 GY | 1716 | Knock Sensor 1 Signal
84 | 0.5 L-BU | 1876 | Knock Sensor 2 Signal
85 | -- | -- | Not Used
86 | 0.5 L-BU | 7329 | Pre-Throttle Air Temp and Press (TMAP) Temperature Signal
87 | -- | -- | Not Used
88 | 0.5 TN | 2752 | Low Reference
89 | 0.5 PU | 486 | Throttle Position Sensor 2 Signal
90 | 0.5 D-GN | 485 | Throttle Position Sensor 1 Signal
91 | 0.5 L-GN | 5278 | Heated Oxygen Sensor Input Pump Current Sensor 1
92 | 0.5 PU/WH | 3110 | Heated Oxygen Sensor High Signal Sensor 1
93-94 | -- | -- | Not Used
95 | 0.5 GY | 597 | 5-Volt Reference 1
96 | 0.5 GY/WH | 3113 | Heated Oxygen Sensor Heater Low Control Sensor 1

### Engine Control Module (ECM) X2

#### Connector Part Information

- OEM: 1 928 404 916
- Service: 19115599
- Description: 58-Way F 280 Series, Sealed (BK)

#### Terminal Part Information

- Pins:10-11,12-19,22-23,25,27,31, 34-36,38-39,41-42,44,46-50,52,54-56,58
- Terminal/Tray: 1928498135/19
- Core/Insulation Crimp: Pins: 10,12-14,16, 18-19,22,27,31, 36,38,42,50,54-56 - J/J
- Core/Insulation Crimp: Pins: 11,15,17,23,25,34-35,39,41,44,46-49,52,58 - P/P
- Release Tool/Test Probe: J-38125-213/J-35616-16 (L-GN)

#### Engine Control Module (ECM) X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-9 | -- | -- | Not Used
10 | 0.5 D-GN/WH | 465 | Fuel Pump Relay Control
11 | 0.35 TN | 5514 | Low Reference (C60)
12 | -- | -- | Not Used
13 | 0.8 YE | 492 | Mass Air Flow Sensor Signal
14 | 0.5 GY | 2709 | 5-Volt Reference 1
15 | 0.35 D-BU | 1161 | Accelerator Pedal Position Sensor 1 Signal
16 | -- | -- | Not Used
17 | 0.35 OG/BK | 1786 | Transmission Park/Neutral Signal (M82)
18 | 0.5 L-GN | 24 | Backup Lamp Supply Voltage (M82)
19 | 0.5 WH | 1310 | Evaporative Emission Canister Vent Solenoid Control
20-21 | -- | -- | Not Used
22 | 0.8 TN | 2760 | Low Reference
23 | 0.5 TN/WH | 3121 | Heated Oxygen Sensor Low Signal Sensor 2
24 | -- | -- | Not Used
25 | 0.35 L-BU | 1162 | Accelerator Pedal Position Sensor 2 Signal
26 | -- | -- | Not Used
27 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal
28-33 | -- | -- | Not Used
34 | 0.35 BN | 1271 | Low Reference
35 | 0.35 GY | 2700 | 5-Volt Reference 3
36 | 0.5 PU | 1589 | Fuel Level Sensor Signal
37 | -- | -- | Not Used
38 | 0.5 PU | 3120 | Heated Oxygen Sensor High Signal Sensor 2
39 | 0.35 OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal (C60)
40 | -- | -- | Not Used
41 | 0.35 BN | 4 | Accessory Voltage
42 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus (+)
43 | -- | -- | Not Used
44 | 0.35 D-GN/WH | 459 | A/C Compressor Clutch Relay Control (C60)
45 | -- | -- | Not Used
46 | 0.35 WH | 2368 | Cooling Fan Speed Control
47 | 0.35 PU | 1272 | Low Reference
48 | 0.35 TN | 1274 | 5-Volt Reference 3
49 | 0.35 WH/BK | 1164 | 5-Volt Reference 2
50 | 0.8 L-BU | 6289 | Induction Air Temperature Sensor Signal
51 | -- | -- | Not Used
52 | 0.35 L-BU | 20 | Stop Lamp Supply Voltage (M82)
53 | -- | -- | Not Used
54 | 0.5 PK | 1039 | Ignition 1 Voltage
55 | 0.5 TN | 2501 | High Speed GMLAN Serial Data BUS (-)
56 | 0.5 RD/WH | 840 | Battery Positive Voltage
57 | 0.35 PU/WH | 6386 | Starter Relay Coil Control
58 | 0.35 YE | 5991 | Powertrain Relay Coil Control

### Engine Coolant Level Switch

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Engine Coolant Level Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-GN | 1478 | Coolant Level Switch Signal
B | 0.5 BK/WH | 451 | Ground

### Engine Coolant Temperature (ECT) Sensor

#### Connector Part Information

- OEM: 13584122
- Service: 88987993
- Description: 2-Way F Metri-Pack 150.2 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Engine Coolant Temperature (ECT) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN | 2761 | Low Reference
B | 0.5 YE | 410 | Engine Coolant Temperature Sensor Signal

### Engine Cooling Fan

#### Connector Part Information

- OEM: 7283-8496-30
- Service: 19115593
- Description: 4-Way F Mixed Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Pins 1, 2 7116-3250/10 Pins: 4 7116-4110-02/9
- Core/Insulation Crimp: Pins 1, 2 See Terminal Repair Kit Pins: 4 E/C
- Release Tool/Test Probe: Pins: 1, 2 12094430/J-35616-22 (RD) Pins: 4 12094430/J-35616-4A (PU)

#### Engine Cooling Fan

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 8.0 RD/BK | 342 | Battery Positive Voltage
2 | 8.0 BK | 650 | Ground
3 | -- | -- | Not Available
4 | 0.35 WH | 2368 | Cooling Fan Speed Control

### Engine Oil Pressure (EOP) Switch

#### Connector Part Information

- OEM: 15474881
- Service: 88988620
- Description: 4-Way F Metri-Pack 150 Series Sealed (GY)

#### Terminal Part Information

- Pins: A
- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Engine Oil Pressure (EOP) Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/BK | 231 | Oil Pressure Switch Signal
B-D | -- | -- | Not Available

### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

#### Connector Part Information

- OEM: 12052643
- Service: 12101858
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 5291 | Ignition 1 Voltage
B | 0.5 D-GN/WH | 428 | Evaporative Emission Canister Purge Solenoid Control

### Evaporative Emission (EVAP) Canister Vent Solenoid Valve

#### Connector Part Information

- OEM: 12052643
- Service: 12101858
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Evaporative Emission (EVAP) Canister Vent Solenoid Valve

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 RD/WH | 140 | Battery Positive Voltage
B | 0.5 WH | 1310 | Evaporative Emission Canister Vent Solenoid Control

### Evaporator Temperature Sensor (C60)

#### Connector Part Information

- OEM: 12047662
- Service: 12085535
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Evaporator Temperature Sensor (C60)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 YE | 1791 | Low Reference
B | 0.35 GY | 6137 | Evaporator Core Temperature Sensor Signal

### Fog Lamp - Left Front (T96)

#### Connector Part Information

- OEM: 12124819
- Service: 12085498
- Description: 2-Way F Metri-Pack 280 Series (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fog Lamp - Left Front (T96)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PU | 2234 | Front Fog Lamp Supply Voltage
B | 0.5 BK | 150 | Ground

### Fog Lamp - Right Front (T96)

#### Connector Part Information

- OEM: 12124819
- Service: 12085498
- Description: 2-Way F Metri-Pack 280 Series, Sealed (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fog Lamp - Right Front (T96)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PU | 2234 | Front Fog Lamp Supply Voltage
B | 0.5 BK | 250 | Ground

### Fog Lamp Switch (T96)

#### Connector Part Information

- OEM: 15419483
- Service: 89046742
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Fog Lamp Switch (T96)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK | 550 | Ground
B | -- | -- | Not Used
C | 0.35 OG | 192 | Front Fog Lamp Switch Signal
D | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage

### Folding Top Cover Actuator

#### Connector Part Information

- OEM: 15326870
- Service: 88953160
- Description: 2-Way FGT 280 (BK)

#### Terminal Part Information

- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: 2/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Folding Top Cover Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 TN/WH | 56 | Trunk Release Motor Supply Voltage
B | 1.0 BK | 850 | Ground

### Fuel Injector 1

#### Connector Part Information

- OEM: 1 928 403 874
- Service: See Catalog
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.0 TN | 4801 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 1
2 | 1.0 TN | 4901 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 1

### Fuel Injector 2

#### Connector Part Information

- OEM: 1 928 403 874
- Service: See Catalog
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.0 TN | 4802 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 2
2 | 1.0 TN | 4902 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 2

### Fuel Injector 3

#### Connector Part Information

- OEM: 1 928 403 874
- Service: See Catalog
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.0 TN | 4803 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 3
2 | 1.0 TN | 4903 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 3

### Fuel Injector 4

#### Connector Part Information

- OEM: 1 928 403 874
- Service: See Catalog
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.0 TN | 4804 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 4
2 | 1.0 TN | 4904 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 4

### Fuel Pump and Sender Assembly

#### Connector Part Information

- OEM: 15326631
- Service: 15306360
- Description: 4-Way F GT 280 Series Sealed (BK)

#### Terminal Part Information

- Pins: A, D, B, C
- Terminal/Tray: 15304719/19
- Core/Insulation Crimp: Pins A, D - 2/5
- Core/Insulation Crimp: Pins B, C - E/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Fuel Pump and Sender Assembly

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 BK | 750 | Ground
B | 0.5 PU | 1589 | Fuel Level Sensor Signal
C | 0.5 TN | 2759 | Low Reference
D | 1.0 GY | 120 | Fuel Pump Supply Voltage

### Fuel Rail Pressure (FRP) Sensor

#### Connector Part Information

- OEM: 1 928 403 966
- Service: See Catalog
- Description: 3-Way F 2.8 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Rail Pressure (FRP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN | 808 | Low Reference
2 | 0.5 YE | 2918 | Fuel Rail Pressure Sensor Signal
3 | 0.5 GY | 598 | 5-Volt Reference 1

### Fuel Tank Pressure (FTP) Sensor

#### Connector Part Information

- OEM: 13511996
- Service: 88986451
- Description: 3-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Fuel Tank Pressure (FTP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal
2 | 0.5 TN | 2759 | Low Reference
3 | 0.5 GY | 2709 | 5-Volt Reference 1

### Generator X1

#### Connector Part Information

- OEM: 12186568
- Service: See Catalog
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Pins: B, C
- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Generator X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 OG | 225 | Generator Turn On Signal
C | 0.35 GY | 23 | Generator Field Duty Cycle Signal
D | -- | -- | Not Used

### Generator X2

#### Terminal Part Information

- Terminal: 12146365
- Description: Ring Terminal

#### Generator X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 19 RD | 2 | Battery Positive Voltage

### Ground Table

#### Terminal Part Information

- Terminal: 12146365
- Description: Ring Terminal

#### Ground Table

Ground | Wire | Circuit | Ring Terminal
--- | --- | --- | ---
G101 - X1 | 0.8 BK | 150 | 15355522
G102 - X1 | 1.0 BK | 250 | 12162100
G102 - X2 | 8.0 BK | 650 | 15354754
G103 - X1 | 0.8 BK | 450 | 15355521
G104 - X1 | 3.0 BK/WH | 451 | 12103506
G105 - X1 | 5.0 BK | 350 | 15354757
G106 - X1 | 13.0 BK | 50 | 13588147
G300 - X1 | 2.0BK | 550 | R-62287-004-B1
3.0BK
G300 - X2 | 2.0 BK/WH | 651 | R-62287-002-B1
G301 - X1 | 0.5 BK/WH | 851 | R-3020-004
G301 - X2 | 1.0 BK | 850 | R-62287-002-B1
G302 - X1 | -- | -- | Not Used
G302 - X2 | 0.8 BK/WH | 551 | R-3020-004
G303 - X1 | 2.0 BK/WH | 751 | R-62287-002-B1
G304 - X1 | 0.5 BK/WH | 351 | R-62287-005-B1
0.5 BK/WH
G304 - X2 | 0.5 BK | 1150 | R-62287-005-B1
0.5 BK
G400 - X1 | 0.8 BK | 1050 | R-3020-004
G402 - X1 | 0.8 BK | 750 | R-3020-004

### Hazard Warning Switch

#### Connector Part Information

- OEM: 12047781
- Service: 12102900
- Description: 3-Way F Metri-Pack 150 Series (NA)

#### Terminal Part Information

- Pins: A, B, C
- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Hazard Warning Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
B | 0.35 BK | 550 | Ground
C | 0.35 WH | 111 | Hazard Warning Switch Signal

### Headlamp - Left High Beam

#### Connector Part Information

- OEM: 15393199
- Service: 88987187
- Description: 2-Way F Metri-Pack 280 Series, Sealed (GY)

#### Terminal Part Information

- Terminal: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Left High Beam

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BK | -- | Left Headlamp High Beam Supply Voltage
B | 0.8 BK | -- | Ground

### Headlamp - Left Low Beam

#### Connector Part Information

- OEM: 15393199
- Service: 88987187
- Description: 2-Way F Metri-Pack 280 Series, Sealed (GY)

#### Terminal Part Information

- Terminal: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Left Low Beam

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 RD | -- | Left Headlamp Low Beam Supply Voltage
B | 0.8 BK | -- | Ground

### Headlamp - Right High Beam

#### Connector Part Information

- OEM: 15393199
- Service: 88987187
- Description: 2-Way F Metri-Pack 280 Series, Sealed (GY)

#### Terminal Part Information

- Terminal: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Right High Beam

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BK | -- | Right Headlamp High Beam Supply Voltage
B | 0.8 BK | -- | Ground

### Headlamp - Right Low Beam

#### Connector Part Information

- OEM: 15393199
- Service: 88987187
- Description: 2-Way F Metri-Pack 280 Series, Sealed (GY)

#### Terminal Part Information

- Terminal: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Right Low Beam

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 RD | -- | Right Headlamp Low Beam Supply Voltage
B | 0.8 BK | -- | Ground

### Heated Oxygen Sensor (HO2S) 1

#### Connector Part Information

- OEM: 1 928 404 900
- Service: See Catalog
- Description: 6-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Oxygen Sensor (HO2S) 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 WH | 5279 | Heated Oxygen Sensor Pump Current Sensor 1
2 | 0.5 TN/WH | 3111 | Heated Oxygen Sensor Low Signal Sensor 1
3 | 0.5 GY/WH | 3113 | Heated Oxygen Sensor Heater Low Control Sensor
4 | 0.5 PK/BK | 5291 | Ignition 1 Voltage
5 | 0.5 L-GN | 5278 | Heated Oxygen Sensor Input Pump Current Sensor 1
6 | 0.5 PU/WH | 3110 | Heated Oxygen Sensor High Signal Sensor 1

### Heated Oxygen Sensor (HO2S) 2

#### Connector Part Information

- OEM: 15326423
- Service: See Catalog
- Description: 4-Way M Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Oxygen Sensor (HO2S) 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/WH | 3121 | Heated Oxygen Sensor Low Signal Sensor 2
B | 0.5 PU | 3120 | Heated Oxygen Sensor High Signal Sensor 2
C | 0.5 GY/WH | 3122 | Heated Oxygen Sensor Heater Low Control Sensor 2
D | 0.5 PK/BK | 5291 | Ignition 1 Voltage

### High Pressure Fuel Pump

#### Connector Part Information

- OEM: 1 928 403 874
- Service: See Catalog
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### High Pressure Fuel Pump

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.0 PU | 7300 | High Pressure Fuel Pump Actuator Low Control
2 | 1.0 YE | 7301 | High Pressure Fuel Pump Actuator High Control

### Horn - Left

#### Connector Part Information

- OEM: E-2157-000
- Service: See Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4103-0819
- Core/Insulation Crimp: 2E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Horn - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 BK | 150 | Ground
2 | 0.8 D-GN | 29 | Horn Control

### Horn - Right

#### Connector Part Information

- OEM: E-2157-000
- Service: 88988305
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4103-0819
- Core/Insulation Crimp: 2E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Horn - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 BK | 250 | Ground
2 | 0.8 D-GN | 29 | Horn Control

### Horn Switch X1

#### Connector Part Information

- OEM: C-173531-1
- Service: See Catalog
- Description: 1-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Horn Switch X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 TN | 28 | Horn Relay Control

### Horn Switch X2

#### Connector Part Information

- OEM: C-174463-1
- Service: See Catalog
- Description: 1-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Horn Switch X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK | 1150 | Ground

### HVAC Control Module X1

#### Connector Part Information

- OEM: 15118642
- Service: 88988350
- Description: 5-Way F (BK)

#### Terminal Part Information

- Pins: 1, 5
- Terminal/Tray: 964328-1/25
- Core/Insulation Crimp: 4/B
- Release Tool/Test Probe: 12093647/J-35616-40 (BU)

- Pins: 2, 3, 4
- Terminal/Tray: 927837-1/25
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12093647/J-35616-40 (BU)

#### HVAC Control Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3.0 OG | 52 | Blower Motor High Control
2 | 2.0 L-BU | 72 | Medium 2 Blower Motor Control
3 | 2.0 TN | 63 | Blower Motor Medium Control (1)
4 | 2.0 YE | 60 | Blower Motor Low Control
5 | 3.0 BK | 550 | Ground

### HVAC Control Module X2

#### Connector Part Information

- OEM: 15336594
- Service: 15336594
- Description: 12-Way F Micro-Pack 100 Series (GY)

#### Terminal Part Information

- Pins: B, C, D, F, G, J, K, L
- Terminal/Tray: 12146447/3
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### HVAC Control Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 RD/WH | 1540 | Battery Positive Voltage
C | 0.35 BK | 550 | Ground
D | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
E | -- | -- | Not Used
F | 0.35 WH | 193 | Rear Defog Relay Control
G | 0.35 D-GN/WH | 762 | A/C Request Signal
H | -- | -- | Not Used
J | 0.35 L-BU | 292 | Rear Defog Switch Signal
K | 0.5 PK | 339 | Ignition 1 Voltage
L | 0.35 BK/WH | 651 | Ground
M | -- | -- | Not Used

### HVAC Control Module X3

#### Connector Part Information

- OEM: 12064799
- Service: 15305996
- Description: 12-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12146447/3
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### HVAC Control Module X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 YE | 1791 | Low Reference
B | 0.35 L-GN/BK | 2276 | Defrost Door Position Signal
C | 0.35 GY | 6137 | Evaporator Core Temperature Sensor Signal
D | 0.35 D-BU | 1646 | Auxiliary Air Temperature Door Position Signal
E | 0.35 L-BU | 733 | Air Temperature Door Position Signal
F | 0.35 L-BU/BK | 1688 | 5-Volt Reference
G | 0.35 D-GN | 1614 | Recirculation Door Control
H | 0.35 TN/BK | 2274 | Recirculation Door Control Circuit
J | 0.35 L-GN | 2275 | Mode Door Position Signal
K | 0.35 TN | 2273 | Mode Door Control
L | 0.35 L-GN/BK | 1647 | Recirculation Door Control B
M | 0.35 D-BU | 1199 | Air Temperature Door Control

### I/P Dimmer Switch

#### Connector Part Information

- OEM: 12020299
- Service: See Catalog
- Description: 5-Way F P/C Edgeboard - Standard (NA)

#### Terminal Part Information

- Terminal: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### I/P Dimmer Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 PU | 719 | Low Reference
C | 0.35 D-GN | 44 | Instrument Panel Lamp Dimmer Switch Signal
D-E | -- | -- | Not Used

### Ignition Coil 1

#### Connector Part Information

- OEM: 7283-3392-30
- Service: 88988338
- Description: 4-Way F GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Ignition Coil 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 450 | Ground
2 | 0.35 BN | 2129 | Low Reference
3 | 0.35 PU | 2121 | IC 1 Control
4 | 0.5 PK/BK | 5292 | Ignition 1 Voltage

### Ignition Coil 2

#### Connector Part Information

- OEM: 7283-3392-30
- Service: 88988338
- Description: 4-Way F GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Ignition Coil 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 450 | Ground
2 | 0.35 BN/WH | 2130 | Low Reference
3 | 0.35 OG/WH | 2122 | IC 2 Control
4 | 0.5 PK/BK | 5292 | Ignition 1 Voltage

### Ignition Coil 3

#### Connector Part Information

- OEM: 7283-3392-30
- Service: 88988338
- Description: 4-Way F GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Ignition Coil 3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 450 | Ground
2 | 0.35 BN | 2129 | Low Reference
3 | 0.35 L-BU | 2123 | IC 3 Control
4 | 0.5 PK/BK | 5292 | Ignition 1 Voltage

### Ignition Coil 4

#### Connector Part Information

- OEM: 7283-3392-30
- Service: 88988338
- Description: 4-Way F GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Ignition Coil 4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 450 | Ground
2 | 0.35 BN/WH | 2130 | Low Reference
3 | 0.35 D-GN/WH | 2124 | IC 4 Control
4 | 0.5 PK/BK | 5292 | Ignition 1 Voltage

### Ignition Switch

#### Connector Part Information

- OEM: 1L-AG5-6S-S3C1
- Service: See Catalog
- Description: 6-Way F 1L - AG5 Series (GN)

#### Terminal Part Information

- Pins: 2, 3, 4, 5, 6
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Ignition Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 RD/WH | 1040 | Battery Positive Voltage
3 | 0.35 YE | 5199 | Run/Crank Relay Coil Control
4 | 0.35 BN | 4 | Accessory Voltage
5 | 0.35 WH | 1390 | Off/Run/Crank Voltage
6 | 0.35 WH/BK | 1073 | Ignition Key Resistor Signal

### Inflatable Restraint Front End Sensor - Left

#### Connector Part Information

- OEM: 15356727
- Service: 15306405
- Description: 2-Way F GT 150 Series Sealed 4.0 (YE)

#### Terminal Part Information

- Terminal/Tray: Serviced with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Front End Sensor - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/OG | 5045 | Low Reference
B | 0.5 YE | 1834 | Forward Discriminating Sensor Signal

### Inflatable Restraint Front End Sensor - Right

#### Connector Part Information

- OEM: 15356727
- Service: 15306405
- Description: 2-Way F GT 150 Series Sealed 4.0 (YE)

#### Terminal Part Information

- Terminal/Tray: Serviced with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Front End Sensor - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 GY | 5600 | Low Reference
B | 0.5 YE/BK | 2160 | Front End Discriminating Sensor Signal

### Inflatable Restraint I/P Module X1

#### Connector Part Information

- OEM: 54550268
- Service: Service By Complete Passenger Air Bag Jumper Harness
- Description: 2-Way F Micro-Pack 100 Series (GY) With (YE) Case

#### Terminal Part Information

- Terminal/Tray: Serviced with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: N/A

#### Inflatable Restraint I/P Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 3024 | Instrument Panel Module - Stage 1 - Low Control
B | 0.5 L-BU/RD | 3025 | Instrument Panel Module - Stage 1 - High Control

### Inflatable Restraint I/P Module X2

#### Connector Part Information

- OEM: 54550266
- Service: Service By Complete Passenger Air Bag Jumper
- Description: 2-Way F Micro-Pack 100 Series (PU) With (YE) Case

#### Terminal Part Information

- Terminal/Tray: Serviced with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: N/A

#### Inflatable Restraint I/P Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-GN/RD | 3026 | Instrument Panel Module - Stage 2 - Low Control
B | 0.5 RD/WH | 3027 | Instrument Panel Module - Stage 2 - High Control

### Inflatable Restraint I/P Module Indicator

#### Connector Part Information

- OEM: HCMPB-05-5
- Service: Not Serviced
- Description: 5-Way F HCM Series (NA)

#### Terminal Part Information

- Terminal/Tray: Serviced with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Inflatable Restraint I/P Module Indicator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN/BK | 723 | Instrument Panel Module Disable Switch Signal
2 | 0.35 BK/WH | 651 | Ground
3 | 0.35 PK | 353 | Instrument Panel Module Suppression Indicator Control
4 | 0.5 PK | 339 | Ignition 1 Voltage
5 | 0.35 PU | 5234 | Passenger Seat Belt Indicator

### Inflatable Restraint Passenger Presence System (PPS) Module

#### Connector Part Information

- OEM: 15332142
- Service: 89046638
- Description: 6-Way M GT 150 Series (BK)

#### Terminal Part Information

- Pins: A, B, C, D, E
- Terminal/Tray: Serviced with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Passenger Presence System (PPS) Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PK | 1339 | Ignition 1 Voltage
B | 0.35 PK | 5018 | Occupant Sensor Serial Data
C | 0.35 TN/BK | 723 | Instrument Panel Module Disable Switch Signal
D | 0.35 BK/WH | 351 | Ground
E | 0.35 PK | 353 | Instrument Panel Module Suppression Indicator Control
F | -- | -- | Not Used

### Inflatable Restraint Sensing and Diagnostic Module (SDM)

#### Connector Part Information

- OEM: 6-638595-2
- Service: 88988363
- Description: 60-Way F (YE)

#### Terminal Part Information

- Terminal/Tray: Serviced with Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Sensing and Diagnostic Module (SDM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD/WH | 1240 | Battery Positive Voltage
2 | 0.35 D-GN/YE | 5060 | Low Speed GMLAN Serial Data
3 | 0.35 PK | 5057 | Low Reference
4 | 0.35 TN/WH | 238 | Seat Belt Switch - Left
5 | -- | -- | Not Used
6 | 0.35 OG | 1362 | Seat Belt Switch - Right - Signal
7 | -- | -- | Not Used
8-11 | -- | -- | Not Available
12 | 0.5 PU | 3026 | Instrument Panel Module Stage 2 Low Control
13 | 0.5 GY | 3027 | Instrument Panel Module Stage 2 High Control
14 | 0.5 TN | 3021 | Steering Wheel Module - Stage 1 High Control
15 | 0.5 BN | 3020 | Steering Wheel Module - Stage 1 Low Control
16 | 0.5 PK | 3022 | Steering Wheel Module - Stage 2 Low Control
17 | 0.5 WH | 3023 | Steering Wheel Module - Stage 2 High Control
18 | 0.5 YE | 3025 | Instrument Panel Module - Stage 1 High Control
19 | 0.5 OG | 3024 | Instrument Panel Module - Stage 1 Low Control
20-30 | -- | -- | Not Available
31 | 0.5 BK/WH | 351 | Ground
32 | -- | -- | Not Available
33 | 0.35 PK | 1339 | Ignition 1 Voltage
34-35 | -- | -- | Not Available
36 | 0.5 GY | 5600 | Front End Sensor - Voltage - Right
37 | 0.5 YE/BK | 2160 | Front End Sensor - Signal - Right
38 | 0.5 YE | 1834 | Front End Sensor - Voltage - Left
39 | 0.5 TN/OG | 5045 | Front End Sensor - Signal - Left
40-51 | -- | -- | Not Available
52 | 0.5 L-GN | 2116 | Seat Belt Pretensioner - Right - High Control
53 | 0.5 OG | 2117 | Seat Belt Pretensioner - Right - Low Control
54-55 | -- | -- | Not Available
56 | 0.5 TN/WH | 2118 | Seat Belt Pretensioner - Left - High Control
57 | 0.5 OG/BK | 2119 | Seat Belt Pretensioner - Left - Low Control
58-59 | -- | -- | Not Available
60 | 0.35 PK | 5018 | Occupant Sensor Serial Data

### Inflatable Restraint Steering Wheel Module X1

#### Connector Part Information

- OEM: 15359118
- Service: See Catalog
- Description: 2-Way F Micro-Pack 100 Series (GY) With (YE) Case

#### Terminal Part Information

- Terminal/Tray: Serviced with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: N/A

#### Inflatable Restraint Steering Wheel Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
B | 0.5 TN | 3021 | Steering Wheel Module - Stage 1 - High Control
A | 0.5 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control

### Inflatable Restraint Steering Wheel Module X2

#### Connector Part Information

- OEM: 54560222
- Service: See Catalog
- Description: 2-Way F Micro-Pack 100 Series (PU) With (YE) Case

#### Terminal Part Information

- Terminal/Tray: Serviced with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: N/A

#### Inflatable Restraint Steering Wheel Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 3022 | Steering Wheel Module - Stage 2 - Low Control
B | 0.5 WH | 3023 | Steering Wheel Module - Stage 2 - High Control

### Inflatable Restraint Steering Wheel Module Coil X1

#### Connector Part Information

- OEM: 15393433
- Service: 22710638
- Description: 10-Way F Micro-Pack 064 Series, Unsealed (BK)

#### Terminal Part Information

- Pins: C, D, E, F, G, H, J, K
- Terminal/Tray: 12177007/19
- Core/Insulation Crimp: E/2
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Inflatable Restraint Steering Wheel Module Coil X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | 0.35 PK | 1539 | Ignition 1 Voltage
D | 0.35 GY | 1884 | Cruise Control Switch Signal (K34)
E | 0.35 D-BU | 1796 | Steering Wheel Controls Signal (UK3)
F | 0.35 WH/BK | 644 | 10-Volt Reference
G | 0.35 GY | 1458 | Instrument Panel Lamp Supply Voltage (UK3)
H | 0.35 D-GN/WH | 1358 | Driver Information Center Switch Signal
J | 0.35 TN | 28 | Horn Relay Control
K | 0.35 BK | 1150 | Ground

### Inflatable Restraint Steering Wheel Module Coil X2

#### Connector Part Information

- OEM: 15393433
- Service: 22710638
- Description: 10-Way F Micro-Pack 064 Series, Unsealed (BK)

#### Terminal Part Information

- Pins: C, D, E, F, G, H, J, K
- Terminal/Tray: 12177007/19
- Core/Insulation Crimp: E/2
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Inflatable Restraint Steering Wheel Module Coil X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | 0.35 PK | 1539 | Ignition 1 Voltage
D | 0.35 GY | 1884 | Cruise Control Switch Signal (K34)
E | 0.35 D-BU | 1796 | Steering Wheel Controls Signal (UK3)
F | 0.35 WH/BK | 644 | 10-Volt Reference (UK3)
G | 0.35 GY/BK | 1458 | Instrument Panel Lamp Supply Voltage
H | 0.35 D-GN/WH | 1358 | Driver Information Center Switch Signal
J | 0.35 TN | 28 | Horn Relay Control
K | 0.5 BK | 1150 | Ground

### Inflatable Restraint Steering Wheel Module Coil X3

#### Connector Part Information

- OEM: 15393421
- Service: 88987853
- Description: 4-Way F Micro-Pack 064 (YE)

#### Terminal Part Information

- Terminal/Tray: Serviced with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: N/A

#### Inflatable Restraint Steering Wheel Module Coil X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control
2 | 0.5 TN | 3021 | Steering Wheel Module - Stage 1 - High Control
3 | 0.5 PK | 3022 | Steering Wheel Module - Stage 2 - Low Control
4 | 0.5 WH | 3023 | Steering Wheel Module - Stage 2 High Control

### Input Speed Sensor (ISS), Wiring Harness Side (M82)

#### Connector Part Information

- OEM: 12162201
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150.2 Series P2S (NA)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Input Speed Sensor (ISS), Wiring Harness Side (M82)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | YE | 1230 | Automatic Transmission Input Speed Sensor High Signal
B | WH | 1231 | Automatic Transmission Input Speed Sensor Low Signal

### Inside Rearview Mirror

#### Connector Part Information

- OEM: VHR-7N-NK
- Service: 15306078
- Description: 7-Way F VH Series (BK)

#### Terminal Part Information

- Terminal/Tray: SVH-21T-P1.1/20
- Core/Insulation Crimp: E/2
- Release Tool/Test Probe: 12094429/J-35616-18 (BK)

#### Inside Rearview Mirror

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 BK | 550 | Ground
3-5 | -- | -- | Not Used
6 | 0.5 GY | 157 | Courtesy Lamp Control
7 | 0.5 D-BU/WH | 149 | Courtesy Lamp Supply Voltage

### Instrument Panel Cluster (IPC)

#### Connector Part Information

- OEM: 15429805
- Service: 89047195
- Description: 16-Way F (NA)

#### Terminal Part Information

- Pins: 1-3, 10-12
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

- Pins: 5, 6, 8, 9, 13, 14, 15, 16
- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Instrument Panel Cluster (IPC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 PK/BK | 5982 | PRNDL B Signal
3 | 0.35 PU/WH | 5981 | PRNDL A Signal
4 | -- | -- | Not Used
5 | 0.35 D-GN/WH | 1358 | Driver Information Center Switch Signal
6 | 0.35 BN/WH | 419 | MIL Control
7 | -- | -- | Not Used
8 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
9 | 0.35 D-GN/BK | 5060 | Low Speed GMLAN Serial Data
10 | 0.35 L-GN/WH | 5984 | PRNDL D Signal
11 | 0.35 PK | 339 | Ignition 1 Voltage
12 | 0.35 OG/BK | 5983 | PRNDL C Signal
13 | 0.35 RD/WH | 1440 | Battery Positive Voltage
14 | 0.35 D-GN | 264 | Security Indicator Supply Voltage
15 | 0.5 BK | 1150 | Ground
16 | 0.35 BK | 550 | Ground

### Intake Air Pressure and Temperature Sensor

#### Connector Part Information

- OEM: 12162187
- Service: See Catalog
- Description: 4-Way F Metri-Pack 150.2 Series Sealed, Pull to Seat (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Intake Air Pressure and Temperature Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN | 407 | Low Reference
B | 0.5 L-BU | 7329 | Pre-Throttle Air Temp and Press (TMAP) Temperature Signal
C | 0.5 GY | 597 | 5-Volt Reference 1
D | 0.5 PU | 7330 | Pre-Throttle Air Temp and Press (TMAP) Air Pressure Signal

### Internal Mode Switch (IMS) Assembly, Wiring Harness Side (M82)

#### Connector Part Information

- OEM: 12146095
- Service: See Catalog
- Description: 6-Way F Metri-Pack 150.2 Series P2S (NA)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Internal Mode Switch (IMS) Assembly, Wiring Harness Side (M82)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | 1786 | Park/Neutral Signal
B | GY | 776 | Transmission Range Signal P
C | BK | 772 | Transmission Range Signal B
D | RD | 771 | Transmission Range Signal A
E | BU | 773 | Transmission Range Signal C
F | GN | 451 | Ground

### Knock Sensor (KS) - 1

#### Connector Part Information

- OEM: 12077900
- Service: See Catalog
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Knock Sensor (KS) - 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-BU | 496 | Knock Sensor 1 Signal
B | 0.5 GY | 1716 | Knock Sensor 1 Signal

### Knock Sensor (KS) - 2

#### Connector Part Information

- OEM: 12077900
- Service: See Catalog
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Knock Sensor (KS) - 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-BU | 1876 | Knock Sensor 2 Signal
B | 0.5 GY | 2303 | Knock Sensor 2 Signal

### License Lamp - Left

#### Connector Part Information

- OEM: 1452680-1
- Service: See Catalog
- Description: 2-Way F Micro-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### License Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 750 | Ground
2 | 0.5 BN | 9 | Tail/License Lamps Supply Voltage

### License Lamp - Right

#### Connector Part Information

- OEM: 1452680-1
- Service: See Catalog
- Description: 2-Way F Micro-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### License Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 750 | Ground
2 | 0.5 BN | 9 | Tail/License Lamps Supply Voltage

### Manifold Absolute Pressure (MAP) Sensor

#### Connector Part Information

- OEM: 184032-1
- Service: See Catalog
- Description: 3-Way F SSC Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Manifold Absolute Pressure (MAP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY | 597 | 5-Volt Reference 1
2 | 0.5 TN | 407 | Low Reference
3 | 0.5 L-GN | 432 | Manifold Absolute Pressure Sensor Signal

### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor

#### Connector Part Information

- OEM: 13519051
- Service: 88987186
- Description: 5-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 YE | 492 | Mass Air Flow Sensor Signal
B | 0.35 BK/WH | 451 | Ground
C | 0.35 PK/BK | 5291 | Ignition 1 Voltage
D | 0.35 TN | 2760 | Low Reference
E | 0.35 L-BU | 6289 | Induction Air Temperature Sensor Signal

### Mode Actuator

#### Connector Part Information

- OEM: 12064982
- Service: 12102633
- Description: 5-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Mode Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 1791 | Low Reference
2 | 0.35 L-GN/BK | 2276 | Defrost Door Position Signal
3 | 0.35 L-BU/BK | 1688 | 5-Volt Reference
4 | 0.35 TN | 2273 | Mode Door Control
5 | 0.35 L-GN | 2275 | Mode Door Position Signal

### Output Speed Sensor (OSS), Wiring Harness Side (M82)

#### Connector Part Information

- OEM: 12162201
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150.2 Series P2S (NA)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Output Speed Sensor (OSS), Wiring Harness Side (M82)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | OG | 400 | Vehicle Speed Sensor High Signal
B | WH | 401 | Vehicle Speed Sensor Low Signal

### Outside Air Temperature Sensor

#### Connector Part Information

- OEM: 12052642
- Service: 12101856
- Description: 2-Way F Metri-Pack 150 Series, Sealed (L-GN)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Outside Air Temperature Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-GN/WH | 636 | Ambient Air Temperature Signal
B | 0.5 YE | 61 | Low Reference

### Outside Rearview Mirror - Driver (D48)

#### Connector Part Information

- OEM: E-5965-003
- Service: 88988356
- Description: 3-Way M 1.5 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### Outside Rearview Mirror - Driver (D48)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 L-BU | 82 | Driver Mirror Motor Left Control
2 | 0.35 TN | 329 | Driver Mirror Motor Supply Voltage
3 | 0.35 YE | 88 | Driver Mirror Motor Up Control

### Outside Rearview Mirror - Passenger (D48)

#### Connector Part Information

- OEM: E-5965-003
- Service: 88988356
- Description: 3-Way M 1.5 Series, Sealed (BK)

#### Terminal Part Information

- Pins: 1
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit
- Pins: 2, 3
- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### Outside Rearview Mirror - Passenger (D48)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | 90 | Passenger Mirror Motor Left Control
2 | 0.35 TN/WH | 330 | Passenger Mirror Motor Supply Voltage
3 | 0.35 BN/WH | 1498 | Passenger Mirror Motor Up Control

### Outside Rearview Mirror Switch (D48)

#### Connector Part Information

- OEM: 12064769
- Service: 12101762
- Description: 10-Way F Metri-Pack 150 Series (NA)

#### Terminal Part Information

- Pins: B, C, D, E, F, G, H, J, K
- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Outside Rearview Mirror Switch (D48)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 BK | 550 | Ground
C | 0.35 TN | 329 | Driver Mirror Motor Supply Voltage
D | 0.35 GY | 90 | Passenger Mirror Motor Right Control
E | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
F | 0.35 BN/WH | 1489 | Passenger Mirror Motor Down Control
G | 0.35 RD/WH | 440 | Battery Positive Voltage
H | 0.35 TN/WH | 330 | Passenger Mirror Motor Supply Voltage
J | 0.35 L-BU | 82 | Driver Mirror Motor Right Control
K | 0.35 YE | 88 | Driver Mirror Motor Down Control

### Park Brake Switch

#### Connector Part Information

- OEM: 12047682
- Service: 12101850
- Description: 1-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Park Brake Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-BU | 1134 | Park Brake Switch Signal

### Park Lamp - Left Front

#### Connector Part Information

- OEM: E-3550-000
- Service: 89046838
- Description: 2-Way F 1.5 Series, Sealed (BK)

#### Terminal Part Information

- Terminal: Pin 1: 7116-4102-08/9Pin 2: 7116-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Park Lamp - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN | 9 | Park Lamp Supply Voltage
2 | 0.8 BK | 150 | Ground

### Park Lamp - Right Front

#### Connector Part Information

- OEM: E-3550-000
- Service: 89046838
- Description: 2-Way F 1.5 Series, Sealed (BK)

#### Terminal Part Information

- Terminal: Pin 1: 7116-4102-08/9Pin 2: 7116-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Park Lamp - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN | 9 | Park Lamp Supply Voltage
2 | 0.8 BK | 250 | Ground

### Pressure Control (PC) Solenoid Valve, Wiring Harness Side (M82)

#### Connector Part Information

- OEM: 12146094
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150.2 Series P2S (GY)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Pressure Control (PC) Solenoid Valve, Wiring Harness Side (M82)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | GN | 1228 | Pressure Control Solenoid Valve High Control
B | WH | 1229 | Pressure Control Solenoid Valve Low Control

### Radio - X1

#### Connector Part Information

- OEM: 7283-9076-30
- Service: See Catalog
- Description: 16-Way F Kaizen 0.64 Series (BK)

#### Terminal Part Information

- Pins: 3, 4, 5, 6, 7, 14, 15
- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Radio - X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.35 PK | 314 | Radio On Signal
4 | 0.5 TN | 1946 | Right Rear Low Level Audio Signal (-)
5 | 0.5 D-BU | 546 | Right Rear Low Level Audio Signal (+)
6 | 0.5 BN | 1999 | Left Rear Low Level Audio Signal (-)
7 | 0.5 BN/WH | 599 | Left Rear Low Level Audio Signal (+)
8-13 | -- | -- | Not Used
14 | 0.35 WH/BK | 644 | 10-Volt Reference (UK3)
15 | 0.35 L-GN | 1011 | Remote Radio Control Signal
16 | -- | -- | Not Used

### Radio - X2

#### Connector Part Information

- OEM: 7283-4490-30
- Service: See Catalog
- Description: 14-Way F (BK)

#### Terminal Part Information

- Pins: 1, 8
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: 4, 5, 6, 7, 9, 11
- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Radio - X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 RD/WH | 1140 | Battery Positive Voltage
2-3 | -- | -- | Not Used
4 | 0.5 L-GN | 1948 | Right Front Low Level Audio Signal (-)
5 | 0.5 L-GN/WH | 512 | Right Front Low Level Audio Signal (+)
6 | 0.5 D-GN | 1947 | Left Front Low Level Audio Signal (-)
7 | 0.5 TN | 511 | Left Front Low Level Audio Signal (+)
8 | 0.8 BK/WH | 551 | Ground
9 | 0.35 D-GN/WH | 5060 | Low Speed GMLAN Serial Data
10 | -- | -- | Not Used
11 | 0.35 D-BU | 1796 | Steering Column Controls Signal
12-14 | -- | -- | Not Used

### Rear Compartment Courtesy Lamp

#### Connector Part Information

- OEM: 12047662
- Service: 12085535
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Rear Compartment Courtesy Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 750 | Ground
B | 0.5 OG/BK | 737 | Rear Compartment Lamp Control

### Rear Compartment Lid Ajar Switch

#### Connector Part Information

- OEM: 12129082
- Service: 15305896
- Description: 2-Way F Metri-Pack 280 Series, Flexlock (M-GY)

#### Terminal Part Information

- Pins: A, B
- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: Pins: E/C
- Core/Insulation Crimp: Pins: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Rear Compartment Lid Ajar Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 OG/BK | 744 | Rear Compartment Lid Ajar Switch Signal
B | 0.5 BK | 850 | Ground

### Rear Compartment Lid Latch Release Actuator

#### Connector Part Information

- OEM: 12129081
- Service: 12129081
- Description: 2-Way F Metri-Pack 280 Series, Flexlock (BK)

#### Terminal Part Information

- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Rear Compartment Lid Latch Release Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 TN/WH | 56 | Rear Compartment Lid Release Motor Supply Voltage
B | 1.0 BK | 850 | Ground

### Rear Compartment Lid Release Switch

#### Connector Part Information

- OEM: 12044785
- Service: 12102900
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Pins: A, C
- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A

#### Rear Compartment Lid Release Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK/WH | 651 | Ground
B | -- | -- | Not Used
C | 0.35 TN | 1576 | Rear Compartment Lid Release Actuator
D | -- | -- | Not Used

### Rear Window Defogger Grid X1

#### Connector Part Information

- OEM: 12004267
- Service: 08911256
- Description: 1-Way F 56 Series Lock Type (BK)

#### Terminal Part Information

- Terminal/Tray: 12124515/1
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Rear Window Defogger Grid X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 PU | 293 | Rear Defog Element Supply Voltage

### Rear Window Defogger Grid X2

#### Connector Part Information

- OEM: 12004267
- Service: 08911256
- Description: 1-Way F 56 Series Lock Type (BK)

#### Terminal Part Information

- Terminal/Tray: 12124515/1
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Rear Window Defogger Grid X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 BK | 850 | Ground

### Recirculation Actuator

#### Connector Part Information

- OEM: 12064982
- Service: 12102633
- Description: 5-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Pins: 4, 5
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Recirculation Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-3 | -- | -- | Not Used
4 | 0.35 L-BU | 1614 | Recirculation Door Control
5 | 0.35 L-GN | 2274 | Recirculation Door Control Circuit

### Remote Control Door Lock Receiver (RCDLR) (AU3/AU0)

#### Connector Part Information

- OEM: HCMPB-04-K
- Service: See Catalog
- Description: 4-Way F HCM Series (BK)

#### Terminal Part Information

- Pins: 1, 2, 4
- Terminal/Tray: 12146447/3
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### Remote Control Door Lock Receiver (RCDLR) (AU3/AU0)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK/WH | 851 | Ground
2 | 0.35 D-GN/RD | 5060 | Low Speed GMLAN Serial Data
3 | -- | -- | Not Used
4 | 0.35 RD/WH | 1340 | Battery Positive Voltage

### Seat Adjuster Switch - Driver (AF2)

#### Connector Part Information

- OEM: 12052854
- Service: 88953358
- Description: 7-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12015858/4
- Core/Insulation Crimp: F/G
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Seat Adjuster Switch - Driver (AF2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 2.0 BK | 550 | Ground
B | 2.0 D-BU | 287 | Driver Seat Front Vertical Motor Down Control
C | 2.0 D-GN | 286 | Driver Seat Front Vertical Motor Up Control
D-E | -- | -- | Not Used
F | 2.0 RD/BK | 642 | Battery Positive Voltage
G | 2.0 BK | 550 | Ground

### Seat Belt Pretensioner - Driver

#### Connector Part Information

- OEM: 15380395
- Service: See Catalog
- Description: 2-Way F Squib Unsealed (YE)

#### Terminal Part Information

- Terminal/Tray: Serviced with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: N/A

#### Seat Belt Pretensioner - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 OG/BK | 2119 | Seat Belt Pretensioner - Left - Low Control
2 | 0.5 TN/WH | 2118 | Seat Belt Pretensioner - Left - High Control

### Seat Belt Pretensioner - Passenger

#### Connector Part Information

- OEM: 15380395
- Service: See Catalog
- Description: 2-Way F Squib Unsealed (YE)

#### Terminal Part Information

- Terminal/Tray: Serviced with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: N/A

#### Seat Belt Pretensioner - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 OG | 2117 | Seat Belt Pretensioner - Right - Low Control
2 | 0.5 L-GN | 2116 | Seat Belt Pretensioner - Right - High Control

### Seat Belt Switch - Driver

#### Connector Part Information

- OEM: 15332132
- Service: 88953364
- Description: 3-Way F GT 150 Series (BK)

#### Terminal Part Information

- Pins: A, C
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Seat Belt Switch - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 TN/WH | 238 | Seat Belt Switch - Left
B | -- | -- | Not Used
C | 0.35 PK | 5057 | Low Reference

### Seat Belt Switch - Passenger

#### Connector Part Information

- OEM: 15332133
- Service: 88987881
- Description: 3-Way F GT 150 Series (BK)

#### Terminal Part Information

- Pins: A, C
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Switch - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 OG | 1362 | Seat Belt Switch - Right - Signal
B | -- | -- | Not Used
C | 0.35 PK | 5057 | Low Reference

### Seat Front Vertical Motor - Driver (AF2)

#### Connector Part Information

- OEM: 1379217-3
- Service: Not Serviced
- Description: 5-Way F MQS/MPQ Mixed Series (BK)

#### Terminal Part Information

- Terminal/Tray: 968075-5/17
- Core/Insulation Crimp: 2/4
- Release Tool/Test Probe: 12031876-1/J-35616-4A (PU)

#### Seat Front Vertical Motor - Driver (AF2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.0 D-GN | 286 | Driver Seat Front Vertical Motor Up Control
2-4 | -- | -- | Not Used
5 | 2.0 D-BU | 287 | Driver Seat Front Vertical Motor Down Control

### Speaker - Left Front

#### Connector Part Information

- OEM: 12064869
- Service: 12117323
- Description: 2-Way F Metri-Pack 150 Series (BU)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 GY | 118 | Left Front Speaker Output (-)
B | 0.8 TN | 201 | Left Front Speaker Output (+)

### Speaker - Left Rear

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 YE | 116 | Left Rear Speaker Output (-)
B | 0.8 BN | 199 | Left Rear Speaker Output (+)

### Speaker - Left Tweeter

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Left Tweeter

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 TN | 1856 | Left Front Tweeter Speaker Output (+)
B | 0.8 YE | 1956 | Left Front Tweeter Speaker Output (-)

### Speaker - Right Front

#### Connector Part Information

- OEM: 12064869
- Service: 12117323
- Description: 2-Way F Metri-Pack 150 Series (BU)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 D-GN | 117 | Right Front Speaker Output (-)
B | 0.8 L-GN | 200 | Right Front Speaker Output (+)

### Speaker - Right Rear

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 L-BU | 115 | Right Rear Speaker Output (-)
B | 0.8 D-BU | 46 | Right Rear Speaker Output (+)

### Speaker - Right Tweeter

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Right Tweeter

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 L-GN | 1852 | Right Front Tweeter Speaker Output (+)
B | 0.8 PU | 1952 | Right Front Tweeter Speaker Output (-)

### Speaker - Subwoofer

#### Connector Part Information

- OEM: 12064760
- Service: 12085208
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Subwoofer

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 L-BU/BK | 315 | Right Subwoofer Speaker Output (-)
B | 0.8 D-GN | 1795 | Right Subwoofer Speaker Output (+)
C | 0.8 L-GN/BK | 1794 | Left/Rear Subwoofer Speaker Output (-)
D | 0.8 D-BU/WH | 346 | Left/Rear Subwoofer Speaker Output (+)

### Starter Motor X1

#### Connector Part Information

- OEM: 12089916
- Service: See Catalog
- Description: 1-Way F Metri-Pack 280 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Starter Motor X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 2.0 PU | 6 | Starter Solenoid Crank Voltage

### Starter Motor X2

#### Terminal Part Information

- Terminal: 12103502
- Description: Ring Terminal

#### Starter Motor X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 8 BK | 2 | Starter Solenoid Crank Voltage

### Steering Angle Sensor

#### Connector Part Information

- OEM: 1488752-1
- Service: See Catalog
- Description: 6-Way F 064 GET Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Steering Angle Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 2087 | 5-Volt Reference
2 | 0.5 PK/BK | 6434 | Can Bus High Serial Data
3 | 0.5 PK/BK | 6434 | Can Bus High Serial Data
4 | 0.5 GY/BK | 6435 | Can Bus Low Serial Data
5 | 0.5 GY/BK | 6435 | Can Bus Low Serial Data
6 | 0.5 L-BU | 2088 | Low Reference

### Steering Wheel Control Switch - Left (K34)

#### Connector Part Information

- OEM: 50-57-9407
- Service: 88988695
- Description: 7-Way F SL Series Unsealed (BK)

#### Terminal Part Information

- Pins: 3, 4, 5, 6, 7
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Steering Wheel Control Switch - Left (K34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN/WH | 1358 | Driver Information Center Switch Signal
2 | -- | -- | Not Used
3 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
4 | 0.35 PK | 1539 | Ignition 1 Voltage
5 | 0.35 GY | 1884 | Cruise Control Switch Signal
6 | -- | -- | Not Used
7 | 0.35 BK | 1150 | Ground

### Steering Wheel Control Switch - Right (UK3)

#### Connector Part Information

- OEM: 50-57-9404
- Service: 88987918
- Description: 4-Way F SL Series, Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Steering Wheel Control Switch - Right (UK3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK | 1150 | Ground
2 | 0.35 WH/BK | 644 | 10-Volt Reference
3 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
4 | 0.35 D-BU | 1796 | Steering Column Controls Signal

### Tail/Stop Lamp - Left

#### Connector Part Information

- OEM: 7822-2945-A22
- Service: See Catalog
- Description: 3-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Tail/Stop Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 D-GN/WH | 20 | Stop Lamp Supply Voltage
B | 0.8 RD | 809 | Tail/License Lamps Supply Voltage
G | 0.8 BK | 1050 | Ground

### Tail/Stop Lamp - Right

#### Connector Part Information

- OEM: 7822-2945-A22
- Service: See Catalog
- Description: 3-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Tail/Stop Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 L-BU | 20 | Stop Lamp Supply Voltage
B | 0.8 WH | 609 | Tail/License Lamps Supply Voltage
G | 0.8 BK | 750 | Ground

### Theft Deterrent Module (TDM)

#### Connector Part Information

- OEM: 50-57-9705
- Service: 88988353
- Description: 5-Way F SL Series Unsealed (BK)

#### Terminal Part Information

- Pins: 1-4
- Terminal/Tray: 16-02-1110/20
- Core/Insulation Crimp: H/H
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

#### Theft Deterrent Module (TDM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD/WH | 1540 | Battery Positive Voltage
2 | 0.35 BN | 4 | Accessory Voltage
3 | 0.35 BK/WH | 651 | Ground
4 | 0.35 L-GN | 5060 | Low Speed GMLAN Serial Data
5 | -- | -- | Not Used

### Throttle Body

#### Connector Part Information

- OEM: 15355297
- Service: See Catalog
- Description: 6-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Throttle Body

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BN | 582 | Throttle Actuator Control Motor Control - 2
B | 0.8 YE | 581 | Throttle Actuator Control Motor Control - 1
C | 0.5 TN | 2752 | Low Reference
D | 0.5 D-GN | 485 | Throttle Position Sensor 1 Signal
E | 0.5 GY | 2701 | 5-Volt Reference 3
F | 0.5 PU | 486 | Throttle Position Sensor 2 Signal

### Torque Converter Clutch Pulse Width Modulated (TCC PWM) Solenoid Valve, Wiring Harness Side (M82)

#### Connector Part Information

- OEM: 12162202
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150.2 Series P2S (BU)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Torque Converter Clutch Pulse Width Modulated (TCC PWM) Solenoid Valve, Wiring Harness Side (M82)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | YE | 418 | Torque Converter Clutch Pulsewidth Modulated Solenoid Valve Control
B | WH | 1525 | Clutch Pressure Control Solenoid Valve 1 High Control

### Traction Control Switch (TCS)

#### Connector Part Information

- OEM: 12047785
- Service: See Catalog
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Traction Control Switch (TCS)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK | 550 | Ground
B | -- | -- | Not Used
C | 0.35 L-BU | 1788 | Traction Control Switch Signal
D | 0.35 GY | 8 | Instrument Panel Lamp Supply

### Transmission Control Module (TCM) (M82)

#### Connector Part Information

- OEM: 1-1393455-2
- Service: 15434189
- Description: 42-Way F Sealed Module 1 Socket Housing (BK)

#### Terminal Part Information

- Terminal/Tray: 2-1411578-2/Yazaki 15
- Core/Insulation Crimp: 7/7
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Transmission Control Module (TCM) (M82)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
F1 | 0.35 YE | 400 | Vehicle Speed Sensor Signal
F2 | 0.35 PU | 401 | Low Reference
F3 | 0.35 OG/BK | 1228 | Pressure Control Solenoid Valve High Control
F4 | 0.35 BN | 418 | Torque Converter Clutch Pulse Width Modulated Solenoid Valve Control
F5 | 0.35 BN | 4 | Accessory Voltage
F6 | 1.0 BK/WH | 451 | Ground
F7 | -- | -- | Not Used
F8 | 0.8 OG | 1525 | Clutch Pressure Control Solenoid Valve 1 High Control
F9 | 0.8 PK | 1039 | Ignition 1 Voltage
F10 | 0.35 OG/BK | 1230 | Automatic Transmission Input Speed Sensor High Signal
F11 | 0.35 D-BU/WH | 1231 | Automatic Transmission Input Speed Sensor Low Signal
F12-F14 | -- | -- | Not Used
F15 | 0.35 YE/BK | 1227 | Transmission Fluid Temperature Sensor Signal
F16-F17 | -- | -- | Not Used
F18 | 0.35 YE/BK | 1223 | 2-3 Shift Solenoid Valve Control
F19 | 0.35 PU | 898 | 4-5 Shift Solenoid Valve Control
F20 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus (+)
F21 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-)
F22-F23 | -- | -- | Not Used
F24 | 0.35 YE | 772 | Transmission Range Switch Signal B
F25 | 0.35 GY | 773 | Transmission Range Switch Signal C
F26 | 0.35 TN | 2762 | Low Reference
F27 | 0.5 RD/WH | 840 | Battery Positive Voltage
F28 | -- | -- | Not Used
F29 | 0.35 L-BU/WH | 1229 | Pressure Control Solenoid Valve Low Control
F30 | 0.35 L-GN | 1222 | 1-2 Shift Solenoid Valve Control
F31 | -- | -- | Not Used
F32 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus (+)
F33 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-)
F34-F35 | -- | -- | Not Used
F36 | 0.35 TN/WH | 771 | Transmission Range Switch Signal A
F37 | 0.35 WH | 776 | Transmission Range Switch Signal P
F38 | 0.35 L-BU | 20 | Stop Lamp Supply Voltage
F39-F42 | -- | -- | Not Used

### Transmission Manual Shift Shaft Switch, Wiring Harness Side (M82)

#### Connector Part Information

- OEM: 12146095
- Service: See Catalog
- Description: 6-Way F Metri-Pack 150.2 Series P2S (NA)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Transmission Manual Shift Shaft Switch, Wiring Harness Side (M82)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | 1786 | Park/Neutral Signal
B | GY | 776 | Transmission Range Signal P
C | BK | 772 | Transmission Range Signal B
D | RD | 771 | Transmission Range Signal A
E | BU | 773 | Transmission Range Signal C
F | GN | 451 | Ground

### Turbocharger Bypass Valve Solenoid

#### Connector Part Information

- OEM: 1 928 402 571
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Turbocharger Bypass Valve Control Solenoid

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 6391 | Turbocharger Bypass Valve Control
2 | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply (4)

### Turbocharger Wastegate Solenoid

#### Connector Part Information

- OEM: 1 928 402 571
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Turbocharger Wastegate Solenoid

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE | 258 | Turbocharger Wastegate Solenoid Control
2 | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply (4)

### Turn Signal Lamp - Left Front

#### Connector Part Information

- OEM: 15354865
- Service: See Catalog
- Description: 3-Way F W3 Socket (WH)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Turn Signal Lamp - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-BU | 14 | Left Turn Signal Lamps Supply Voltage
B | 0.5 BN | 9 | Park Lamp Supply Voltage
G | 0.5 BK | 150 | Ground

### Turn Signal Lamp - Left Rear

#### Connector Part Information

- OEM: 7822-2945-A22
- Service: See Catalog
- Description: 3-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Turn Signal Lamp - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 D-GN | 618 | Left Rear Stop/Turn Lamp Supply Voltage
B | -- | -- | Not Used
G | 0.8 BK | 1050 | Ground
0.8 BK | 1050 | Ground

### Turn Signal Lamp - Right Front

#### Connector Part Information

- OEM: 15354865
- Service: See Catalog
- Description: 3-Way F W3 Socket (WH)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Turn Signal Lamp - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-BU | 15 | Right Turn Signal Lamps Supply Voltage
B | 0.5 BN | 9 | Park Lamp Supply Voltage
G | 0.5 BK | 250 | Ground

### Turn Signal Lamp - Right Rear

#### Connector Part Information

- OEM: 7822-2945-A22
- Service: See Catalog
- Description: 3-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Turn Signal Lamp - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-GN | 619 | Right Rear Stop/Turn Lamp Supply Voltage
B | -- | -- | Not Used
G | 0.5 BK | 750 | Ground
0.5 BK | 750 | Ground

### Turn Signal Repeater Lamp - Left

#### Connector Part Information

- OEM: 15326806
- Service: 15306166
- Description: 2-Way M 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Turn Signal Repeater Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-BU | 14 | Left Turn Signal Lamps Supply Voltage
B | 0.5 BK | 150 | Ground

### Turn Signal Repeater Lamp - Right

#### Connector Part Information

- OEM: 15326806
- Service: 15306166
- Description: 2-Way M 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Turn Signal Repeater Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-BU | 15 | Right Turn Signal Lamps Supply Voltage
B | 0.5 BK | 250 | Ground

### Turn Signal/Multifunction Switch X1

#### Connector Part Information

- OEM: NACP-08-S
- Service: See Catalog
- Description: 8-Way F Misc (NA)

#### Terminal Part Information

- Pins: 1, 2, 3, 4
- Terminal/Tray: SNAC-A03T-M040/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-12 (BU)

#### Turn Signal/Multifunction Switch X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK/WH | 651 | Ground
2 | 0.35 WH | 103 | Headlamp Switch Headlamps On Signal
3 | 0.35 BN/WH | 301 | Park Lamp Switch On Signal
4 | 0.35 PU/WH | 549 | Headlamp Switch Headlamps Off Signal
5-8 | -- | -- | Not Used

### Turn Signal/Multifunction Switch X2

#### Connector Part Information

- OEM: 15393435
- Service: 88986438
- Description: 10-Way F Micro (BK)

#### Terminal Part Information

- Pins: B, C, D, E, F, G, H
- Terminal/Tray: 12177007/19
- Core/Insulation Crimp: E/2
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Turn Signal/Multifunction Switch X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 BK/WH | 651 | Ground
C | 0.35 BN | 1356 | Flash To Pass Switch Signal
D | 0.35 PU | 524 | Headlamp Dimmer Switch High Beam Signal
E | -- | -- | Not Used
F | 0.35 PK/WH | 1970 | Headlamp Low Beam Relay Control
G | 0.35 YE/BK | 1418 | Left Rear Turn Signal Switch Signal
H | 0.35 D-GN/WH | 1419 | Right Rear Turn Signal Switch Signal
J-K | -- | -- | Not Used

### Wheel Speed Sensor (WSS) - Left Front

#### Connector Part Information

- OEM: 1-928-403-698
- Service: See Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Wheel Speed Sensor (WSS) - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 L-BU | 830 | Left Front Wheel Speed Sensor Signal
2 | 0.8 YE | 873 | Low Reference

### Wheel Speed Sensor (WSS) - Left Rear

#### Connector Part Information

- OEM: 1-928-403-698
- Service: See Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Wheel Speed Sensor (WSS) - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 TN | 884 | Left Rear Wheel Speed Sensor Signal
2 | 0.8 OG | 885 | Low Reference

### Wheel Speed Sensor (WSS) - Right Front

#### Connector Part Information

- OEM: 1-928-403-698
- Service: See Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Wheel Speed Sensor (WSS) - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 D-GN | 872 | Right Front Wheel Speed Sensor Signal
2 | 0.8 TN | 833 | Low Reference

### Wheel Speed Sensor (WSS) - Right Rear

#### Connector Part Information

- OEM: 1-928-403-698
- Service: See Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Wheel Speed Sensor (WSS) - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 BN | 882 | Right Rear Wheel Speed Sensor Signal
2 | 0.8 WH | 883 | Low Reference

### Window Motor - Driver (A31)

#### Connector Part Information

- OEM: 12129487
- Service: 88988609
- Description: 2-Way F Metri-Pack Series, Flexlock, Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12110845/4
- Core/Insulation Crimp: F/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Motor - Driver (A31)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 3.0 BN | 165 | Power Window Motor Left Front Down Control
B | 3.0 D-BU | 164 | Power Window Motor Left Front Up Control

### Window Motor - Passenger (A31)

#### Connector Part Information

- OEM: 12129487
- Service: 88988609
- Description: 2-Way F Metri-Pack 280 Series, FlexLock, Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12110845/4
- Core/Insulation Crimp: F/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Motor - Passenger (A31)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 3.0 BN | 667 | Power Window Motor Right Front Down Control
B | 3.0 D-BU | 666 | Power Window Motor Right Front Up Control

### Window Switch - Driver (A31)

#### Connector Part Information

- OEM: 15449340
- Service: 15306174
- Description: 8-Way F GT 280 (BK)

#### Terminal Part Information

- Pins: B
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)
- Pins: A, C, D, F, G, H
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: Pins A, C, D, G, H F/D
- Core/Insulation Crimp: Pins F 4/4
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Switch - Driver (A31)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 3.0 L-BU | 166 | Power Window Master Switch Right Front Up Signal
B | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
C | 3.0 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
D | 3.0 TN | 167 | Power Window Master Switch Right Front Down Signal
E | -- | -- | Not Used
F | 2.0 BK | 550 | Ground
G | 3.0 D-BU | 164 | Power Window Motor Left Front Up Control
H | 3.0 BN | 165 | Power Window Motor Left Front Down Control

### Window Switch - Passenger (A31)

#### Connector Part Information

- OEM: 12192825
- Service: 15306048
- Description: 8-Way F Metri-Pack 280 Series (BN)

#### Terminal Part Information

- Pins: H
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit
- Pins: A, D, F, G
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: F/D
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)
- Pins: B, C
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Switch - Passenger (A31)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 3.0 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
B | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
C | 0.35 BK | 550 | Ground
D | 3.0 TN | 167 | Power Window Master Switch Right Front Down Signal
E | -- | -- | Not Used
F | 3.0 BN | 667 | Power Window Motor Right Front Down Control
G | 3.0 D-BU | 666 | Power Window Motor Right Front Up Control
H | 3.0 L-BU | 166 | Power Window Master Switch Right Front Up Signal

### Windshield Washer Fluid Pump

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Windshield Washer Fluid Pump

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 OG | 228 | Windshield Washer Pump Control
B | 0.5 BK | 250 | Ground

### Windshield Wiper Motor

#### Connector Part Information

- OEM: 7283-7050-30
- Service: 89046627
- Description: 5-Way F 090 II Class III Series, Sealed (BK)

#### Terminal Part Information

- Pins: 1, 4, 5
- Terminal/Tray: 7116-4026/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

- Pins: 2
- Terminal/Tray: 7116-4025/11
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

#### Windshield Wiper Motor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.0 BK | 250 | Ground
2 | 0.35 YE | 196 | Windshield Wiper Motor Park Switch Signal
3 | -- | -- | Not Used
4 | 1.0 PU | 92 | Windshield Wiper Motor High Speed Control
5 | 1.0 D-GN | 95 | Windshield Washer Switch Signal

### Windshield Wiper/Washer Switch

#### Connector Part Information

- OEM: 12059800
- Service: 15306169
- Description: 5-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Pins: B, C, D, E
- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Windshield Wiper/Washer Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 OG | 228 | Windshield Washer Pump Control
C | 0.35 L-GN | 1715 | Windshield Wiper Switch High Signal
D | 0.35 PK | 439 | Ignition 1 Voltage
E | 0.35 GY | 112 | Windshield Wiper Switch Signal

### Yaw and Lateral Accelerometer Sensor

#### Connector Part Information

- OEM: 2-967616-1
- Service: See Catalog
- Description: 6-Way F MQS Socket Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Yaw and Lateral Accelerometer Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY/BK | 6435 | Can Bus Low Serial Data
2 | 0.5 PK/BK | 6434 | Can Bus High Serial Data
3 | 0.5 D-GN | 2087 | 5-Volt Reference
4 | -- | -- | Unavailable
5 | 0.5 L-BU | 2088 | Low Reference
6 | -- | -- | Unavailable