For 1990-2009 cars

Table 1: | Supplemental Inflatable Restraint Scan Tool Data Parameters
Table 2: | Supplemental Inflatable Restraint Scan Tool Output Controls

#### Supplemental Inflatable Restraint Scan Tool Data Parameters

Parameter | System State | Expected Value | Description
--- | --- | --- | ---
Operating Conditions: Ignition ON
Battery Voltage Signal | -- | Varies | This displays Volts. This is the current battery voltage signal.
Driver Frontal Stage 1 Loop | -- | Present | The scan tool displays Present or Not Present. This is the state of the driver frontal stage 1 loop.
Driver Frontal Stage 2 Loop | -- | Present | The scan tool displays Present or Not Present. This is the state of the driver frontal stage 2 loop.
Driver Pretensioner Loop | -- | Present | The scan tool displays Present or Not Present. This is the state of the driver pretensioner loop.
Driver Roof Rail | -- | Present | The scan tool displays Present or Not Present. This is the state of the driver roof rail.
Driver Seat Belt Switch | -- | Present | The scan tool displays Present or Not Present. This is the state of the driver seat belt switch.
Driver Seat Belt Switch | -- | Unbuckled | The scan tool displays Buckled or Unbuckled. This is the state of the driver seat belt switch.
Driver Seat Position Sensor | -- | Present | The scan tool displays Present or Not Present. This is the state of the driver seat position sensor.
Driver Side Impact Sensor | -- | Present | The scan tool displays Present or Not Present. This is the state of the driver impact sensor.
Front End Sensor 1 | -- | Present | This displays Present or Not Present. This is the state of the front end sensor 1.
Front End Sensor 2 | -- | Present | This displays Present or Not Present. This is the state of the front end sensor 2.
Passenger Presence System | -- | Present | This displays Present or Not Present. Present is displayed if the passenger presence system is available.
Passenger Pretensioner Loop | -- | Present | The scan tool displays Present or Not Present. This is the state of the passenger pretensioner loop.
Psgr. Frontal Stage 1 Loop | -- | Present | This displays Present or Not Present. This is the state of the passenger frontal stage 1 loop.
Psgr. Frontal Stage 2 Loop | -- | Present | This displays Present or Not Present. This is the state of the passenger frontal stage 2 loop.
Psgr. Roof Rail | -- | Present | This displays Present or Not Present. This is the state of the passenger roof rail.
Psgr. Seat Position Sensor | -- | Present | This displays Present or Not Present. This is the state of the passenger seat position sensor.
Psgr. Side Impact Sensor | -- | Present | This displays Present or Not Present. This is the state of the passenger impact sensor.
SIR Warning Indicator | -- | Off | The scan tool displays On or Off. This is the state of the SIR warning indicator.

#### Supplemental Inflatable Restraint Scan Tool Output Controls

Output Control | Description
--- | ---
Setup New SDM | This output control is used to setup a new inflatable restraint sensing and diagnostic module (SDM).
Setup SDM Part Number in IPM | This output control is used to setup the SDM part number into the instrument panel module (IPM).