For 1990-2009 cars

The following table provides the description of the Regular Production Option (RPO) codes that are available on the vehicle. The vehicle's RPO list is printed on the Service Parts Identification Label.

RPO | Description
--- | ---
AF2 | Adjuster - Seat, Power, 2 Way, Vertical, Driver
AL0 | Sensor Indicator - Inflatable Restraint, Front Passenger/Child Presence Detector
AU3 | Lock Control - Side Door, Electric
AU8 | Lock Control, Entry - Remote Entry, Specific Frequency
AZ5 | Covering Headliner - Convertible Top Trim
A31 | Window - Power Operated, All Doors
A50 | Seat - Front Bucket
B70 | Plate - Door Sill Cover
CW1 | Country - South Korea
C60 | HVAC System - Air Conditioner Front, Manual Controls
DRX | Model Conversion - Daewoo
EXP | Export
FE3 | Suspension System - Sport
FE9 | Certification - Emission, Federal
GT4 | Axle Rear - 3.73 Ratio
G80 | Axle Positraction - Limited Slip
IP2 | Trim - Interior Trim (P2)
JF5 | Pedals - Sporty, Alloy
KG7 | Generator - 125 Amp
K34 | Cruise Control - Automatic, Electronic
LNF | Engine - Gas, 4 Cylinder, 2.0L, DI, Aluminum, DOHC, Turbo, GM
NT7 | Emission System - Federal, Tier 2
N34 | Steering Wheel - Leather, 3 Spokes
QSL | Tire All - P245/45R18-96W BW TL HW4
QF8 | Wheel - 18 X 8, Aluminum, Polished
T62 | Lamp System Daytime Running - Delete
T96 | Lamp - Fog, Front
T98 | Stamping - Vehicle Identification Number
UK3 | Control - Steering Wheel, Accessory
US6 | Antenna - Fixed, Painted, Radio
US9 | Radio - AM/FM Stereo, Seek/Scan, RDS, Multiple Compact Disc, Auto Tone Control, Clock, ETR, MP3
U19 | Speedometer - Instrument, Kilometer and Miles, Kilometer Odometer
U68 | Display - Driver Information Center
VK3 | License Plate Front - Front Mounting Package
VP6 | Noise Control
V78 | Vehicle Statement - Delete
WIL | Plant Code - Wilmington, Delaware, USA