For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel lower trim panel. Refer to Instrument Panel Lower Trim Panel Replacement .
2. Remove the shift indicator. Refer to Transmission Control Lever Knob Replacement .

1 | Front Floor Console Cover Assembly

#### Procedure

Use a flat-bladed plastic trim tool in order to release the retainer tabs securing the cover to the console.

2 | Retainer Clips (Qty: 8)