For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Compressor and Condenser Hose Assembly Bolt | 22 N·m | 16 lb ft
A/C Compressor and Condenser Hose Assembly Nut | 9 N·m | 80 lb in
A/C Compressor Bolt | 22 N·m | 16 lb ft
A/C Compressor Tube Assembly Nut | 16 N·m | 12 lb ft
A/C Condenser Bolt | 9 N·m | 80 lb in
A/C Condenser Tube Assembly Nut | 9 N·m | 80 lb in
A/C Condenser Tube Nut | 9 N·m | 80 lb in
A/C Evaporator Hose Assembly Clip Nut | 9 N·m | 80 lb in
A/C Evaporator Hose Assembly Nut | 16 N·m | 12 lb ft
A/C Refrigerant Pressure Sensor | 5 N·m | 44 lb in
Air Inlet Housing Screw | 1.5 N·m | 13 lb in
Air Inlet Housing Nut | 9 N·m | 80 lb in
Air Distribution Case Screw | 1.5 N·m | 13 lb in
Air Outlet Duct Screw | 1.5 N·m | 13 lb in
Blower Motor Resistor Screw | 1.5 N·m | 13 lb in
Blower Motor Screw | 1.5 N·m | 13 lb in
Distributor Air Bolt | 2.5 N·m | 22 lb in
Distributor Air Nut | 2.5 N·m | 22 lb in
Evaporator Case Assembly Screw | 1.5 N·m | 13 lb in
Heater Core Cover Screw | 1.5 N·m | 13 lb in
HVAC Module Assembly Nut | 9 N·m | 80 lb in
Mode Actuator Screw | 1.5 N·m | 13 lb in
Radiator Assembly Bolt | 25 N·m | 18 lb ft
Rear Air Outlet Duct Screw | 1.5 N·m | 13 lb in
Receiver Dehydrator Assembly Bolt | 6 N·m | 53 lb in
Receiver Dehydrator Screw | 1.5 N·m | 13 lb in
Thermal Expansion Valve Bolt | 16 N·m | 12 lb ft