For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Drain the cooling system. Refer to Cooling System Draining and Filling .

1 | Radiator Surge Tank Hose Assembly - Inlet Tip Note routing of the radiator surge tank inlet hose to ensure proper insulation.

#### Procedure

Using J 38185 position radiator surge tank inlet hose clamps aside and remove hose from the fittings.

#### Special Tools

J 38185 Hose Clamp Pliers