For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Door Check Link Bolt | 10 N·m | 89 lb in
Door Check Link Nuts | 10 N·m | 89 lb in
Door Hinge Lower Bolts | 35 N·m | 26 lb ft
Door Lower Hinge to Body Bolts | 25 N·m | 18 lb ft
Door Upper Hinge Bolts | 35 N·m | 26 lb ft
Front Fender Bolts | 10 N·m | 89 lb in
Fuel Door Pocket Screws | 10 N·m | 89 lb in
Hood Hinge Nuts | 25 N·m | 18 lb ft
Hood Latch Bolts | 25 N·m | 19 ft in
Hood Latch Release Cable Handle Screws | 10 N·m | 89 lb in
Hood Release Handle to Knee Bolster Screws | 2 N·m | 18 lb in
Rear Compartment Lid Hinge Bolts | 25 N·m | 19 ft in