For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the rear stowage compartment lid to gain access to the striker.

1 | Striker Rear Folding Top Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tip Remove the striker plate screws and buttress if broken. Tighten
2 N·m (18 lb in)

2 | Striker Rear Top Folding Bolt Tighten 11 N·m (97 lb in)
3 | Rear Folding Top Striker