For 1990-2009 cars

#### Automatic Transmission (5L40E)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | L-GN/BK | 0.5 | VSS High Signal
2 | OG/BK | 0.5 | Park/Neutral Signal
3 | PU/WH | 0.5 | VSS Low Signal
4 | BK | 0.5 | Ground
5 | WH | 0.5 | Shift Solenoid C Valve Control
6 | BN/WH | 0.5 | Low Reference
7 | YE | 0.5 | Transmission Range Switch Signal B
8 | L-BU/WH | 0.5 | PC Solenoid Valve Low Control
9 | YE/BK | 0.5 | Shift Solenoid B Valve Control
10 | YE/BK | 0.5 | TFT Sensor Signal
11 | WH | 0.5 | Transmission Range Switch Signal P
12 | -- | -- | Not Used
13 | OG/BK | 0.5 | PC Solenoid Valve High Control
14 | L-GN | 0.5 | Shift Solenoid A Valve Control
15 | L-BU | 0.5 | Transmission Turbine Speed Switch Low Reference
16 | BN/YE | 0.5 | Transmission Range Switch Signal A
17 | OG | 0.5 | Clutch Pressure Control Solenoid Valve 1 High Control
18 | OG | 0.5 | Transmission Turbine Speed Switch Signal
19 | GY | 0.5 | Transmission Range Switch Signal C
20 | BN | 0.5 | TCC PWM Solenoid Valve Control