For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector to the sunroof switch.
2. Disengage the retaining clips (1) securing the sunroof switch to the sunroof overhead console.
3. Remove the sunroof switch from the sunroof overhead console.

### Installation Procedure

1. Install the sunroof switch to the sunroof overhead console.
2. Engage the retaining clips (1) to secure the sunroof switch to the sunroof overhead console.
3. Connect the electrical connector to the sunroof switch.