For 1990-2009 cars

## Fastener Tightening Specifications LHD

Application | Specification | Specification
--- | --- | ---
Metric | Imperial
A/C Compressor Bracket Mounting Bolt | 55 N·m | 41 lb ft
A/C Compressor Mounting Bolt V6 | 23 N·m | 17 lb ft
A/C Compressor Mounting Bolt V8 | 23 N·m | 17 lb ft
Air Inlet Assembly Lower Bolt | 9 N·m | 80 lb in
Air Inlet Assembly Upper Bolts | 9 N·m | 80 lb in
Air Outlet Duct Screws | 2 N·m | 18 lb in
Blower Motor Mounting Screws | 2 N·m | 18 lb in
Compressor Discharge Hose Bolt | 23 N·m | 17 lb ft
Compressor Suction Hose Bolt | 23 N·m | 17 lb ft
Condenser Inlet Hose Bolt | 23 N·m | 17 lb ft
Condenser Mounting Bolts | 11 N·m | 97 lb in
Condenser Discharge Hose Bolt | 23 N·m | 17 lb ft
Desiccant Bag Plug | N·m |
Evaporator Tube to Fan Shroud Screw | 2 N·m | 18 lb in
Heater Hose Bracket Screws | 2 N·m | 18 lb in
HVAC Module Assembly Mounting Nuts | 9 N·m | 80 lb in
HVAC Retaining bolts | 7 N·m | 62 lb in
Liquid pipe Bracket Screw | 23 N·m | 17 lb ft
Power Steering Line Bracket Nuts | N·m |
Rear Air Outlet Duct Nut | 1 N·m | 9 lb in
Refrigerant Pressure Sensor | 6 N·m | 53 lb in
TX valve Nut | 23 N·m | 17 lb ft