For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Inflatable Restraint Front End Module Sensor Retaining Bolts | 8 N·m | 71 lb in
Inflatable Restraint Instrument Panel Module Retaining Bolts | 16 N·m | 12 lb ft
Inflatable Restraint Roof Rail Module Retaining Bolts | 7 N·m | 62 lb in
Inflatable Restraint Sensing and Diagnostic Module to Body Retaining Nuts | 10 N·m | 89 lb in
Inflatable Restraint Side Impact Module Bracket to Seat Frame Retaining Bolts | 6 N·m | 53 lb in
Inflatable Restraint Side Impact Sensor Bolts | 8 N·m | 71 lb in
Seat Belt Buckle Pretensioner to Seat Retaining Bolts | 43 N·m | 32 lb ft