For 1990-2009 cars

### Removal Procedure

Important: Pull the front door bottom auxiliary sealing strip (1) from the door (2) to detach the retainers.

Remove the front door bottom auxiliary sealing strip (1) from the door (2).

### Installation Procedure

Important: Push the bottom auxiliary sealing strip (1) to the door (2) by hand to attach the retainers.

Install the front door bottom auxiliary sealing strip (1) to the door (2).