For 1990-2009 cars

## Clutch Backing Plate Retaining Ring Specifications 6L50

Table 1: | 3-5 Reverse Clutch
Table 2: | 1-2-3-4 Clutch
Table 3: | 4-5-6 Clutch
Table 4: | 2-6 Clutch
Table 5: | Low/Reverse Clutch

#### 3-5 Reverse Clutch

Clutch Pack Travel Specification - 1.20-1.74 mm (0.047-0.069 in)
Retaining Ring Thickness | O.D. Color
--- | ---
Metric | English
Note: After measuring clutch pack travel, determine if the measurement is within the specification. If the measurement is not within the specification, measure the thickness of the existing retaining ring, and then choose a thicker or thinner retaining ring that will bring the measurement within specification.
2.24-2.34 mm | 0.088-0.092 in | Purple - Purple
2.25-2.35 mm | 0.089-0.093 in | Light Green - Light Green
2.47-2.57 mm | 0.097-0.101 in | Gray - Gray
2.69-2.79 mm | 0.106-0.110 in | Yellow - Yellow
2.91-3.01 mm | 0.115-0.119 in | Orange - Orange
3.13-3.23 mm | 0.123-0.127 in | Light Blue - Light Blue
3.35-3.45 mm | 0.132-0.136 in | White - White
3.57-3.67 mm | 0.141-0.144 in | Yellow - Purple
3.79-3.89 mm | 0.149-0.153 in | Light Blue - Purple

#### 1-2-3-4 Clutch

Clutch Pack Travel Specification - 1.50-1.98 mm (0.059-0.078 in)
Retaining Ring Thickness | O.D. Color
--- | ---
Metric | English
Note: After measuring clutch pack travel, determine if the measurement is within the specification. If the measurement is not within the specification, measure the thickness of the existing retaining ring, and then choose a thicker or thinner retaining ring that will bring the measurement within specification.
2.25-2.35 mm | 0.089-0.093 in | Light Green - Light Green
2.47-2.57 mm | 0.097-0.101 in | Gray - Gray
2.69-2.79 mm | 0.106-0.110 in | Yellow - Yellow
2.91-3.01 mm | 0.115-0.119 in | Orange - Orange
3.13-3.23 mm | 0.123-0.127 in | Light Blue - Light Blue
3.35-3.45 mm | 0.132-0.136 in | White - White
3.57-3.67 mm | 0.141-0.144 in | Yellow - Purple
3.79-3.89 mm | 0.149-0.153 in | Light Blue - Purple

#### 4-5-6 Clutch

Clutch Pack Travel Specification - 1.17-1.76 mm (0.046-0.069 in)
Retaining Ring Thickness | O.D. Color
--- | ---
Metric | English
Note: After measuring clutch pack travel, determine if the measurement is within the specification. If the measurement is not within the specification, measure the thickness of the existing retaining ring, and then choose a thicker or thinner retaining ring that will bring the measurement within specification.
2.24-2.34 mm | 0.088-0.092 in | Purple - Purple
2.52-2.62 mm | 0.099-0.103 in | Light Green - Light Green
2.80-2.90 mm | 0.110-0.114 in | Gray - Gray
3.08-3.18 mm | 0.121-0.125 in | Yellow - Yellow
3.36-3.46 mm | 0.132-0.136 in | Orange - Orange
3.64-3.74 mm | 0.143-0.147 in | Light Blue - Light Blue
3.92-4.02 mm | 0.154-0.158 in | White - White
4.20-4.30 mm | 0.165-0.169 in | Yellow - Purple

#### 2-6 Clutch

Clutch Pack Travel Specification - 1.20-1.96 mm (0.047-0.077 in)
Retaining Ring Thickness | O.D. Color
--- | ---
Metric | English
Note: After measuring clutch pack travel, determine if the measurement is within the specification. If the measurement is not within the specification, measure the thickness of the existing retaining ring, and then choose a thicker or thinner retaining ring that will bring the measurement within specification.
1.64-1.74 mm | 0.065-0.069 in | Orange
1.92-2.02 mm | 0.076-0.080 in | Yellow Stripe
2.20-2.30 mm | 0.087-0.091 in | Light Blue Stripe
2.48-2.58 mm | 0.098-0.102 in | Purple Stripe
2.76-2.86 mm | 0.109-0.113 in | Green

#### Low/Reverse Clutch

Clutch Pack Travel Specification - 1.65-2.33 mm (0.065-0.092 in)
Retaining Ring Thickness | O.D. Color
--- | ---
Metric | English
Note: After measuring clutch pack travel, determine if the measurement is within the specification. If the measurement is not within the specification, measure the thickness of the existing retaining ring, and then choose a thicker or thinner retaining ring that will bring the measurement within specification.
1.98-2.08 mm | 0.078-0.082 in | Orange
2.28-2.38 mm | 0.090-0.094 in | Yellow Stripe
2.58-2.68 mm | 0.102-0.106 in | Light Blue Stripe
2.88-2.98 mm | 0.113-0.117 in | Purple Stripe
3.18-3.28 mm | 0.125-0.129 in | Green