For 1990-2009 cars

### Removal Procedure

1. Remove the convenience net (if fitted). Refer to Rear Compartment Stowage Tray Net Replacement .
2. Remove the rear carpet. Refer to Rear Compartment Floor Panel Carpet Replacement .
3. Remove the four convenience net retaining hooks (1) or the four fir tree retainers.

Important: Pull the end panel (1) to disengage the end panel retaining pins.

4. Remove the end panel (1) from the vehicle (2).

### Installation Procedure

Important: Push the end panel (1) to engage the end panel retaining pins.

1. Install the end panel (1) to the vehicle (2).
2. Install the four convenience net retaining hooks (1) or the four fir tree retainers.
3. Install the rear carpet. Refer to Rear Compartment Floor Panel Carpet Replacement .
4. Install the convenience net (if fitted). Refer to Rear Compartment Stowage Tray Net Replacement .