For 1990-2009 cars

### Removal Procedure

1. Cycle the sunroof window to the rear.
2. Remove the air deflector to sunroof module retaining bolt (1). Repeat for the opposite side.
3. Disconnect deflector spring (2) from the sunroof module. Repeat for opposite side.
4. With the aid of an assistant, slide the air deflector towards the rear of the vehicle to disengage the retaining clips (1) of the sunroof module.
5. Remove the air deflector from the vehicle.

### Installation Procedure

1. Install the air deflector to the sunroof module.
2. With the aid of an assistant, slide the air deflector towards the front of the vehicle to engage the retaining clips (1) of the sunroof module.
3. While holding the right side down push the left front side of the air deflector towards the right side.
4. Pull up on the left side until the lower tab (1) clears the roof opening.
5. Connect the deflector spring (2) to the sunroof module. Repeat for opposite side.
6. Install the air deflector to sunroof module retaining bolt (1). Repeat for opposite side.

Tighten
Tighten the bolts to 1 N·m (9 lb in).

7. Push the left front side of the air deflector inwards and down so the tab clears the roof opening.
8. Close the sunroof window.