For 1990-2009 cars

## Headliner Description LHD

### Formed Headliner

Important: The headliner is only serviced as a complete assembly

• | The headliner (4) is a one-piece composite substrate that is covered with a foam cloth facing.

• | The electrical wiring harness (2) for the roof lighting (3, 5), is not a serviceable item and should be left attached to the headliner when the headliner is being removed.

• | The headliner is held up to the roof panel by the use of located components, the overhead console (3), the assist handles (1) fasteners, the rear high mounted stop lamp (6).

• | If the vehicle is equipped with a sunroof, there are six patches of velcro™ material around the sunroof opening which add extra support for the headliner.