For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Wiper Motor Module to Bulk Head Retaining Bolts | 8 N·m | 71 lb in
Wiper Arm to Pivot Stud Retaining Nut | 35 N·m | 26 lb ft
Washer Solvent Container to Front End Module Support Retaining Bolts | 5 N·m | 44 lb in
Washer Solvent Container Filler Neck to Front End Module Bracket Retaining Bolt and Nut | 5 N·m | 44 lb in
Washer Solvent Container Filler Neck to Front End Module Bracket Retaining Torx Screw | 4 N·m | 35 lb in
Air Inlet Grille Brace to Air Inlet Grille Retaining Torx Screws | 2 N·m | 18 lb in
Heater Bracket to Engine Fastener | 22 N·m | 17 lb ft
Heater Bracket to Master Cylinder Fastener | 17 N·m | 12.5 lb ft