For 1990-2009 cars

Important: The recessed hub and the smaller sprocket of the right camshaft intermediate drive chain idler (2) is installed outward. The raised hub and the larger sprocket of the right camshaft intermediate drive chain idler (2) is installed towards the block.

1. Install the right camshaft intermediate drive chain idler (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the camshaft intermediate drive chain idler bolt (1).

Tighten
Tighten the bolt to 58 N·m (43 lb ft).