For 1990-2009 cars

Important: Take note of the following statements:

• | Do not try to repair a damaged energy absorber.

• | Replace the energy absorber if damaged.

• | Do not apply heat to the energy absorber.

• | Do not weld the energy absorber.

Important: Inspect the following components for signs of visible distortion:

• | Inspect the bumper impact bar (2).

• | Inspect the front end module (1).

• | Inspect the energy absorber (3).

• | Replace the energy absorber if damage is evident. Replace the energy absorber if a collision is so severe that the bumper impact bar does not return to its original position.