For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Door Striker to Pillar Retaining Screws | 13 N·m | 115 lb in
Door Latch to Door Retaining Screws | 13 N·m | 115 lb in
Fuel Filler Door Release Actuator to Upper Fuel Filler Neck Retaining Screws | 2 N·m | 18 lb in
Inside Door Handle to Door Trim Panel Retaining Screws | 3 N·m | 27 lb in
Lock Cylinder to Outside Door Handle Retaining Bolt | 4 N·m | 35 lb in
Outside Door Handle to Door Retaining Bolt | 4 N·m | 35 lb in
Outside Door Handle to Door Retaining Nut | 4 N·m | 35 lb in