For 1990-2009 cars

## Torque Converter Installation and Holding Fixture Removal 6L50

Callout | Procedure
--- | ---
Tip Rotate the transmission so that the fluid pan assembly is down.
1 | Transmission Case Assembly

#### Special Tools

• | DT-48067 Holding Fixture Adapter

• | DT-48989 Holding Fixture

• | J 3289-20 Holding Fixture Base Assembly

• | J 8763-B Holding Fixture

For equivalent regional tools, refer to Special Tools.

2 | Torque Converter Assembly