For 1990-2009 cars

## Fastener Tightening Specifications LWB

Application | Specification
--- | ---
Metric | English
Rear Quarter Window Retaining Nuts | 3 N-m | 27 lb in
Window Channel to Door Retaining Bolts | 8 N-m | 71 lb in
Window Regulator Motor to Window Regulator Retaining Bolts | 8 N-m | 71 lb in
Window Regulator to Door Retaining Bolts | 10 N-m | 89 lb in
Window Regulator to Window Retaining Bolts | 8 N-m | 71 lb in
Window Run Channel to Door Upper Retaining Screws | 3 N-m | 27 lb in