For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Manual Shaft Detent Lever Hub Pin Important: Discard the pin. Replace with NEW pin.
2 | Manual Shift Shaft Pin Important: Discard the pin. Replace with NEW pin.
3 | Manual Shift Shaft Important: Ensure the manual shift shaft seal is replaced before installing the shaft. Refer to Manual Shift Shaft Seal Replacement.
4 | Manual Shaft Detent Lever Assembly
5 | Park Pawl Actuator Assembly
6 | Park Pawl Actuator Guide Pin Important: Discard the pin. Replace with NEW pin. Tip Use a large pair of side cutters to "walk" the pin out.
7 | Park Pawl Actuator Guide
8 | Park Pawl Actuator Guide (O-ring) Seals Important: Discard seals. Replace with NEW seals.
9 | Park Pawl Important: Inspect for damage only. Do not remove. The park pawl is not a serviceable component.
10 | Park Pawl Spring Important: Inspect for damage only. Do not remove. The park pawl spring is not a serviceable component.