MODEL PAINT INFORMATION PAINT CODES. GMC Truck Caballero 1984

For 1990-2009 cars

# MODEL PAINT INFORMATION PAINT CODES

#### Models: All 1984 Models

The following is the list of paint code numbers from various suppliers for the 1984 model year. These colors can be obtained locally.

DuPont refinish paints are available in:

L-Lucite Acrylic Lacquer

A-Centari Acrylic Enamel

D Dulux Enamel

355S Flexible Additive

123 Vinyl Lacquer - Chip resiant

When ordering DuPont paint, use "L", "A", "D", 355S or 123 with the appropriate DuPont code.

Ditzler refinish paints are available in:

DDL - duracryl Acrylic Lacquer

DAR Delstar Acrylic Enamel

DAU - Deltron Acrylic Urethane

UCV - Vinyl Colors

DX-369 - Flexative - Flexible Finishes

DX-54 Roadguard - Road Abrasion Protection

When ordering Ditzler paint use "DDL", "DAR", "DAU", "UCV", "DX-369", or"DX-54" with appropriate Ditzler code.

Sherwin-Williams, Acme/Rogers, and Martin-Senour are available in acrylic lacquer or acrylic enamel.

S-W use: prefix 34, J4, or L10 for acrylic lacquer prefix 35, J5, or F10 for acrylic enamel

Acme use: prefix 84 for acrylic lacquer prefix 85 for acrylic enamel

Rogers use: prefix 94 for acrylic lacquer prefix 95 for acrylic enamel

Martin Senour: jobber will interchange number shown when acrylic lacquer is needed.

GMC EXTERIOR COLOR REFINISH NUMBERS

PART FISHER SHERWIN WILLIAMS COLOR WAEM DITZLER DUPONT MARTIN RINSHED CODE COLOR NAME CODE NUMBER NUMBER SENOUR ACME/ROGERS MASON

07 Black 20 DEG WA-2D 9348 B8479 32-16082 J5-1900/9739 EM-848 09 Black 30 DEG WA-30 9475 B8260 99-5533 32200 12864 EM-5118 12 White 5111 2185 817 82-1208 F8W-2030/1492 1347 14 Silver Metallic* 5281 8982* 44777 99-2433* J5-7981/25329* 17 Silver Metallic 7736 3507 C8251 99-5571 32369 12651

19 Black 5118 9000 99 3069 F10B-1738/3000 A946 P403 M403 21 Light Blue Metallic7470 3455 B8237 82-5580 32378 12868 23 Medium Blue 7154 3250 B8041 82-5258 30527 28 Dark Blue Metallic 8264 3685 B8461 82-5802 34073 14240 29 Dark Blue 7349 3362 B8139 82-5448 31514 12283 46 Dark Green 7156 3255 B8046 82-5263 30530 11505D 53 Yellow 5283 2929 44782 82-2436 F10Y-3752/25190 9156 61 Tan 8265 3686 B8462 82-5799 34070 14241 64 Light Saddle 8266 3687 B8463 82-5803 34076 14242 Metallic 66 Dark Brown Metallic 8267 3688 B8464 82-5800 34071 14243 71 Red Orange 7753 3463 B8250 82-5586 32384 12884F 72 Bright Red 7475 3464 B8241 82-5539 32097 12885V 73 Red 5285 2932 44774 82-2437 F10R-37555/25193 9158F 74 Red Metallic* 8301 72632*B8460 99-5804* 34077* 76 Red Metallic 8278 72616 B8465 82-5801 34072 14244R 79 Dark Carmine 8066 3164 45827 82-5152 30086 80 Slate Gray 7382 33470 B8207 82-5512 31993 85 Gray Metallic 4969 2964 44723 82-2455 F11A-3781/25221 87 Whetland Yellow 5247 2785 43536 82-5074 F10Y-3952/25511 2876D 88 Tangier Orange 5108 60156 31 82-5073 F10E-3953/25512 1597 93 Polar White 5704 2680 45107 82-2274 F10A-3553/11691 4430

*CLEARCOAT

Interior Color Refinish Codes

Ditzler-Number Dupont* Martin Senour Trim Color Fisher Semi- Low Semi-Gloss Semi Low Code Name Code Gloss Gloss UCV & Flat Gloss Gloss ---- ---- ---- ----- ----- --- ------ ----- ----- 12DN Graphite 7701 3708 33622 2-1020 C8457 32-16955 32-16963 16AN Light Gray 7771 33631 2-1010 D8323 32-16937 16BN Medium Gray 7772 33632 2-1011 D8324 32-16938 16CN Dark Gray 7773 33633 33707 2-1012 D8325 32-16939 32-16940 18DN Dark Charcoal 7350 33467 33492 2-871 D8213 3-16839 32-16851 23CN Medium Blue 7151 15391 15389 2-770 C8001 32-16737 32-16741 23DN Dark Blue 7163 15390 15392 2-765 C8002 32-16738 32-16742 62AN Light Saddle 7769 25361 25230 2-1025 C8451 32-16956 32-16912 62BN Medium Saddle 7770 25362 25231 2-1026 C8353 32-16957 32-16913 62DN Dark Saddle 8257 25367 25354 2-1086 C8452 32-16959 32-16969 62EN Very Dark Saddle 8285 25363 25355 2-1087 C8455 32-16961 32-16971 74CN Dark Carmine 7039 72273 72291 2-570 45224 32-16598 32-16621

74DN Very Dark Carmine 6212 72462 72343 2-694 C8103 32-16795 32-16747 76DN Dark Bronze 74656 25065 25069 2-837 D8211 32-16975 32-16975 795N Very Dark Bronze 8286 25364 25372 2-1033 C8456 32-16962 32-16972 77DN Dark Maple 7298 72435 73435 2-803 C8115 32-16777 32-16803 T7EN Very Dark Maple 8284 72602 72596 2-1089 C8454 32-16960 32-16970 82CN Medium Dark Gray 8247 33701 33665 2-1048 C8453 32-16958 32-16965

Sherwin-Williams Trim Color Acme/Rogers Rinshed-Mason Code Name Semi Gloss Low Gloss Semi Gloss Flat ---- ---- ---------- --------- ---------- ----- 12DN Graphite 33759 33767 W12A-7701 W5A-7701 16AN Light Gray 33199 16BN Medium Gray 33200 16CN Dark Gray 33201 33237 18DN Dark Charcoal 31889 31901 W25A-7350 W5A-7350 23CN Medium Blue 30816 30820 W25A-7151 W5A-7151 23DN Dark Blue 30817 30821 W25A-7163 W5A-7163 62AN Light Saddle 33760 32996 W12A-7769 62BN Medium Saddle 33761 32997 W12A-7770 62DN Dark Saddle 33763 33773 W12A-8257 W5A-8257 62EN Very Dark Saddle 33765 33775 W25A-8285 W5A-8285 74CN Dark Carmine J4-8580 J4-8684 W25A-7039 W5A-7039 92348 92441 74DN Very Dark Carmin 31551 30826 W25A-8212 76DN Dark Bronze 321722 32244 W25A-7465 W5A-7465 795N Very Dark Bronze 33766 33776 W25A-8286 W5A-8286 77DN Dark Maple 31201 31423 W25A-7298 W5A-7298 77EN Very Dark Maple 33764 33774 W12A-8284 W5A-8284 82CN Medium Dark Gray 33762 33769 W12A-8247 W5A-8247

*DuPont interior colors are formulated to the higher degree gloss as shown on the color card. To achieve a lower degree of gloss, add 4528S flattening compound according to the chart in the color book.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.