PAINT INFORMATION FOR 1994 TRUCK MODELS. GMC Truck S15 Pickup - 2WD 1994

For 1990-2009 cars

# PAINT INFORMATION FOR 1994 TRUCK MODELS

#### SUBJECT: PAINT INFORMATION

#### MODELS: 1994 TRUCK PRODUCTS

THE FOLLOWING CHART PROVIDES PAINT INFORMATION ON 1994 TRUCK PRODUCTS. THE PAINT TYPES LISTED BELOW THE MODELS INDICATE THE MATERIAL THE VEHICLE WAS MANUFACTURED WITH.

#### MODELS PAINT TYPE

CODE# NAME WA# C/K M/L G M/D S/T # PPG BASF DUP * 10 GHOST WHITE 9225 X 12 LINEN WHITE 5111 X X 14 GUNMETAL 8915 X 15 ASTRAL SILVER 8914 X 16 WARM GRAY MET. 9659 X 17 LT. SLATE MET. 7468 X 18 DOVE GRAY 9017 X 19 LAMP BLACK 5118 X X 20 LT QUASAR BLUE MET 9790 X X 21 RADAR BLUE MET. 9018 X 22 BAHAMA BLUE MET. 9656 X X 23 OCEAN BLUE 7154 X 24 MEDIUM BLUE MET. 9222 X 29 DK. BLUE 7349 X 30 ATLANTIC BLUE MET. 158A X 34 LT. TEAL MET. 9793 X 36 MED. DK. TEAL MET. 9828 X X 38 BRIGHT TEAL MET. 9794 X X 39 INDIGO MET. 9792 X X 41 BLACK 8555 X X X 43 EMERALD GREEN MET. 159A X 44 FOREST GREEN MET. 7964 X 46 DK. GREEN 7156 X 47 DK. BLUE MET. 9095 X 48 DK. RED 9096 X 50 OLYMPIC WHITE 8624 X X 52 KHAKI 9087 X 55 LT. AUTUMNWOOD MET. 228A X X 56 DK. AUTUMNWOOD MET. 161A X X 57 BEIGE MET. 5400 X 61 TAN 8265 X 71 RED ORANGE 7753 X 72 STANDARD RED 7475 X X X 74 VICTORY RED 9260 X X 75 GARNET RED MET. 8919 X 76 DK. GARNET RED MET. 9154 X X 80 MED.QUASAR BLUE MET 9791 X 83 RADISSON RED MET. 9916 X 84 DK.HUNT CLUB RED MET 9927 X 85 RASPBERRY MET. 9928 X 90 GRAY MET. 8798 X X 91 DK. ARGENT 6270 X 94 CHERRY RED MET. 8919 X 96 ULTRA SILVER MET. 8867 X X X

PAINT TYPES: DUP= DUPONT, PPG= PPG, BASF= BASF

#= C/K MODELS BUILT IN FT. WAYNE (PLANT CODE Z) USE DUPONT C/K MODELS BUILT IN OSHAWA (PLANT CODE 1) USE PPG C/K MODELS BUILT IN PONTIAC EAST (PLANT CODE E) USE DUPONT

*= S/T MODELS BUILT IN MORAINE (PLANT CODE 2) USE DUPONT S/T MODELS BUILT IN SHREVEPORT (PLANT CODE 8) USE BASF S/T MODELS BUILT IN LINDEN (PLANT CODE K) USE BASF S/T MODELS BUILT IN PONTIAC WEST (PLANT CODE 0) USE BASF

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1993 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.