SPECIAL POLICY: POWER DOOR LOCK SWITCHES. GMC Truck S15 Pickup - 2WD 1986

For 1990-2009 cars

# SPECIAL POLICY: POWER DOOR LOCK SWITCHES

GENERAL MOTORS HAS DETERMINED THAT SOME POWER DOOR LOCK FAILURES HAVE OCCURRED ON 1986-87 S/T MODEL TRUCKS. THE FAILURE MODES INCLUDE: INOPERATIVE SWITCHES, INTERMITTENT LOCKING AND UNLOCKING WHILE DRIVING OR PARKED, ACTUATOR STICKING AND ACTUATOR POPPING OUT OF SWITCH, IN ADDITION TO DURABILITY IMPROVEMENT IN THE NEW SWITCHES, THERE IS AN APPEARANCE CHANGE WHICH NECESSITATES CHANGING BOTH THE RIGHT AND LEFT DOOR LOCK SWITCHES WHEN ONE REQUIRES REPLACEMENT.

#### VEHICLES INVOLVED:

INVOLVED ARE CERTAIN 1986-87 S/T MODEL TRUCKS WITHIN THE FOLLOWING VIN BREAKPOINTS:

GMC

YEAR PLANT FROM THROUGH 1986 PONTIAC G0500004 G0521489 1987 PONTIAC H0500001 H0525609 1986 MORAINE G2500035 G2533216 1987 MORAINE H2500001 H2538543 1986 SHREVEPORT G8500005 G8530693 1987 SHREVEPORT H8500001 H8542190

CHEVROLET

1986 PONTIAC G0100001 G0171774 1987 PONTIAC H0100008 H0188556 1986 MORAINE G2100001 G2238717 1987 MORAINE H2100001 H2271470 1986 SHREVEPORT G8100001 G8212409 1987 SHREVEPORT H8100001 H8237837

SPECIAL POLICY ADJUSTMENT

SHOULD THIS CONDITION OCCUR, GENERAL MOTORS WILL REPAIR INVOLVED VEHICLES AT NO CHARGE FOR A PERIOD OF FIVE YEARS, REGARDLESS OF MILEAGE, FROM THE DATE THE VEHICLE WAS ORIGINALLY PLACED IN SERVICE.

THIS SPECIAL POLICY ADJUSTMENT BULLETIN SHOULD BE FILED IN THE THREE RING BINDER FURNISHED EACH DEALER BY GENERAL MOTORS.

OWNER NOTIFICATION

OWNERS OF VEHICLES INVOLVED IN THIS SPECIAL POLICY ADJUSTMENT WILL BE NOTIFIED BY GMC TRUCK (SEE COPY OF OWNER LETTER INCLUDED WITH THIS BULLETIN).

SERVICE PROCEDURE - 1986-87 S/T DOOR LOCK SWITCHES - REPLACE

REMOVE OR DISCONNECT (FIGURE NO. 1)

1. BATTERY GROUND CABLE FROM BATTERY.

2. DOOR TRIM PANELS INCLUDING ARM RESTS. REFERENCE DOORS (SECTION 10A1) IN SERVICE MANUAL X-8729.

3. EACH HARNESS CONNECTOR (FIGURE NO. 1-A).

4. EACH SWITCH (FIGURE NO. 1-B). PRESS IN BOTH SPRING CLIPS TO REMOVE EACH SWITCH.

INSTALL OR CONNECT (FIGURE NO. 1)

1. SWITCHES (B).

2. HARNESS CONNECTORS (A).

3. BOTH DOOR TRIM PANELS AND ARM RESTS (SECTION 10A1).

4. BATTERY GROUND CABLE TO THE BATTERY.

#### PARTS INFORMATION:

PARTS ARE AVAILABLE FROM GENERAL MOTORS SERVICE PARTS OPERATION (GMSPO).

PART NUMBER DESCRIPTION QUANTITY

15622301* LEFT POWER DOOR 1 LOCK SWITCH

15622302* RIGHT POWER DOOR 1 LOCK SWITCH

* APPEARANCE CHANGE NECESSITATES CHANGING BOTH SWITCHES WHEN ONE NEEDS REPLACEMENT.

#### WARRANTY INFORMATION:

DEALERS SHOULD SUBMIT A WARRANTY CLAIM ON EACH VEHICLE COMPLETED.

LABOR OPERATION TIME NUMBER DESCRIPTION ALLOWANCE

T7510 REPLACE BOTH POWER .8 HRS. DOOR LOCK SWITCHES

T7511 REIMBURSEMENT IF PREVIOUS REPAIR PERFORMED - NET ITEM COLUMN TYPE CODE M

#### REIMBURSEMENT:

CLAIMS FOR CUSTOMER REIMBURSEMENT FOR PREVIOUSLY PAID REPAIRS ARE ELIGIBLE FOR REIMBURSEMENT OF REPAIR EXPENSES DUE TO A PREVIOUS POWER DOOR LOCK MALFUNCTION.

TO OBTAIN REIMBURSEMENT, ELIGIBLE OWNERS MUST SUBMIT CLAIMS TO AN AUTHORIZED GMC TRUCK DEALER PRIOR TO MAY 31, 1989. THE REIMBURSEMENT SHOULD NOT EXCEED THE AMOUNT APID BY GMC TRUCK FOR THE APPLICABLE LABOR OPERATION.

WHEN A CUSTOMER REQUESTS REIMBURSEMENT THE FOLLOWING MUST ACCOMPANY THAT REQUEST:

PROOF OF OWNERSHIP, AND ORIGINAL PAID RECEIPT, OR A COPY OF RECEIPT WITH PROOF OF PAYMENT.

CLAIMS FOR CUSTOMER REIMBURSEMENT ON PREVIOUSLY PAID REPAIRS ARE TO BE SUBMITTED ON A WARRANT CLAIM.

GMC DISCLAIMER.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.