A/C NOISE/VIBRATION (INSTALL NEW SERVICE PART). GMC Truck S15 Pickup - 4WD 1989

For 1990-2009 cars

# A/C NOISE/VIBRATION (INSTALL NEW SERVICE PART)

#### SUBJECT: AIR CONDITIONING NOISE/VIBRATION, (INSTALL NEW PART).

#### VEHICLES AFFECTED: 1987-89 TRUCKS W/2.8L ENGINE AND A/C

Some 1987-89 S/T Trucks equipped with 2.8L engines may exhibit a noise/ vibration when the air conditioning compressor is engaged. The noise/vibration is the result of a resonance set up in the serpentine accessory drive system with air conditioning on. If this condition is experienced, install kit P/N 10115893. Installation instructions are included with the kits.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.