PAINT CODES & SUPPLIES LISTED INTERIOR/BASECOAT/CLEARCOAT. GMC Truck S15 Pickup - 2WD 1990

For 1990-2009 cars

# PAINT CODES & SUPPLIES LISTED INTERIOR/BASECOAT/CLEARCOAT

#### VEHICLES AFFECTED: ALL TRUCKS

The following is a list of paint code numbers from various suppliers for the 1990 model year. These colours can be obtained locally. (List Attached).

DuPont refinish paints are available in:

L-Lucite(R) - Acrylic Lacquer A-Centari(R) - Acrylic Enamel J-Cronar(R) - Polyoxithane Enamel K-Chromabase(R) 350S-Flexible Additive 310S-Black 123 Vinyl Lacquer - Chip Resistant 330S-White 123 Vinyl Lacquer - Chip Resistant

#### IMPORTANT: Vinyl resin must be added to the base colour when painting interior components.

DuPont vinyl resin #304 - instrument panel

DuPont vinyl resin #305 - all remaining interior parts except seats.

DuPont vinyl resin #306 - seats and vinyl roofs.

When ordering DuPont paint, use "L", "A", "J", "K", 350S or 123 White or 123 Black with the appropriate DuPont code.

* DDL - Duracryl Acrylic Lacquer or Acrylic B/C * DBU - Deltron Basecoat/Clearcoat * DAR - Deltron Acrylic Enamel * DAU - Deltron Acrylic Urethane * UCV - Vinyl Colours * DX - 369 Flexative Flexible Finishes * DX - 54 Roadguard Road Abrasion Protection

When ordering PPG (Ditzler) paint, use "DDL", "DBU", "DAR", "DAU", "UCV", "DX-54", "DX-369" with appropriate Ditzler code.

Sherwin-Williams, Acme/Rogers, and Martin-Senour are available in acrylic lacquer, acrylic enamel, or acrylic urethane.

S-W use: prefix 34, J4 or L10 for acrylic lacquer, prefix 35, J5 or F10 for acrylic enamel, prefix UB for acrylic urethane in a basecoat/clearcoat system prefix US for acrylic urethane in a single stage system

ACME use: prefix 84 for acrylic lacquer, prefix 85 for acrylic enamel, a prefix PB for acrylic urethane in basecoat/clearcoat system prefix PS for acrylic urethane in a single stage system

Rogers use: prefix 94 for acrylic lacquer, prefix 95 for acrylic enamel, prefix AU for acrylic urethane in a basecoat/clearcoat system prefix AS for acrylic urethane in a single stage system

Martin-Senour: Jobber will interchange number shown when acrylic lacquer is need. use prefix 98 for acrylic urethane as a pre-mix basecoat/clearcoat use prefix 88 for acrylic urethane as a factory packaged basecoat/clearcoat use prefix 97 for acrylic urethane as a pre-mix single stage system use prefix 87 for acrylic urethane as a factory packaged single stage system

1990 TRUCK INTERIOR COLORS

Sherwin- PPG GM Gloss Fisher Martin- Williams PPG Vinyl Trim Color Name W-Code Senour Acme- DIA Interior Code Semi Flat Rogers Code UCV Code ---- ---------- ---- ---- ------ ------ ------ ---- -------- 12DN Graphite x 7701 16963 33767 33870 2-1020 16CN Dark Gray x 7773 17117 34995 33871 2-1012 x 16940 33237 33707 18DN Dark Charcoal x 7350 17113 34991 33872 2-871 x 16851 31901 33492

19DN Black 16918 33024 9640 848 16615 J4-8677 120 92387 9433 23CN Medium Blue x 7151 17111 34989 15951 2-770 16741 30820 15389 23DN Dark Blue x 7163 16742 30821 15392 2-765 24CN Dark Blue x 9059 36478 36478 16323 2-1276 x 39838 39838 24DN Very Dark Blue x 8576 17067 34598 15886 2-1098 x 17075 34606 16092 24EN Midnight Blue x 9541 42600 42600 16998 2-1396 x F425-99 42599 16999 47CN Dark Red x 9104 42602 42602 73381 2-1394 x 42601 42601 73380 47DN Very Dark Red x 9253 42604 42604 73383 2-1395 x 42603 42603 73382 60BN Medium Cognac x 9205 38394 38394 26281 2-1292 38393 38393 -- 60CN Dark Cognac x 9099 38395 38395 26284 2-1315 x 38392 38392 -- 60DN Very Dark x 9252 38391 38391 26285 2-1316 Cognac 69BN Medium Beige x 8248 16950 33715 25313 2-1045 x 16966 33770 -- 69CN Medium Dark x 8280 17066 34597 25514 2-1117 Beige x 17074 34605 25571 82CN Medium Dark Gray 8247 16949 33714 33665 2-1048 16965 33769 33873 82DN Dark Gray x 8595 17071 34602 33824 2-1125 17080 34611 33874

GM Gloss Fisher (BASF) Trim Color Name W-Code Rinshed DuPont Code Semi Flat Mason ---- ---------- ---- ---- ------ ----- -------- 12DN Graphite x 7701 14028 C8345 16CN Dark Gray x 7773 16067 C8586 x 16068 18DN Dark Charcoal x 7350 12730 C8575 x 14030

19DN Black 4401 848 12812 C8535

23CN Medium Blue x 7151 11535 C8576 11593 23DN Dark Blue x 7163 11595 C8002 24CN Dark Blue x 9059 17124 C8792 x 19021 24DN Very Dark Blue x 8576 15080 C8539 x 16045 24EN Midnight Blue x 9541 20065 C9006 x 20066 47CN Dark Red x 9104 20061 C9007 x 20062 47DN Very Dark Red x 9253 20063 C9008 x 20064 60BN Medium Cognac x 9205 18055 C8808 19022 60CN Dark Cognac x 9099 18056 C8810 x 18057 60DN Very Dark x 9252 18059 C8819 Cognac 69BN Medium Beige x 8248 14006 C8446 x 20060 69CN Medium Dark x 8280 17120 C8554 Beige x 15065 82CN Medium Dark Gray 8247 14009 C8447 14088 82DN Dark Gray x 8595 15268 C8550

#### 1990 TRUCK EXTERIOR COLORS

Paint Sherwin- Color Color Name Fisher DuPont Martin-Senour Williams Code W-Code Acme-Rogers ---- ---------- ------ ------ ------------- ------------ 10 White B/C 9225 B8796 36783 36783 12 White 5111 817 30-3563 L10A-1369 1492 15 Silver Metallic B/C 8914 C8501 32-5452 34856 17 Slate Metallic 7468 B8235 - - 19 Black 5118 99S 3069 L10B-1738 3000/4590 20 Black B/C 8555 99S 30-5296 33756 21 Light Blue Metallic 7470 B8237 30-5143 32378 23 Medium Blue 7154 B8041 30-4907 30527 24 Bright Blue Metallic 9222 B8894 38144 38144 27 Light Blue Metallic B/C 9264 B8944 39337 39337 29 Dark Blue 7349 B8139 30-5079 31514 30 Medium Blue Metallic B/C 9086 B9017 42478 42478 33 Light Mesa Brown B/C 9207 B8945 39338 39338 34 Light Mesa Brown Metallic B/C 9208 B8895 38145 38145 36 Dark Hunter Green Metallic B/C 9210 B8896 38146 38146 37 Light Mesa Brown 9219 B8897 38147 38147 40 Dark Mesa Brown Metallic 9202 B8942 40380 40380 42 Bright Blue 9203 B8943 40381 40381 44 Forest Green Metallic 7964 D8801 30-5539 35441 46 Woodland Green 7156 B8046 30-4912 30530 47 Dark Blue Metallic 9095 B9019 42479 42479 48 Dark Red 9096 B9020 42480 42480 50 White B/C 8624 B8550 32-5455 34851 52 Gold Metallic B/C 9008 B8738 36345 36345 58 Light Sandstone Metallic B/C 8865 B8792 36450 36450 61 Tan 8265 B8462 30-5329 34070 67 Saddle Metallic 8799 B8630 30-5489 35342 68 Dark Saddle Metallic B/C 9212 B8741 36452 36452 70 Red B/C 8832 B8793 36453 36453 71 Red Orange 7753 B8250 30-5146 32384 72 Bright Red 7475 B8241 30-5120 32097 74 Red B/C 9260 B8946 39339 39339 75 Red Metallic B/C 8919 C6506 32-5459 34855 77 Dark Garnet Red Metallic B/C 9154 B8742 36454 36454 78 Dark Maple Metallic 8800 B8632 32-5524 35366 83 Gunmetal Metallic B/C 8915 C8502 32-5467 35082 86 Wheatland Yellow B/C 9014 B8743 32-8545 35586 87 Wheatland Yellow 5247 43536 30-4761 L10Y-3952 25511 88 Tangier Orange 5108 31 30-4760 L10E-3953 25512 89 Tangier Orange B/C 9013 B8744 30-5550 35587 90 Gray Metallic 8798 B8629 30-5490 35367 94 Red Metallic B/C 9088 B9018 42481 42481 96 Silver Metallic B/C 8867 B8795 36457 36457 98 Black Saphire Metallic B/C 8863 B8745 36458 36458

Paint BASF Color Color Name PPG Rinshed Code DDL-DAR Mason ---- ---------- -------- ----- 10 White B/C 4015* 18121 12 White 2185 1347

15 Silver Metallic B/C 3796* 15251 17 Slate Metallic 3453 12866 19 Black 9000/9300 Standard Package 20 Black B/C 9700 13572 21 Light Blue Metallic 3455 12868 23 Medium Blue 3250 11500 24 Bright Blue Metallic 4110 18120 27 Light Blue Metallic B/C 4146 19031 29 Dark Blue 3362 12238 30 Medium Blue Metallic B/C 4238 20050 33 Light Mesa Brown B/C 4152 19028 34 Light Mesa Brown Metallic B/C 4107 18116 36 Dark Hunter Green Metallic B/C 4108 18117 37 Light Mesa Brown 4111 18118 40 Dark Mesa Brown Metallic 4180 19026 42 Bright Blue 16813 19027 44 Forest Green Metallic 4114 15366 46 Woodland Green 3255 11505 47 Dark Blue Metallic 4251 20052 48 Dark Red 4239 20053 50 White B/C 3800 15255 52 Gold Metallic B/C 3917 17113 58 Light Sandstone Metallic B/C 4020 18111 61 Tan 3686 14241 67 Saddle Metallic 3914 16116 68 Dark Saddle Metallic B/C 4001 17116 70 Red B/C 4021 18115 71 Red Orange 3463 12884 72 Bright Red 3464 12885 74 Red B/C 4154 19030 75 Red Metallic B/C 3804* 15259 77 Dark Garnet Red Metallic B/C 4002* 17117 78 Dark Maple Metallic 3915 16117 83 Gunmetal Metallic B/C 3805 15260 86 Wheatland Yellow B/C 3911 15616 87 Wheatland Yellow 2785 2876 88 Tangier Orange 60156 1597 89 Tangier Orange B/C 3912 15617 90 Gray Metallic 3916 16118 94 Red Metallic B/C 4240 20051 96 Silver Metallic B/C 4023 18112 98 Black Saphire Metallic B/C 4003 17118

B/C Basecoat/Clearcoat

*M Van Only

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.