For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Luggage Carrier Side Rail Finish Covers (Qty: 3) Tip Using a suitable tool to lift upward on the lower corner, this will access in the removal.
2 | Luggage Carrier Side Rail Mounting Nuts (Qty: 5) Caution: Refer to Fastener Caution in the Preface section. Tighten 10N·m(89 lb in)
3 | Luggage Carrier Side Rail
4 | Luggage Carrier Side Rail Gasket (Qty: 3)