For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Axle Shaft Caulking Hub Nut | 320 N·m | 236 lb ft
Intermediate Axle Shaft Mounting Bracket Bolts | 70 N·m | 52 lb ft
Knuckle to Upper Control Arm Nut and Bolt | 160 N·m | 118 lb ft
Lower Ball Joint Nut | 10 N·m | 89 lb in
Lower Control Arm to Knuckle Bolt and Nut | 160 N·m | 118 lb ft
Outer Tie Rod Nut | 50 N·m | 37 lb ft
Toe Link to Knuckle Nut and Bolt | 160 N·m | 118 lb ft
Trailing Arm Bracket to Underbody Bolt | 110 N·m | 81 lb ft
Wheel Nuts | 125 N·m | 92 lb ft