For 1990-2009 cars

Connector 1: | Driver Information Center (C100/Long Body)
Connector 2: | Driver Information Center (C105/Short Body)
Connector 3: | Clock
Connector 4: | Instrument Cluster
Connector 5: | Outside Air Temperature/Air Quality Sensor

### Driver Information Center (C100/Long Body)

#### Connector Part Information

- OEM: PED 15394150
- Service: N/A
- Description: 16-Way F Mirco 064 Unsealed

#### Driver Information Center (C100/Long Body)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RD/WH | -- | Battery Positive Voltage
2 | BK | -- | Ground
3 | -- | -- | Not Used
4 | YE | -- | Backlight Lamp Control
5 | BN/WH | -- | Signal Ground
6 | PK | -- | Run/Crank Ignition 1 Voltage
7 | D-GN | -- | Low Speed GMLAN Serial Data
8-14 | -- | -- | Not Used
15 | BN/WH | -- | CAN Bus High Serial Data
16 | -- | -- | Not Used

### Driver Information Center (C105/Short Body)

#### Connector Part Information

- OEM: TYCO 968265-1
- Service: N/A
- Description: 32-Way F 064 Quadlock (BK)

#### Driver Information Center (C105/Short Body)

Pin | WireColor | Circuit No | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | BK/WH | -- | Ground
3 | RD/WH | -- | Battery Positive Voltage
4 | -- | -- | Not Used
5 | RD/WH | -- | Battery Positive Voltage
6-16 | -- | -- | Not Used
17 | BN/WH | -- | MID Speed CAN High
18 | BN | -- | MID Speed CAN Low
19 | BN | -- | MID Speed CAN Low
20 | BN/WH | -- | MID Speed CAN High
21 | -- | -- | Not Used
22 | BN/WH | -- | MID Speed CAN High
23 | BN | -- | MID Speed CAN Low
24 | -- | -- | Not Used
25 | D-GN | -- | Low Speed GMLAN Serial Data
26-32 | -- | -- | Not Used

### Clock

#### Connector Part Information

- OEM: PED 15499930
- Service: N/A
- Description: 6-Way F Mirco 064 Unsealed

#### Clock

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | RD/WH | -- | Battery Positive Voltage
3 | YE | -- | Accessory Voltage
4 | YE | -- | Backlight Lamp Control
5 | BN/WH | -- | Signal Ground
6 | -- | -- | Not Used

### Instrument Cluster

#### Connector Part Information

- OEM: PED 15394150
- Service: N/A
- Description: 16-Way F Mirco 064 Unsealed

#### Instrument Cluster

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | -- | Run/Crank Ignition 1 Voltage
2 | RD/WH | -- | Battery Positive Voltage
3 | -- | -- | Not Used
4 | PU | -- | Passenger Seat Belt Indicator
5 | BN/WH | -- | Transfer Case Positive Switch Ch 4 Encoder Signal
6 | OG/BK | -- | Sensor Low Reference
7 | D-GN/WH | -- | Outside Ambient Air Temperature Sensor S
8 | BN/WH | -- | Windshield Washer Fluid Level Sensor Signal
9 | YE | -- | Backlight Lamp Control
10 | BK | -- | Ground
11 | -- | -- | Not Used
12 | GY | -- | Rear Parking Assist Red Indicator Control
13 | BK | -- | Ground
14 | D-GN | -- | Low Speed GMLAN Serial Data
15 | -- | -- | Not Used
16 | PU | -- | Brake Fluid Level Sensor Signal

### Outside Air Temperature/Air Quality Sensor

#### Connector Part Information

- OEM: KET MG 610331
- Service: N/A
- Description: 4-Way F SWP Sealed

#### Outside Air Temperature/Air Quality Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG/BK | -- | Low Reference
2 | BN | -- | Ignition 3 Voltage
3 | GN/WH | -- | Outside Air Temperature Signal
4 | PU/WH | -- | Air Quality Sensor Signal