For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Center Pillar Lower Garnish Molding Screw | 22 N·m | 16 lb ft
Driver Knee Bolster Bolts | 20 N·m | 15 lb ft
Driver Knee Bolster Screws | 2.5 N·m | 23 lb in
Floor Console Bolts | 8 N·m | 71 lb in
Front Console Retainer Screw | 2 N·m | 18 lb in
Hood Latch Release Handle Mounting Screw | 3 N·m | 27 lb in
Quarter Window Garnish Molding Screw | 2 N·m | 18 lb in
Rear Compartment Stow Tray Bolts | 8 N·m | 71 lb in
Rear Wheelhouse Trim Panel Screws | 2 N·m | 18 lb in
Windshield Garnish Molding Screw | 2 N·m | 18 lb in