For 1990-2009 cars

Connector 1: | Accelerator Pedal Position Sensor
Connector 2: | Boost Pressure Sensor
Connector 3: | Camshaft Position (CMP) Sensor
Connector 4: | Crankshaft Position (CKP) Sensor
Connector 5: | Diesel Particulate Filter Pressure Sensor
Connector 6: | Engine Coolant Temperature (ECT) Sensor
Connector 7: | Exhust Gas Recirculation (EGR) Valve
Connector 8: | Exhust Gas Temperature Sensor 1
Connector 9: | Exhust Gas Temperature Sensor 2
Connector 10: | Fuel Filter Heater/Temperature Sensor
Connector 11: | Glow Plug Control Unit
Connector 12: | Fuel Injector 1
Connector 13: | Fuel Injector 2
Connector 14: | Fuel Injector 3
Connector 15: | Fuel Injector 4
Connector 16: | Fuel Pump Module
Connector 17: | Fuel Rail Pressure Control Valve
Connector 18: | Fuel Rail Pressure Sensor
Connector 19: | High Pressure Pump
Connector 20: | Mass Air Flow (MAF) Sensor
Connector 21: | Oil Level Switch
Connector 22: | Oil Pressure Switch
Connector 23: | PTC Heater
Connector 24: | Throttle Plate Actuator
Connector 25: | Water In Fuel Sensor

### Accelerator Pedal Position Sensor

#### Connector Part Information

- OEM: PED 15326830
- Service: N/A
- Description: 6-Way F GT 150 Series Unsealed

#### Accelerator Pedal Position Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WH/BK | -- | Accelerator Pedal Position 5-Volt Reference 1
2 | D-BU | -- | Accelerator Pedal Position Signal 1
3 | BN | -- | Accelerator Pedal Position Low Reference 1
4 | PU | -- | Accelerator Pedal Position Low Reference 2
5 | L-GN | -- | Accelerator Pedal Position Signal 2
6 | BN | -- | Accelerator Pedal Position 5-Volt Reference 2

### Boost Pressure Sensor

#### Connector Part Information

- OEM: TYCO 368162-1
- Service: N/A
- Description: 4-Way F JPT Sealed

#### Boost Pressure Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN/WH | -- | Heated O2 Sensor High Control Sensor 2
2 | YE | -- | Signal
3 | GN/WH | -- | Heated O2 Sensor Low Control Sensor 1
4 | WH | -- | Battery Positive Voltage

### Camshaft Position (CMP) Sensor

#### Connector Part Information

- OEM: TYCO 85205-1
- Service: N/A
- Description: 3-Way F JPT Sealed

#### Camshaft Position (CMP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WH/BN | -- | Signal
2 | RD | -- | Heated O2 Sensor High Signal
3 | PK/BK | -- | Engine Main Relay Fused Control (3)

### Crankshaft Position (CKP) Sensor

#### Connector Part Information

- OEM: TYCO 85205-1
- Service: N/A
- Description: 3-Way F JPT Sealed

#### Crankshaft Position (CKP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN | -- | Input
2 | GY | -- | Heated O2 Sensor Heater Low Control Bank 1 Sensor 1
3 | BK/WH | -- | Input

### Diesel Particulate Filter Pressure Sensor

#### Connector Part Information

- OEM: FEP 1J0973703
- Service: N/A
- Description: 3-Way F Sealed

#### Diesel Particulate Filter Pressure Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | -- | 5-Volt Reference (LHD)
D-GN | -- | 5-Volt Reference (RHD)
2 | BN/WH | -- | Low Reference
3 | D-GN | -- | Signal

### Engine Coolant Temperature (ECT) Sensor

#### Connector Part Information

- OEM: PED 12040753
- Service: N/A
- Description: 2-Way F 150 Series Sealed

#### Engine Coolant Temperature (ECT) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | -- | CTS Ground
2 | YE | -- | CTS Signal

### Exhust Gas Recirculation (EGR) Valve

#### Connector Part Information

- OEM: TYCO 827551-3
- Service: N/A
- Description: 2-Way F Timmer Sealed

#### Exhust Gas Recirculation (EGR) Valve

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | -- | EGR
2 | PK/BK | -- | Engine Main Relay Coil Control (3)

### Exhust Gas Temperature Sensor 1

#### Connector Part Information

- OEM: 621-02020
- Service: N/A
- Description: 2-Way F

#### Exhust Gas Temperature Sensor 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GN | -- | Signal 1
2 | BK/WH | -- | Low Reference

### Exhust Gas Temperature Sensor 2

#### Connector Part Information

- OEM: 621-02020
- Service: N/A
- Description: 2-Way F

#### Exhust Gas Temperature Sensor 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GN/BK | -- | Signal 2
2 | BK | -- | Low Reference

### Fuel Filter Heater/Temperature Sensor

#### Connector Part Information

- OEM: FCI 17260406A
- Service: N/A
- Description: 6-Way F 150/280 Series Sealed

#### Fuel Filter Heater/Temperature Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | BK | -- | Ground (LHD)
Ignition Voltage (RHD)
4 | BU | -- | Power Take Off Enable Switch (LHD)
Fuel Filter Heater (RHD)
5 | GN | -- | Heated Oxygen Sensor Low Signal Bank 2 Sensor 1 (LHD)
Fuel Temperature Signal (RHD)
6 | BK/WH | -- | Heated Oxygen Sensor High Signal Bank 2 Sensor 1 (LHD)
Fuel Temperature Ground (RHD)

### Glow Plug Control Unit

#### Connector Part Information

- OEM: FCI 60432001
- Service: N/A
- Description: 11-Way F Sealed

#### Glow Plug Control Unit

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | -- | Shunt High Signal
2 | GY | -- | Shunt High Signal
3 | GY | -- | Shunt High Signal
4 | GY | -- | Shunt High Signal
5 | -- | -- | Not Used
6 | PK/BK | -- | Ignition Voltage
7 | BK/WH | -- | Signal Ground
8 | -- | -- | Not Used
9 | WH | -- | GPCU 01
10 | RD/WH | -- | Battery Positive Voltage
11 | WH/RD | -- | GPCU ST

### Fuel Injector 1

#### Connector Part Information

- OEM: BOSCH 1928403874
- Service: N/A
- Description: 2-Way F Sealed

#### Fuel Injector 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN | -- | High
2 | WH | -- | Low

### Fuel Injector 2

#### Connector Part Information

- OEM: BOSCH 1928403874
- Service: N/A
- Description: 2-Way F Sealed

#### Fuel Injector 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE/D-BU | -- | High
2 | D-BU | -- | Low

### Fuel Injector 3

#### Connector Part Information

- OEM: BOSCH 1928403874
- Service: N/A
- Description: 2-Way F Sealed

#### Fuel Injector 3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE/BK | -- | High
2 | D-GN/BK | -- | Low

### Fuel Injector 4

#### Connector Part Information

- OEM: BOSCH 1928403874
- Service: N/A
- Description: 2-Way F Sealed

#### Fuel Injector 4

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | -- | High
2 | GY | -- | Low

### Fuel Pump Module

#### Connector Part Information

- OEM: KET MG641521
- Service: N/A
- Description: 5-Way F 090II Sealed

#### Fuel Pump Module

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | -- | Run/Crank Ignition Voltage
2 | BN/WH | -- | Fuel Level Sensor Low
3 | D-BU | -- | Primary Fuel Level Sensor
4 | GY | -- | Fuel Pump Supply Voltage
5 | BK | -- | Ground

### Fuel Rail Pressure Control Valve

#### Connector Part Information

- OEM: BOSCH 1928403874
- Service: N/A
- Description: 2-Way F Sealed

#### Fuel Rail Pressure Control Valve

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | -- | Low
2 | D-BU/WH | -- | Ground

### Fuel Rail Pressure Sensor

#### Connector Part Information

- OEM: BOSCH 1928403968
- Service: N/A
- Description: 2-Way F Sealed

#### Fuel Rail Pressure Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WH | -- | Ground
2 | D-BU | -- | Signal
3 | YE | -- | Supply

### High Pressure Pump

#### Connector Part Information

- OEM: BOSCH 1928403874
- Service: N/A
- Description: 2-Way F Sealed

#### High Pressure Pump

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RD/BK | -- | Low
2 | BK | -- | Ground

### Mass Air Flow (MAF) Sensor

#### Connector Part Information

- OEM: BOSCH 1928403736
- Service: N/A
- Description: 4-Way F Sealed

#### Mass Air Flow (MAF) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | -- | Run/Crank Ignition 1 Voltage
2 | D-GN | -- | Ground
3 | D-GN | -- | Signal
4 | YE | -- | STC

### Oil Level Switch

#### Connector Part Information

- OEM: PED 12052641
- Service: N/A
- Description: 2-Way F Metri-Pack 150 Series Sealed

#### Oil Level Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-GN | -- | Oil Level SW Signal
2 | BN | -- | Ground

### Oil Pressure Switch

#### Connector Part Information

- OEM: PKI 832104
- Service: N/A
- Description: 1-Way F 150 Series Sealed

#### Oil Pressure Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | -- | Oil Pressure Gage Signal

### PTC Heater

#### Connector Part Information

- OEM: PED15326878
- Service: N/A
- Description: 3-Way F GT 280 Series Unsealed

#### PTC Heater

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BU/WH | -- | PTC Heater Supply Voltage
GY | -- | Fuel Tank Pressure Sensor 5-Volt Reference
2 | YE/BK | -- | PTC Heater Supply Voltage
GY | -- | Fuel Tank Pressure Sensor Signal
3 | BN | -- | PTC Heater Supply Voltage

### Throttle Plate Actuator

#### Connector Part Information

- OEM: FEP 42121400
- Service: N/A
- Description: 4-Way F Sealed

#### Throttle Plate Actuator

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK/WH | -- | Ground
2 | PK/BK | -- | Ignition Voltage
3 | GN | -- | Feedback
4 | WH | -- | Control

### Water In Fuel Sensor

#### Connector Part Information

- OEM: TYCO 85205-1
- Service: N/A
- Description: 3-Way F JPT Sealed

#### Water In Fuel Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WH | -- | WIF Sensor
2 | BK | -- | Ground
3 | PK | -- | Run/Crank Ignition 1 Voltage