For 1990-2009 cars

Connector 1: | Inclination Sensor
Connector 2: | Intrusion Sensor
Connector 3: | Power Sounder
Connector 4: | Remote Control Door Lock Receiver
Connector 5: | Theft Deterent Control Module

### Inclination Sensor

#### Connector Part Information

- OEM: PED 15324229
- Service: N/A
- Description: 4-Way F Timer Micro I Unsealed (BK)

#### Inclination Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RD/WH | -- | Battery Positive Voltage
2 | -- | -- | Not Used
3 | L-BU | -- | Incline Sensor Alarm On Signal
4 | D-GN | -- | Alarm Armed Signal

### Intrusion Sensor

#### Connector Part Information

- OEM: TYCO 368500-1
- Service: N/A
- Description: 3-Way F 070 Unsealed

#### Intrusion Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GN | -- | Alarm Armed Signal
2 | PU | -- | Intrusion Sensor Alarm ON Signal
3 | RD/WH | -- | Battery Positive Voltage

### Power Sounder

#### Connector Part Information

- OEM: TYCO 1-967640-1
- Service: N/A
- Description: 4-Way F MQs Sealed

#### Power Sounder

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | -- | Run/Crank Ignition 1 Voltage
2 | RD/WH | -- | Battery Positive Voltage
3 | PK | -- | Power Sounder Enable Signal
4 | BK | -- | Ground

### Remote Control Door Lock Receiver

#### Connector Part Information

- OEM: JAEIL AG5-4S-S3C1
- Service: N/A
- Description: 4-Way F AG5 Unsealed

#### Remote Control Door Lock Receiver

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RD/WH | -- | Battery Positive Voltage
2 | GN | -- | Low Speed GMLAN Serial Data
3 | -- | -- | Not Used
4 | BK | -- | Ground

### Theft Deterent Control Module

#### Connector Part Information

- OEM: TYCO 368502-1
- Service: N/A
- Description: 6-Way F 070 Unsealed

#### Theft Deterent Control Module

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY/BK | -- | Courtesy Lamp Relay Control
2 | BK | -- | Ground
3 | D-GN | -- | Low Speed GMLAN Serial Data
4 | BK | -- | Ground
5 | D-BU | -- | Accessory Wakeup Serial Data
6 | RD/WH | -- | Battery Positive Voltage