For 1990-2009 cars

### Removal Procedure

1. Remove the driver air bag module. Refer to Inflatable Restraint Steering Wheel Module Replacement .
2. Remove the 2 screws and the steering wheel side cover.
3. Remove the 3 screws from the audio remote controller.
4. Disconnect the connector.
5. Remove the audio remote controller.

### Installation Procedure

1. Connect the connector.
2. Install the audio remote controller with the 3 screws.
3. Install the steering wheel side cover with the 2 screws.
4. Install the driver air bag module. Refer to Inflatable Restraint Steering Wheel Module Replacement .