For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Clutch Master Cylinder Nuts | 23 N·m | 17 lb ft
Concentric Slave Cylinder Retaining Bolts | 8-12 N·m | 71-106 lb in
Concentric Slave Cylinder-To-Clutch Oil Pipe Screw | 16 N·m | 12 lb ft
Pedal Mounting Shaft Nut | 18 N·m | 13 lb ft
Pressure Plate-To-Flywheel Bolts (2.4L) | 15 N·m | 11 lb ft
Pressure Plate-To-Flywheel Bolts (2.0L Diesel or 3.2L) | 28 N·m | 21 lb ft