For 1990-2009 cars

### Removal Procedure

1. Remove the rear brake rotor. Refer to Rear Brake Rotor Replacement .

Important: The disc brake backing plate and the park brake components are between the wheel bearing/hub assembly and the knuckle.

2. Remove the park brake components. Refer to Parking Brake Shoe Replacement .
3. Remove the rear wheel bearing/hub assembly. Refer to Rear Wheel Bearing and Hub Replacement .
4. Remove the parking brake cable from the backing plate.

### Installation Procedure

1. Install the parking brake cable to the backing plate.
2. Install the rear wheel bearing/hub assembly. Refer to Rear Wheel Bearing and Hub Replacement .
3. Install the park brake components. Refer to Parking Brake Shoe Replacement .
4. Install the rear brake rotor. Refer to Rear Brake Rotor Replacement .