For 1990-2009 cars

## Scan Tool Data List Except Holden

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON, Engine OFF.
Door Ajar Switch | Data | Door Closed/Door Ajar | Door Closed
Door Cylinder Switch | Data | Idle/Unlock/Lock/Invalid | Idle
Driver Door Handle | Data | Active/Inactive | Inactive

## Scan Tool Data List Holden

Scan tool values from an engine that is operating correctly may be used for comparison with the engine you are diagnosing. The Engine Scan Tool Data List represents the values that would be seen on a normal operating engine under the conditions specified in the first row of the Scan Tool Data List table.

Important: Do not use a scan tool that displays faulty data. The scan tool concern should be reported to the manufacturer. Use of a faulty scan tool may result in misdiagnosis and unnecessary parts replacement.

#### Scan Tool Data List

Scan Tool Parameter | System | Expected Value | Description
--- | --- | --- | ---
Engine Idling / Operating Temperature / Closed Throttle / Park or Neutral / Closed Loop / Accessories Off
Last Remote Key used | 1 2 3 4 None | - | This parameter displays the Last Key Used to gain enter to the vehicle.
Remote Key No 1 | Programmed Not Programmed | - | This parameter displays the key fobs that are programmed to the vehicle.
Remote Key No 2
Remote Key No 3
Remote Key No 4
Remote Key 1 Function | None Lock DR Door Unlock All Door Unlock R Closure Unlock | - | This parameter displays the remote key number and the function status used.
Remote Key 2 Function | Lt Sliding Ctrl Rh Sliding Ctrl Panic Fuel Door Power Windows
Remote Key 3 Function | Power Top Engine Start Engine Stop Program Key Locate
Remote Key 4 Function | R Closure Close R Closure Open R Closure Stop Double Lock Lt Sliding Stop
Battery Status Remote Key 1 | OK Not OK | - | This parameter displays the status of each of the remote battery's charge.
Battery Status Remote Key 2
Battery Status Remote Key 3
Battery Status Remote Key 4