SMU - SEC. 6E IGNITION TIMING SETTING PROCEDURE. Geo Metro 1993

For 1990-2009 cars

# SMU - SEC. 6E IGNITION TIMING SETTING PROCEDURE

#### SUBJECT: SECTION 6E IGNITION TIMING SETTING PROCEDURE

VEHICLES AFFECTED: 1992-93 "M" MODEL GEO METRO

#### APPLICATION:

1992 and 1993 Geo Metro

Steps 8 and 9 listed under the 1992 model year heading in this service bulletin replace Steps 8 and 9 on Page 6E2-C4-3 in the 1992 Geo Metro Service Manual (ST370-92).

Steps 9 through 1 1 listed under the 1993 model year heading in this service bulletin replace Steps 9 through 1 1 on page 6E2-C4-3 in the 1993 Geo Metro Service Manual (ST370-93).

Whenever it becomes necessary to check the ignition timing, the steps in this service bulletin should be used in conjunction with the remaining steps in the Service Manual.

1992 Geo Metro Model Year

8. Check timing. It should be 5 degree +/- 1 degree at specified idle. Refer to Vehicle Emission Control Information Label.

9. If not within specification, loosen distributor flange bolts and rotate distributor and repeat until timing is within specifications. After timing is within specifications, remove the jumper from the duty check coupler and make sure that the timing advances according to engine speed.

1993 Geo Metro Model Year

9. Check timing. It should be 5 degree +/- 1 degree at specified idle. Refer to Vehicle Emission Control Information Label.

10. If not within specification, loosen distributor flange bolts and rotate distributor and repeat until timing is within specifications.

11. Remove the jumper from the duty check DLC and make sure that the timing advances according to engine speed.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.