SMU-SECTION 6E2-REVISED TECH 1 DATA VALUES. Geo Metro 1994

For 1990-2009 cars

# SMU-SECTION 6E2-REVISED TECH 1 DATA VALUES

#### SUBJECT: SERVICE MANUAL UPDATE-SECTION 6E2-REVISED TECH 1 DATA VALUES

#### MODELS: 1992-94 GEO METRO WITH 1.0L ENGINE (VIN 6 - RPO LP2)

THIS BULLETIN UPDATES THE TECH 1 DATA VALUES FOUND IN SECTION 6E2 OF THE 1992-94 1.0L METRO SERVICE MANUAL: SPARK ADVANCE (NORMAL OPERATING TEMPERATURE): 8-17 DEGREES BTDC ADVANCE.

FIGURES: 0 ATTACHMENTS: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.