SERVICE MANUAL UPDATE SEC. 10 CHILD SEATBELT RESTRAINT SYS.. Geo Metro 1990

For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 10 CHILD SEATBELT RESTRAINT SYS.

#### Subject: CHILD SEAT RESTRAINT SYSTEM INSTALLATION

#### Model and Year: 1990-91 GEO METRO

#### TO: ALL CHEVROLET DEALERS

This bulletin is an addition to the 1990 GEO Metro Service Manual (ST370-90). This bulletin also replaces the "Front Seat Child Restraint" and the "Rear Seat Child Restraint" procedures found on pages 10-11-5 and 10-11-7 of the 1991 GEO Metro Service Manual (ST370-91).

#### FRONT SEAT CHILD RESTRAINT SYSTEM

Figures 1 through 6

1. Mark the anchor nut position on the right sill between the front and rear seats. For two- door model applications refer to Figure 1. For four-door model application, refer to Figure 2.

2. Cut a 60 mm X 60 mm (2.36 inch X 2.36 inch) flap out of the floor carpeting (Figure 1 or 2).

3. Install the anchor bracket and bolt to the right sill. For two-door model applications, refer to Figure 3. For four-door model applications, refer to Figure 4. On two-door models, place the right front seat in its most rearward position before tightening the anchor bolt. If necessary, tilt the bracket rearward to attain the required clearance. On four-door models, the right front seat will not travel to its most rearward position once the anchor bracket has been installed.

#### IMPORTANT

Make certain that the locking tangs on the back of the anchor bracket engage in sheet metal and not just the carpeting.

TIGHTEN

Anchor bolt to 40 N.m (30 lbs. ft.).

4. Install the child seat restraint safety belt. For two-door model applications, refer to Figure 5. For four-door model applications refer to Figure 6.

#### REAR SEAT CHILD RESTRAINT - TOP STRAP ANCHOR

Figure 7

1. Remove the restraint anchor cap from the rear end interior trim panel (Figure 7).

2. Install the anchor bracket to the rear end of the vehicle with the anchor bolt.

TIGHTEN

Anchor bolt to 45 N.m (33 lbs. ft.).

3. Replace the restraint anchor cap.

#### IMPORTANT

There is no center seating position provided for a child seat in the rear seat of this vehicle.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.